For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Removal .
2. Remove the lamp monitor module (1) from mounting bracket.
3. Disconnect the electrical connectors.

Remove the module (1).

### Installation Procedure

1. Install the module (1).
2. Connect the electrical connectors.
3. Install the module (1) to the mounting bracket.
4. Install the instrument panel assembly. Refer to Instrument Panel Assembly Removal .