For 1990-2009 cars

### Removal Procedure

1. Remove the speaker grille. Refer to Radio Rear Speaker Grille Replacement .
2. Remove the fasteners (1) retaining the tweeter speaker and mounting bracket to the grille.

Remove the speaker/mounting bracket.

3. Remove the fasteners retaining the speaker to the mounting bracket.

Remove the speaker.

### Installation Procedure

1. Align the speaker to the mounting bracket.

Install the fasteners.

2. Align the speaker/mounting bracket to the grille.

Install the fasteners (1).

3. Install the speaker grille. Refer to Radio Rear Speaker Grille Replacement .