For 1990-2009 cars

### Data Display

The scan tool displays the module data. This information assists in determining if the module is operating properly and if the module is sending or receiving the proper data to and from a particular system. The module uses data received from other systems in order to carry out some functions. If the module receives the incorrect data from another system, the module may function improperly. Use the scan tool in order to review the data from the systems that interact with the module.

### Displayed Input Status

The scan tool also displays the module input status. Select the module input status display in order to display the data and in order to determine if the switched inputs may be properly interpreted. The display also indicates if the input has changed states. For example, when a door is closed, the scan tool displays the input status of the door ajar switch as INACTIVE. When the door is open, the scan tool reads ACTIVE. Use this type of information when diagnosing a malfunction associated with a particular module input or an input that is shared with another system.

### Cycle Outputs

Use a scan tool in order to cycle the module output functions. When the module output cycling is selected, the scan tool may command the module to cycle an output. This feature may be used in order to determine if the module is able to cycle an output regardless of the inputs or any specific program instructions. Once a test is selected, the scan tool will command the module to energize the selected output. The scan tool then displays the status of the selected output. The displayed information represents only what module was commanded, not what action was actually performed. Verify that the module is actually performing each of the selected output functions.