For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Clutch | On the right lower front of the engine, on the A/C compressor | HVAC Component Views | HVAC Connector End Views
A/C Compressor Diode | On the right front of the engine, near the A/C compressor, in the harness | HVAC Component Views | --
A/C Compressor Relay | In the center rear of the engine compartment, below the right side MaxiFuse® block | HVAC Component Views | HVAC Connector End Views
A/C Refrigerant Pressure Sensor | Right hand lower front corner of engine, in compressor hose | HVAC Component Views | HVAC Connector End Views
Ambient Temperature Sensor | Center front of vehicle on lower radiator rail | HVAC Component Views | --
Blower Control Module | In the center rear of the engine compartment, below the right side MaxiFuse® block | HVAC Component Views | HVAC Connector End Views
Blower Motor | In the center rear of the engine compartment, below the left side MaxiFuse® block | HVAC Component Views | --
Blower Relay | In the center rear of the engine compartment, below the right side MaxiFuse® block | HVAC Component Views | Engine Controls Connector End Views in Engine Controls
Data Link Connector (DLC) | Under the left side of the IP, on the IP sound insulator | Data Link Communications Component Views in Wiring Systems | Data Link Communications Connector End Views in Wiring Systems
Heater and A/C Control Assembly (Buick/Oldsmobile w/ CJ2) | In the center of the IP, near the radio | Engine Controls Components in Engine Controls | HVAC Connector End Views
Heater and A/C Control Assembly (Pontiac w/ C68) | In the center of the IP, near the radio | HVAC Component Views | HVAC Connector End Views
Heater and A/C Programmer (Pontiac) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views | HVAC Connector End Views
Heater and A/C Programmer (Buick) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views | HVAC Connector End Views
Heater and A/C Programmer (Oldsmobile) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views | HVAC Connector End Views
Heater and A/C Vacuum Solenoid | Under the right side of the IP, on the right of the HVAC module | HVAC Component Views | --
High Blower Relay | In the center rear of the engine compartment, below the right side MaxiFuse® block | HVAC Component Views | --
Inside Air Temperature Sensor | Right hand side of the instrument panel, behind the instrument panel on the HVAC case | HVAC Component Views | HVAC Connector End Views
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
IP Junction Block | Under the right side of the IP, near the rear of the IP compartment | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
Passenger Temperature Control | On the right front door, on the door trim panel | HVAC Component Views | HVAC Connector End Views
Sunload Sensor | Top of the instrument panel in defroster grille | HVAC Component Views | HVAC Connector End Views
Temperature Actuator | Under the right side of the IP, on the right of the HVAC module | Harness Routing Views in Wiring Systems | HVAC Connector End Views
C200 | The body harness to the IP harness, under the center of the IP | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G105 | In the right front of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
G201 | In the right front of the passenger compartment, behind the right kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
G202 | In the left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P101 | In the right rear of the engine compartment, near the right front strut tower | Harness Routing Views in Wiring Systems | --
P600 | On the front of the right front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S207 | In the body harness, approximately 12 cm (4.7 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S213 (Buick) | In the IP harness, approximately 4 cm (1.6 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S213 (Oldsmobile) | In the IP harness, approximately 22 cm (8.7 in) from C200 | Harness Routing Views in Wiring Systems | --
S213 (Pontiac) | In the IP harness, approximately 6 cm (2.4 in) from the IP compartment lamp breakout | Harness Routing Views in Wiring Systems | --
S214 (Buick) | In the IP harness, approximately 10.5 cm (4.1 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.5 in) from the top edge of the left kick wall channel | Harness Routing Views in Wiring Systems | --
S241 | In the body harness, approximately 40 cm (15.7 in) from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --
S264 | In the IP harness, approximately 22 cm (8.6 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S268 | In the body harness, approximately 26 cm (10.2 in) into the HVAC programmer breakout | Harness Routing Views in Wiring Systems | --
S269 | In the body harness, approximately 19.5 cm (7.7 in) into the HVAC programmer breakout | Harness Routing Views in Wiring Systems | --
S270 | In the body harness, approximately 8 cm (3.1 in) from edge of the right hand IP harness channel end | Harness Routing Views in Wiring Systems | --
S277 | In the IP harness, approximately 17 cm (6.7 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S308 | In the body harness, approximately 33 cm (13 in) from the G201 breakout | Harness Routing Views in Wiring Systems | --