For 1990-2009 cars

## Approximate Fluid Capacities 3.8L

Application | Specification
--- | ---
Metric | English
Cooling system

- 3.8 L

12.5 liters

13 quarts

Engine crankcase

- Engine oil with filter

4.3 liters

4.5 quarts

Fuel tank

- L67

73.4 liters

19.4 gallons

Power steering

- Pump only

0.5 liters

1 pint

- Complete system

0.7 liters

1.5 pints

Transaxle

- Drain and refill

7.0 liters

7.4 quarts

- Overhaul

9.5 liters

10.0 quarts

- Dry

12.7 liters

13.4 quarts