For 1990-2009 cars

The engine oil life monitor will indicate when to change the engine oil usually between 5 000 km (3,000 miles) and 12 000 km (7,500 miles) since the last oil change. Under severe conditions, the CHANGE OIL massage may be displayed before 5 000 km (3,000 miles). Never drive the vehicle more than 12 500 km (7,500 miles) or 12 months, (whichever occurs first), without an oil change. The engine oil life monitor will not detect dust in the oil. If the vehicle is driven in a dusty area, be sure to change the oil every 5 000 km (3,000 miles) or sooner if the CHANGE OIL message is displayed. Reset the oil life monitor when the oil has been change, use the following procedure.

### Resetting Procedure

Follow this procedure to reset the engine oil life monitor:

1. Turn the ignition to RUN.
2. Press the TRIP button on the driver information center (DIC) switch to view various menu choices and stop on OIL LIFE REMAINING.
3. Press and hold the RESET button on the DIC switch for more than 5 seconds. The oil life will change to 100%. The engine oil life monitor is now reset.
4. Turn the ignition OFF.