For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Accelerator Controls Cable Bracket | 16 N·m | 12 lb ft
Accelerator Pedal Assembly Bolt and Stud | 3 N·m | 27 lb in
Air Cleaner Assembly Support Bolts | 4 N·m | 35 lb in
Air Cleaner Intake Duct Screws | 2 N·m | 18 lb in
Boost Control Solenoid Bracket Nut | 8 N·m | 72 lb in
Bypass Valve Actuator Bolts | 25 N·m | 18 lb ft
Camshaft Position (CMP) Sensor Retaining Bolt | 10 N·m | 90 lb in
Crankshaft Balancer Bolt | 150 N·m +76° | 110 lb ft +76°
Crankshaft Position (CKP) Sensor Bolts | 20-40 N·m | 14-28 lb ft
EGR Valve Nuts | 30 N·m | 22 lb ft
Engine Coolant Temperature (ECT) Sensor | 30 N·m | 22 lb ft
Engine Oil Level Sensor | 17-27 N·m | 13-20 lb ft
EVAP Vent Valve Bracket | 2 N·m | 18 lb in
Exhaust Gas Recirculation Valve to Throttle Body Adapter Bolts | 30 N·m | 22 lb ft
Fuel Filler Neck Bolts | 2 N·m | 18 lb in
Fuel Injector Sight Shield | 2 N·m | 18 lb in
Fuel Line Retainer | 12 N·m | 106 lb in
Fuel Pump Control Module Attaching Nut | 9 N·m | 80 lb in
Fuel Rail Attaching Nuts or Bolts | 10 N·m | --
Fuel Rail Hold-Down Stud | 25 N·m | --
Fuel Return Tube Nut | 17 N·m | --
Fuel Tank Filler Pipe - EVAP Pipe Hose Clamp | 2.5 N·m | 22 lb in
Fuel Tank Filler Pipe Hose Clamp | 2.5 N·m | 22 lb in
Fuel Tank Retaining Strap Bolts | 34 N·m | --
Heated Oxygen Sensors | 41 N·m | --
Idle Air Control Attaching Screws | 3 N·m | 27 lb in
Ignition Coil to Ignition Control Module Screws | 4-5 N·m | 40 lb in
In-Line Fuel Filter Outlet Nut | 30 N·m | 22 lb ft
Intake Air Duct Clamp Screws | 2 N·m | 18 lb in
Intake Air Tube Clamp | 2 N·m | 18 lb in
Knock Sensors | 19 N·m | 14 lb in
Manifold Absolute Pressure (MAP) Sensor Bracket Retaining Bolt | 30 N·m | 22 lb ft
Mass Air (MAF) Flow Sensor Attaching Screws | 3 N·m | 27 lb in
Powertrain Control Module (PCM) Housing to Chassis Bolts | 5-9 N·m | 50-80 lb in
Spark Plugs | 27 N·m | 20 lb ft
Throttle Body Retaining Nuts or Bolts | 10 N·m | 7 lb ft
Throttle Body Support Bracket (VIN K) | 10 N·m | 7 lb ft
Throttle Position (TP) Sensor Attaching Screws | 2 N·m | 18 lb in
Transaxle Range Switch Attaching Bolts | 28 N·m | 20 lb ft
Wheel Lug Nuts | 140 N·m | 104 lb ft