For 1990-2009 cars

#### In-Line Connector C100

Connector Part Information |

• | 12160493

• | 20-Way F Micro-Pack 100W Series (GRY)

Connector Part Information

• | 12176566

• | 20-Way M Micro-Pack 100W Series, Lock Assist/Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control
B | YEL/BLK | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control
C | RED/BLK | 1228 | Pressure Control Solenoid (PC SOL) Valve - High | C | PPL | 1228 | Pressure Control Solenoid (PC SOL) Valve - High
D | LT BLU/WHT | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low | D | LT BLU | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low
E | PNK | 339 | Fused Ignition 1 Feed | E | RED | 839 | Fused Ignition 1 Feed
F-K | - | - | Not Used | F-K | - | - | Not Used
L | YEL/BLK | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal | L | BRN | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal
M | BLK | 808 | Sensor Ground | M | GRY | 452 | Sensor Ground
N | PNK | 1224 | Trans Fluid Pressure Switch A Input | N | PNK | 1224 | Trans Fluid Pressure Switch A Input
P | RED | 1226 | Trans Fluid Pressure Switch C Input | P | ORN | 1226 | Trans Fluid Pressure Switch C Input
R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input | R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input
S | RED/BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High | S | BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High
T | BRN | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control | T | TAN | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control
U | YEL | 657 | TCC Release Switch Input | U | WHT | 1804 | TCC Release Switch Input
V | DK BLU/WHT | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low | V | DK GRN | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low
W | - | - | Not Used | W | - | - | Not Used