For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Radio/Audio System Check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Use the J 39916-A in order to perform the motor speed test. Is the cassette motor speed correct? | -- | Go to Step 3 | Go to Step 4
3 | Use the J 39916-A in order to clean the cassette player. Is the condition still present? | -- | Go to Step 4 | Go to Radio/Audio System Check
4 | Replace the radio. Refer to one of the following:

• | Radio Replacement

• | Radio Replacement

• | Radio Replacement

Did you complete the repair?

--

Go to Radio/Audio System Check

--