For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Driver/Passenger Seat Buckle Nut | 28 N·m | 21 lb ft
Front Driver/Passenger Seat Buckle-Side Dual Retractor Screws | 25 N·m | 19 lb ft
Front Driver/Passenger Seat Buckle-Side Belt Load Bar Bolt | 40 N·m | 30 lb ft
Front Driver/Passenger Seat Shoulder Belt Bolt | 42 N·m | 31 lb ft
Front Seat Shoulder Belt Guide Loop Bolt | 42 N·m | 31 lb ft
Rear Seat Center Nut | 30 N·m | 22 lb ft
Rear Seat Retractor-Side Belt Assembly Bolt | 30 N·m | 22 lb ft
Rear Seat Anchor Bolt | 35 N·m | 26 lb ft