For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Bose® Amplifier | Under the center of the IP, near the back of the radio | Entertainment Component Views | Entertainment Connector End Views
Data Link Connector (DLC) | Under the left side of the IP, on the IP sound insulator | Data Link Communications Components in Wiring Systems | Data Link Communications Connector End Views in Wiring Systems
Ground Coil | In the right rear of the passenger compartment, under the upper sail trim panel | Stationary Windows Component Views in Stationary Windows | Stationary Windows Connector End Views in Stationary Windows
Heater and A/C Control Assembly (Pontiac w/C68) | In the center of the IP, near the radio | -- | HVAC Connector End Views in HVAC
Heater and A/C Programmer (Buick) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Heater and A/C Programmer (Oldsmobile) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Heater and A/C Programmer (Pontiac) | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Inflatable Restraint Steering Wheel Module Coil | In the left front of the passenger compartment, in the top of the steering column | SIR Component Views in Restraints | --
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
IP Junction Block | Under the right side of the IP, near the rear of the IP compartment | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
LH Steering Wheel Controls | In the left front of the passenger compartment, on the steering wheel | Entertainment Component Views | --
Radio (Buick, Oldsmobile) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views | Entertainment Connector End Views
Radio C1(Pontiac) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views | Entertainment Connector End Views
Radio C2 (Pontiac) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views | Entertainment Connector End Views
Radio Antenna Module | In the left rear the passenger compartment, under the upper sail trim panel | Stationary Windows Component Views in Stationary Windows | Stationary Windows Connector End Views in Stationary Windows
RH Steering Wheel Controls | In the left front of the passenger compartment, on the steering wheel | Entertainment Component Views | --
Steering Column Fuse Holder | In the left front of the passenger compartment, on the base of the steering column | -- | --
C200 (116 cavities) | The body harness to the IP harness, under the center of the IP | -- | Inline Harness Connector End Views in Wiring Systems
C202 (48 cavities) | The body harness to the steering column harness, under the left side of the IP, to the left of the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C207 (6 cavities) | The body harness to the body harness, under the right side of the IP | -- | Inline Harness Connector End Views in Wiring Systems
C209 (4 cavities) | The body harness to the right door audio harness, under the right side of the IP | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C212 (2 cavities) | The body harness to the left door audio harness, under the right side of the IP | Harness Routing Views | Inline Harness Connector End Views in Wiring Systems
G201 | In the right front of the passenger compartment, behind the right kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
G202 | In the left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P500 | On the front of the left front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
P600 | On the front of the right front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S203 | In the body harness, approximately 43.5 cm (17.1 in) from the IP fuse block | Harness Routing Views in Wiring Systems | --
S206 | In the IP harness, approximately 52.5 cm (20.7 in) from the radio breakout | Harness Routing Views in Wiring Systems | --
S207 | In the body harness, approximately 12 cm (4.7 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S213 (Buick) | In the IP harness, approximately 4 cm (1.6 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S213 (Oldsmobile) | In the IP harness, approximately 22 cm (8.7 in ) from C200 | Harness Routing Views in Wiring Systems | --
S213 (Pontiac) | In the IP harness, approximately 6 cm (2.4 in) from the IP compartment lamp breakout | Harness Routing Views in Wiring Systems | --
S214 (Buick) | In the IP harness, approximately 10.5 cm (4.1 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S214 (Oldsmobile) | In the IP harness, approximately 30 cm (11.8 in) from C200 | Harness Routing Views in Wiring Systems | --
S214 (Pontiac) | In the IP harness, approximately 6.5 cm (2.6 in) from the IP compartment lamp breakout | Harness Routing Views in Wiring Systems | --
S223 | In the body harness, approximately 4 cm (1.6 in) from the instrument cluster breakout | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.5 in) from the top edge of the left kick wall channel | Harness Routing Views in Wiring Systems | --
S234 (Buick) | In the IP harness, approximately 10 cm (3.9 in) into the C200 breakout | -- | --
S234 (Oldsmobile) | In the IP harness, approximately 32 cm (12.6 in) from C200 | -- | --
S234 (Pontiac) | In the IP harness, approximately 11 cm (4.3 in) from the radio breakout | -- | --
S251 | In the body harness, approximately 10 cm (3.9 in) from the right IP harness channel end | Harness Routing Views in Wiring Systems | --
S301 | In the body harness, approximately 10 cm (3.9 in) from P400 | Harness Routing Views in Wiring Systems | --
S308 | In the body harness, approximately 33 cm (13 in) from the G201 breakout | Harness Routing Views in Wiring Systems | --
S408 | In the body harness, approximately 10 cm (3.9 in) from P400 | Harness Routing Views in Wiring Systems | --
S409 | In the body harness, approximately 17 cm (6.7 in) from P400 | Harness Routing Views in Wiring Systems | --
S410 | In the body harness, approximately 129 cm (50.8 in) from P400 | Harness Routing Views in Wiring Systems | --
S503 | In the body harness, approximately 21 cm (8.3 in) from P500 | Harness Routing Views in Wiring Systems | --
S504 | In the body harness, approximately 13 cm (5.1 in) from P500 | Harness Routing Views in Wiring Systems | --
S601 | In the body harness, approximately 13 cm (5.1 in) from P600 | Harness Routing Views in Wiring Systems | --
S602 | In the body harness, approximately 21 cm (8.3 in) from P600 | Harness Routing Views in Wiring Systems | --