For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Seat Memory System Check? | -- | Go to Step 2 | Go to Memory Seats System Check
2 |

1. Turn the ignition switch to the OFF position.
2. Connect a fused jumper from the memory seat/mirror module diagnostic connector to ground.

• | The connector may be taped up into the body harness.

• | The memory seat/mirror module will beep once in order to acknowledge entrance into the mode 1 diagnostics.

• | Refer to Power Seats Circuit Description for a detailed explanation of the memory seat/mirror module diagnostic modes.

3. Remove the ground from the memory seat/mirror module diagnostic connector, then ground the connector again within 5 seconds.

• | The module will beep twice in order to acknowledge entrance into the mode 2 diagnostics.

• | Refer to Circuit Operation for a detailed explanation of the memory seat/mirror module diagnostic modes.

4. Operate the seat switch in the forward/back directions. (The module will beep once for an open or short circuit to a position sensor or any position sensor discontinuity.)
5. Any time a switch is operated and the module beeps, the module senses a problem with the position sensor.

Does the memory seat/mirror module beep?

--

Go to Step 3

Go to Step 8

3 | Test for an open or short in CKT 569 (DK GRN). Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 569 OK? | -- | Go to Step 4 | Go to Step 7
4 | Test for an open or short in CKT 788 (GRY) between the seat horizontal position sensor and S341. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 788 OK? | -- | Go to Step 5 | Go to Step 7
5 | Test for an open or short in CKT 782 (BLK) between the seat horizontal position sensor and S340. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 782 OK? | -- | Go to Step 6 | Go to Step 7
6 | Replace the seat horizontal position sensor. Is the repair complete? | -- | Go to Memory Seats System Check | --
7 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Memory Seats System Check | --
8 |

1. The system is functioning properly.
2. If the system persists, replace the memory seat/mirror module.

Is the repair complete?

--

Go to Memory Seats System Check

--