For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Ignition Switch | Under the left side of the instrument panel, on the base of the steering column | Power and Grounding Component Views in Wiring Systems | --
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | --
IP Junction Block | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Power and Grounding Component Views in Wiring Systems | --
LH Front Door Lock Actuator C1 | Rear of the left front door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Door Lock Actuator C2 | Rear of the left front door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Power Window Switch (Pontiac) | At the center of the left front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Power Window Switch C1 (Buick) | At the center of the left front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Power Window Switch C2 (Buick) | At the center of the left front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Power Window Switch C1 (Oldsmobile) | At the center of the left front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Front Power Window Switch C2 (Oldsmobile) | At the center of the left front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Rear Door Lock Actuator C1 | Rear of the left rear door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Rear Door Lock Actuator C2 | Rear of the left rear door, on the door lock cylinder | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LH Rear Power Window Switch | Center of the left rear door, in the door trim panel | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Power Window Control Module | Lower center of the left hand front door, behind the door trim panel | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Radio (Buick, Oldsmobile) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Radio C1(Pontiac) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Radio C2 (Pontiac) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Radio C3 (Pontiac) | In the center of the IP, near the heater and the A/C control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Remote Function Actuator (RFA) Module | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Keyless Entry Component Views in Keyless Entry | Keyless Entry Connector End Views in Keyless Entry
RH Front Door Lock Actuator C1 | On the rear of the right hand front door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Front Door Lock Actuator C2 | On the rear of the right hand front door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Front Power Window Switch (Buick) | On the center of the right front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Front Power Window Switch (Oldsmobile) | On the center of the right front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Front Power Window Switch (Pontiac) | On the center of the right front door, near the arm rest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH MaxiFuse® Block | In the center rear of the engine compartment, near the cowl | Power and Grounding Component Views in Wiring Systems | --
RH Rear Door Lock Actuator C1 | On the rear of the right rear door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Rear Door Lock Actuator C2 | On the rear of the right rear door, on the door latch assembly | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RH Rear Power Window Switch | On the center of the left rear door, in the door trim panel | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Steering Wheel Controls | On the left side of the passenger compartment, on the steering wheel | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Sunroof Control Module | Center of the passenger compartment, near the rear of the headliner | Power Roof Systems Component Views in Roof | Power Roof Systems Connector End Views in Roof
C200 (116 cavities) | Body harness to the IP harness, under the center of the IP | Harness Routing Views in Wiring Systems | --
C202 (48 cavities) | Body harness to the steering column harness, under the left side of the IP to the left of the steering column | Harness Routing Views in Wiring Systems | --
C221 (3 cavities) | Body harness to sunroof harness, to the right front of the passenger compartment on the top of the front pillar | Harness Routing Views in Wiring Systems | --
C502 (6 cavities) | Body harness to the left front door harness, at the lower front of the left front door | Harness Routing Views in Wiring Systems | --
C603 (6 cavities) | Body harness to the right front door harness, to the lower front of the right front door | Harness Routing Views in Wiring Systems | --
C702 (4 cavities) | Body harness to the left rear door harness, to the lower front of the left rear door | Harness Routing Views in Wiring Systems | --
C802 (4 cavities) | Body harness to the right rear door harness, to the lower front of the right rear door | Harness Routing Views in Wiring Systems | --
G201 | Right front of the passenger compartment, behind the right kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
G202 | Left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P101 | Right rear of the engine compartment, near the right front strut tower | Harness Routing Views in Wiring Systems | --
P500 | Front of the left front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
P600 | Front of the right front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
P700 | Front of the left rear door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
P800 | Front of the right rear door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S203 | In the body harness, approximately 43.5 cm (17.1 in) from the instrument panel fuse block | Harness Routing Views in Wiring Systems | --
S208 | In the body harness, approximately 6 cm (2.3 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S215 | In the body harness, approximately 73.5 cm (29 in) from the IP fuse block | Harness Routing Views in Wiring Systems | --
S218 | In the body harness, approximately 49.5 cm (19.4 in) from the top edge of the left foot well harness channel | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.4 in) from the top edge of the left hand foot well harness channel | Harness Routing Views in Wiring Systems | --
S251 | In the body harness, approximately 10 cm (3.9 in) from the right edge of the instrument panel harness channel end | Harness Routing Views in Wiring Systems | --
S289 | In the body harness, approximately 31.5 cm (12.4 in) from the top edge of the left hand kick wall channel | Harness Routing Views in Wiring Systems | --
S308 | In the body harness, approximately 33 cm (13 in) from the G201 breakout | Harness Routing Views in Wiring Systems | --
S310 | In the body harness, approximately 9 cm (3.5 in) from the G201 breakout | Harness Routing Views in Wiring Systems | --
S501 | In the body harness, approximately 43 cm (16.9 in) from P500 | Harness Routing Views in Wiring Systems | --
S603 | In the body harness, approximately 5.5 cm (2.1 in) from P500 | Harness Routing Views in Wiring Systems | --