For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Close all the doors.
2. Lock the left or right front door.
3. Operate the left or right front door handle.

The interior lights illuminate.

Refer to Interior Lamps System Check in Lighting Systems.

2 | Press the transmitter (keyfob) UNLOCK button. | The left or right front door unlocks. | Refer to Remote Keyless Entry System Check in Keyless Entry.
3 |

1. Close all the doors.
2. Turn the ignition switch to the RUN position.
3. Turn the ignition switch to the OFF position.
4. Open the left or right front door.

The SECURITY indicator flashes.

Content Theft Deterrent (CTD) Alarm Mode Always On

4 | Press the left or the right front power door lock switch. | The SECURITY indicator illuminates. | Content Theft Deterrent (CTD) Alarm Mode Inoperative
5 |

1. Close the left or the right front door.
2. Stay in the vehicle.

1. The security indicator illuminates for 30 seconds.
2. The CTD system arms.

Content Theft Deterrent (CTD) Alarm Mode Inoperative

6 |

1. After 1 minute, use the mechanical lock/unlock lever in order to unlock the left or the right front door.
2. Open the left or right front door.

1. The horns and exterior lights cycle ON and OFF.
2. The lights cycle approximately once per second for 3 to 7 minutes.
3. The CTD system is in the alarm mode.

• | Content Theft Deterrent (CTD) Alarm Mode Inoperative

• | Horn Inoperative in Content Theft Deterrent (CTD) Alarm Mode

• | Lights Inoperative in Content Theft Deterrent (CTD) Alarm Mode

7 |

1. Wait 3 minutes after the CTD system enters the alarm mode.
2. Use the key in order to lock/unlock the left or the right front door.

1. The horns and exterior lights stop cycling ON and OFF.
2. The CTD system is disarmed.

Content Theft Deterrent (CTD) Alarm Mode Always On

8 |

1. Disarm the CTD system.
2. Press the remote keyless entry transmitter UNLOCK button.

The CTD system is disarmed.

Content Theft Deterrent (CTD) Alarm Mode Always On

9 |

1. Sitting in the vehicle, use the mechanical door lever in order to lock each door.
2. Close all the doors.

1. The SECURITY indicator turns OFF when the last door is closed.
2. The CTD system does not enter the armed mode.

Content Theft Deterrent (CTD) Alarm Mode Always On

10 |

1. Use the mechanical door lock lever or outside key lock in order to unlock the left front door.
2. Open the door.

The CTD system does not enter the alarm mode.

Content Theft Deterrent (CTD) Alarm Mode Always On

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.