For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid (1-2 SS) Valve | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
2-3 Shift Solenoid (2-3 SS) Valve | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
ABS/TCC Switch | Under the left hand of the instrument panel, near the brake pedal | Engine Controls Component Views in Engine Controls - 3.8 L | Engine Controls Connector End Views in Engine Controls - 3.8 L
Automatic Transaxle Fluid Pressure (TFP) Manual Valve Position Switch | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
Automatic Transaxle Fluid Temperature (TFT) Sensor | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
Data Link Connector (DLC) | Under the left hand of the instrument panel, on the instrument panel sound insulator | Data Link Communications Component Views in Wiring System | Data Link Communications Connector End Views in Wiring Systems
IP Fuse Block | Under the left hand of the instrument panel, on the left hand instrument panel sound insulator | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
IP Junction Block (IP Electrical Center) | Under the right hand of the instrument panel, near the rear of the instrument panel compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) | Left hand front of the engine compartment, near the air cleaner housing | Engine Controls Component Views in Engine Controls - 3.8L | Powertrain Control Module Connector End Views in Engine Controls - 3.8L
Pressure Control Solenoid (PC SOL) Valve | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
RH MaxiFuse® Block | Center rear of the engine compartment, near the cowl | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Shift Select Switch | On the center console | Engine Controls Component Views in Engine Controls - 3.8 L | Engine Controls Connector End Views in Engine Controls - 3.8 L
Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve | Left hand of the engine compartment, in the transaxle assembly | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
C100 (20 cavities) | Engine harness to the transaxle, left hand front of the engine compartment below the throttle body | -- | Automatic Transmission Inline Harness Connector End View
C101 (66 cavities) | Body harness to the engine harness, right hand rear of the engine compartment near the strut tower | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (116 cavities) | Body harness to the instrument panel harness, under the center of the instrument panel | -- | Inline Harness Connector End Views in Wiring Systems
G101 | Right hand rear of the engine, below the power steering pump | Harness Routing Views in Wiring Systems | --
G202 | Left hand front of the passenger compartment, behind the left hand kick panel trim plate | Harness Routing Views in Wiring Systems | --
P100 | Left hand rear of the engine compartment, near the left hand front strut tower | Harness Routing Views in Wiring Systems | --
P101 | Right hand rear of the engine compartment, near the right hand front strut tower | Harness Routing Views in Wiring Systems | --
S104 | In the body harness, approx 27 cm (10.6 inches) into the cooling fan relay breakout | Harness Routing Views in Wiring Systems | --
S110 (VIN K) | In the engine harness, approx 6.5 cm (2.6 inches) from the generator breakout | Harness Routing Views in Wiring Systems | --
S110 (VIN 1) | In the engine harness, approx 6.5 cm (2.6 inches) from the generator breakout | -- | --
S121 (VIN 1) | In the engine harness, approx 32 cm (12.6 inches) from C101 | -- | --
S121 (VIN K) | In the engine harness, approx 32 cm (12.6 inches) from C101 | Harness Routing Views in Wiring Systems | --
S130 (VIN 1) | In the engine harness, approx 25.5 cm (10 inches) from C101 | Harness Routing Views in Wiring Systems | --
S130 (VIN K) | In the engine harness, approx 25.5 cm (10 inches) from C101 | Harness Routing Views in Wiring Systems | --
S206 | In the instrument panel harness, approx 52.5 cm (20.6 inches) from the radio breakout | Harness Routing Views in Wiring Systems | --
S207 | In the body harness, approx 12 cm (4.72 inches) from the center instrument panel harness channel breakout | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approx 49.5 cm (19.5 inches) from the top edge of the left hand kick wall channel | Harness Routing Views in Wiring Systems | --
S226 | In the body harness, approx 31.5 cm (12.4 inches) from the data link connector | Harness Routing Views in Wiring Systems | --
S233 | In the body harness, approx 22 cm (8.7 inches) into the C101 breakout | Harness Routing Views in Wiring Systems | --
S239 | In the body harness, approx 26 cm (10.2 inches) from the center instrument panel harness channel breakout | Harness Routing Views in Wiring Systems | --
S241 | In the body harness, approx 40 cm (15.7 inches) from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --
S273 | In the body harness, approx 17 cm (6.7 inches) into the C101 breakout | Harness Routing Views in Wiring Systems | --
S276 | In the instrument panel harness, approx 142.5 cm (56 inches) from C200 | Harness Routing Views in Wiring Systems | --
S278 | In the body harness, approx 42.5 cm (16.7 inches) from the remote function actuator module breakout | Harness Routing Views in Wiring Systems | --
S284 | In the body harness, approx 27 cm (10.6 inches) from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --