For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Fascia to Fenders Nuts | 9.5 N·m | 84 lb in
Front/Rear Energy Absorbers to Body Bolts and Nuts | 27 N·m | 20 lb ft
Front/Rear Energy Absorbers to Body Side Rail Bolt | 4 N·m | 35 lb in
Impact Bar to Energy Absorbers Nuts | 27 N·m | 20 lb ft
Lower Air Deflector Bolts | 2.8 N·m | 25 lb in
Rear Fascia to Quarter Nuts | 9.5 N·m | 84 lb in