For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn ignition switch to the START position. | Engine cranks. |

• | Starter Solenoid Does Not Click

• | Starter Solenoid Clicks, Engine Does Not Crank

2 | Ignition switch in run, engine running. | Charging system operating properly. Volt/charge indicator operating properly |

• | Battery Is Undercharged or Overcharged

• | Charge Indicator Always On

• | Charge Indicator Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.