For 1990-2009 cars

## Transmission Control Replacement Oldsmobile

### Removal Procedure

1. Remove the shift knob from the shifter.
2. Remove the console assembly.
3. Remove the park/lock cable from the floorshift control.
4. Remove the shift control cable from the floorshift control.
5. Remove the floorshift control bolts.
6. Remove the floorshift control.

### Installation Procedure

1. Install the floorshift control.
2. Install the floorshift control bolts.
3. Install the shift control cable to the floorshift control.
4. Install the park/lock cable to the floorshift control.
5. Install the console assembly.
6. Install the shift knob to the shifter.

## Transmission Control Replacement Pontiac

### Removal Procedure

1. Remove the shift knob from the shifter.
2. Remove the console assembly.
3. Remove the park/lock cable from the floorshift control.
4. Remove the shift control cable from the floorshift control.
5. Remove the floorshift control nuts.
6. Remove the floorshift control.

### Installation Procedure

1. Install the floorshift control.
2. Install the floorshift control nuts.
3. Install the shift control cable to the floorshift control.
4. Install the park/lock cable to the floorshift control.
5. Install the console assembly.
6. Install the shift knob to the shifter.