For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) | Under the left side of the IP, on the IP sound insulator | Data Link Communications Component Views | Data Link Communications Connector End Views
Electronic Brake (and Traction) Control Module (EBCM/EBTCM) | In the left front of the engine compartment, near the base of the radiator support | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Electronic Suspension Control (CCR) Module | Left front of the passenger compartment, below the left hand front seat | Suspension Controls Component Views in Real Time Damping (RTD) | Suspension Controls Connector End Views in Real Time Damping (RTD)
Heater and A/C Control (w/ C68) | In the center of the IP, near the radio | HVAC Component Views in HVAC Systems with A/C - Automatic | HVAC Connector End Views in HVAC Systems with A/C - Automatic
Heater and A/C Programmer | Under the right side of the IP, near the rear of the IP compartment | HVAC Component Views in HVAC Systems with A/C - Automatic | HVAC Connector End Views in HVAC Systems with A/C - Automatic
Inflatable Restraint Sensing and Diagnostic Module (SDM) | In the right front of passenger compartment, below the right front seat | SIR Component Views in SIR | SIR Connector End Views in SIR
Instrument Cluster | In the left side of the IP, above the steering column | Instrument Cluster and HUD Component Views in Instrument Panel, Gauges and Console | Instrument Cluster and HUD Connector End Views in Instrument Panel, Gauges and Console
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views | --
Powertrain Control Module (PCM) | In the left front of the engine compartment, near the air cleaner housing | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
Radio | In the center of the IP, near the heater and A/C control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Remote Function Actuator (RFA) Module | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Keyless Entry Component Views in Keyless Entry | Keyless Entry Connector End Views in Keyless Entry
Transmission Position Decoder Module | Center front of the passenger compartment, under the front of the center console | Instrument Cluster and HUD Component Views in Instrument Panel, Gauges and Console | Instrument Cluster and HUD Connector End Views in Instrument Panel, Gauges and Console
C101 (66 cavities) | Body harness to the engine harness, right rear of the engine compartment near the strut tower | Harness Routing Views | Inline Harness Connector End Views
C200 (116 cavities) | Body harness to the IP harness, under the center of the IP | Harness Routing Views | Inline Harness Connector End Views
C304 (8 cavities) | Body harness to the console harness, under the front of the center console | Harness Routing Views | --
G101 | Right rear of the engine, below the power steering pump | Power and Grounding Component Views | --
G202 | Left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views | --
S110 (VIN 1) | In the engine harness, approximately 6.5 cm (2.5 in) from the generator harness breakout | Harness Routing Views | --
S110 (VIN K) | In the engine harness, approximately 6.5 cm (2.5 in) from the generator harness breakout | Harness Routing Views | --
S207 | In the body harness, approximately 12 cm (4.7 in) from the center IP harness channel breakout | Harness Routing Views | --
S209 | In the IP harness, approximately 14 cm (5.5 in) from C200 | Harness Routing Views | --
S224 | In the IP harness, approximately 17 cm (6.7 in) from the radio breakout | Harness Routing Views | --
S225 | In the body harness, approximately 49.5 cm (19.4 in) from the top edge of the left hand foot well harness channel | Harness Routing Views | --
S226 | In the body harness, approximately 31.5 cm (12 in) from the data link connector | Harness Routing Views | --
S273 | In the body harness, approximately 17 cm (6.7 in) into the C101 breakout | Harness Routing Views | --
S278 | In the body harness, approximately 42.5 cm (16.7 in) from the remote function actuator module breakout | Harness Routing Views | --