For 1990-2009 cars

### Removal Procedure

1. Remove the right closeout / insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connectors from the multifunction alarm, lock, and lighting module.
3. Remove the module (1).

Pressing down on the center tab of the mounting bracket, slide downward the module until the rails disengage.

### Installation Procedure

1. Install the module (1).

Align the mounting rails on the module with the bracket, slide upward the module until the locking tab engages.

2. Connect the electrical connectors.
3. Install the right closeout / insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.