For 1990-2009 cars

# NEW DESIGN SECOND CLUTCH PISTON INNER SEAL

1984-1988 THM 440-T4 (ME9)

#### VEHICLE APPLICATIONS:

1984-88 Cutlass Ciera, Delta 88, Ninety-Eight, Toronado 1988 Cutlass Supreme

#### BULLETIN COVERS:

Service part information on a new second clutch piston inner seal (614B) for all 1984 through 1988 vehicles equipped with a THM 440-T4 transaxle. This new seal uses a different material (Viton TM) than the previous seal and can be identified by its part number (8668074) molded into the lip of the seal (Figure 2).

DATE OF PRODUCTION CHANGE: (Figure 1) -------------------------------------

October 30, 1987 (Julian Date 303), all 1988 THM 440-T4 transaxles were built using the new 2nd clutch piston inner seal (614B).

#### SERVICE ACTION:

When replacing the second clutch piston inner seal:

* 1984 through 1986 - Either the new second clutch piston inner seal or previous seal may be used.

* 1987 or 1988 - Only use the new second clutch piston inner seal (614B) contained in the service package listed in the Service Parts Information section.

#### SERVICE PARTS INFORMATION:

Service Package No. Contents ----------- -------- *8662935 (1) 2nd Clutch Piston Inner Seal (614B) (1) 2nd Clutch Piston Outer Seal (614A)

*NOTE: This seal package must be ordered when using the following overhaul packages:

- 8646975 Overhaul Seals and Gaskets Package - 8646976 Overhaul Repair Complete Package

Discard the 2nd clutch piston inner seal (614B) contained in these overhaul packages if it is not identified as shown in Figure 2.

#### SERVICE MANUAL REFERENCE:

Refer to the THM 440-T4 (ME9) Automatic Transaxle Unit Repair Table of Contents for 2nd clutch assembly service information.

#### SERVICE NOTES:

For warranty purposes, when replacing the second clutch seals use labor operation K7535. For this operation and to recondition the transaxle completely, refer to the appropriate labor time guide for applicable labor time information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.