For 1990-2009 cars

# MANUAL SEAT BACK RECLINER MOVEMENT

#### MODELS/YEARS 1987-89 EIGHTY-EIGHT AND NINETY-EIGHT MODELS

Some 1987-1989 Eighty-Eight and Ninety-Eight models equipped with manual seat back recliners may experience slight seat back movement.

To repair this condition replace the recliner assembly with the part numbers listed below:

Recliner Recliner Kit Kit Application (Eighty-Eight) (Ninety-Eight)

12501267 12501269 Coupe Recliner - Passenger 12501268 12501270 Coupe Recliner - Driver

12501271 12501273 Sedan Recliner - Passenger 12501272 12501274 Sedan Recliner - Driver

#### IMPORTANT: Each recliner kit contains a recliner and four bolts.

Parts are expected to be available on November 17, 1989. Until then, normal part orders will not be accepted by GMSPO. Only verifiable emergency VIP orders will be accepted. GMSPO will make every effort to obtain parts. All parts will be placed on 400 control to waive VIP surcharges. However, the part will be shipped premium transportation at dealer's expense. All other order types will be cancelled as incorrectly ordered while the 400 control is in place.

Refer to the appropriate Service Manual, for the installation procedure.

For warranty purposes use Labor Operation C651 0 at .7 hour for passenger recliners or C651 1 at .7 hour for the driver recliner.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.