For 1990-2009 cars

#### 4T60-E C/H car Comploc

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve | In transmission valve body. | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
2-3 Shift Solenoid Valve | In transmission valve body. | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission | LH side of the engine compartment | 7 - Automatic Transmission | 7 - Automatic Transmission | --
Automatic Transmission Fluid Temperature Sensor | In transmission valve body. | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Brake Switch Assembly | Below LH side of IP, on brake pedal support | 8A-201-27 Fig 50 | -- | --
IP Fuse Block | Behind LH side of IP, behind trim panel | 8A-201-23 Fig 43 | 8A-11-0 | --
Powertrain Control Module (PCM) | LH front of engine compartment, near evaporative emission (EVAP) canister | 6 - Engine Controls | -- | --
C1 (80 cavities) | Engine harness to PCM, LH front of engine compartment, near evaporative emission (EVAP) canister | -- | 6 - Engine Controls | --
C2 (80 cavities) | Engine harness to PCM, LH front of engine compartment, near evaporative emission (EVAP) canister | -- | 6 - Engine Controls | --
Relay Center | Behind RH side of IP, on multi-use bracket | 8A-201-29 Fig 54 | 8A-11-2 | --
RH Maxi® Fuse Block | Center rear of the engine compartment | 8A-201-11 Fig 21 | 8A-10-0 | --
Shift Select Switch | Below center console | -- | -- | --
C2 | I/P harness to shift select switch, below center console | -- | -- | --
Torque Converter Clutch Pulse Width Modulation Solenoid Valve (TCC PWM Sol. Valve) | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Torque Converter Clutch Solenoid Valve | In the transmission valve body | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Vehicle Speed Sensor | Lower RH rear of engine, near oil pressure sensor | 7 - Automatic Transmission Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
C101 (66 cavities) | RH rear of engine compartment, near A/C accumulator | 8A-201-28 Fig 53 | 8A-202-0 | --
C129 (7 cavities) | Engine harness to transmission, top LH rear of engine beside transmission | 7 - Automatic Transmission | 7 - Automatic Transmission | --
C200 (116 cavities) | Behind center of IP, right of the steering column | 8A-201-32 Fig 61 | 8A-202-3 | --
G202 | LH front of passenger compartment, center of kick panel | 8A-201-26 Fig 49 | -- | --
P100 | LH rear of engine compartment, behind strut tower | 8A-201-10 Fig 19 | -- | --
P101 | RH rear of engine compartment, near A/C accumulator | 8A-201-12 Fig 23 | -- | --
P102 | RH rear of engine compartment, near A/C accumulator | 8A-201-12 Fig 23 | -- | --
S104 | Body main harness, about 25 cm from cooling fan relay | 8A-201-11 Fig 22 | -- | --
S121 | Engine harness, about 32 cm from A/C accumulator | 8A-201-15 Fig 28 | -- | --
S130 | Engine harness, about 25.5 cm from A/C accumulator | 8A-201-15 Fig 28 | -- | --
S213 (Buick) | IP harness, about 4 cm from connector C200 behind center of IP, right of the steering column | 8A-201-32 Fig 61 | -- | --
S213 (Olds) | IP harness, about 12.5 cm from radio connector breakout | 8A-201-33 Fig 62 | -- | --
S213 (Pontiac) | IP harness, about 6 cm from IP compartment lamp connector breakout | 8A-201-33 Fig 63 | -- | --
S225 | Body main harness, about 33.5 cm from top edge of LH kick panel | 8A-201-26 Fig 49 | -- | --
S233 | Body main harness, about 22 cm from A/C accumulator | 8A-201-28 Fig 53 | -- | --
S239 | Body main harness, about 26 cm from center IP channel harness breakout | 8A-201-21 Fig 39 | -- | --
S241 | Body main harness, about 40 cm from lamp control module connector breakout | 8A-201-21 Fig 39 | -- | --
S918 | IP harness, about 12.5 cm from instrument panel cluster (IPC) connector C1 breakout | 8A-201-33 Fig 63 | -- | --