For 1990-2009 cars

# 1982 PAINT CODES INFORMATION

THE FOLLOWING IS A LIST OF PAINT CODE NUMBERS FROM VARIOUS SUPPLIERS FOR THE 1982 MODEL YEAR. THESE COLOURS CAN BE OBTAINED LOCALLY.

DUPONT REFINISH PAINTS ARE AVAILABLE IN:

L - LUCITE - ACRYLIC LACQUER A - CENTARI - ACRYLIC ENAMEL D - DELUX - ENAMEL

WHEN ORDERING DUPONT PAINT USE 'L' 'A' OR 'D' WITH THE APPROPRIATE DUPONT CODE

DITZLER REFINISH PAINTS ARE AVAILABLE IN:

DDL - DURACRYL - ACRYLIC LACQUER DAR - DELSTAR - ACRYLIC ENAMEL DQE - DITZCO - ALKYD ENAMEL DAU - DELTRON - ACRYLIC URETHANE

WHEN ORDERING DITZLER PAINT, USE 'DDL', 'DAR', 'DQE' OR 'DAU' WITH APPRO- PRIATE DITZLER CODE.

R-M REFINISH PAINTS ARE AVAILABLE IN:

A - ALPHA-CRYL - ACRYLIC LACQUER E - SUPER-MAX - ENAMEL

WHEN ORDERING R-M PAINT, USE 'A' OR 'E' WITH APPROPRIATE R-M NUMBER.

SHERWIN-WILLIAMS REFINISH PAINTS ARE AVAILABLE IN ACRYLIC LACQUER AND ACRYLIC ENAMEL.

USE: PREFIX 34, J4 OR L10 FOR ACRYLIC LACQUER. PREFIX 35, J5 OR F10 FOR ACRYLIC ENAMEL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.