For 1990-2009 cars

# COLUMN MOUNTED GEAR SHIFT LEVER TOO SHORT (NEW LEVERS)

#### SUBJECT COLUMN MOUNTED GEAR SHIFT LEVER TOO SHORT - INSTALL NEW DESIGN SHIFT LEVER

#### MODELS/YEARS 1992 EIGHTY EIGHT 1991-92 NINETY EIGHT

CONDITION: Some owners of 1992 Eighty Eight and 1991-92 Ninety Eight models may comment that the column mounted shift lever is too short.

CORRECTION: If an owner requests the longer, redesigned lever, install P/N 25609054. See the illustration below. Parts are currently available from GMSPO.

#### Note: The new lever is available only in black and is not intended to be painted.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.