For 1990-2009 cars

# TILT AND TELESCOPING STEERING WHEEL REPLACEMENT

A CONDITION MAY BE EXPERIENCED WHERE IT WILL BE NECESSARY TO REPLACE A DESIGN II STEERING WHEEL ON A 1983, 1984 AND 1985 DELTA 88 OR NINETY- EIGHT OLDSMOBILE. SHOULD THIS OCCUR, A DESIGN III STEERING WHEEL MUST BE INSTALLED IN PLACE OF THE DESIGN II STEERING WHEEL. REFER TO FIGURE 1. THREE (3) PART NUMBERS WILL BE REQUIRED FOR THE REPLACEMENT PROCEDURE. 1. STEERING WHEEL (SELECTED BY COLOR) 2. HORN PAD (SELECTED BY COLOR) 3. SERVICE PARTS PACKAGE - CONTAINS ALL NECESSARY HARDWARE PLUS THE LOWER SHROUD (PAINT TO MATCH) DESIGN III PARTS LIST SERVICE PARTS PACKAGE, P/N 22529953 INCLUDES: 1 LEVER ASSEMBLY 1611454 1 ADJUSTER ASSEMBLY 1607063 4 SCREWS 11502816 1 SHROUD (PAINT TO MATCH) 25521033 1 SPRING 1493502 2 SCREWS (4 REQ. REUSE 2 ORIGINAL) 11502843 DESIGN III STEERING WHEEL AND PAD DESIGN III COLOR WHEEL PAD DK. BR. BRWN. 22529908 22529913 W7504

22529907 22529912 DK. BLUE W7625

22528314 22528322 DK. MAPLE W7298

22529909 22529914 DR. GREYFERN W7621

22529910 22529915 DK. CHARCOAL W7713

22528311 22528316 MIDNIGHT SAGE W8581

22529301 22529302 DK. BEIGE W8258

22529911 22529916 DK. GRAPHITE W7701

STEERING WHEEL REPLACEMENT PROCEDURE REMOVE THE FOLLOWING DESIGN II PARTS, SEE FIGURE 1A: HORN PAD, STEERING WHEEL ASSEMBLY, SPRING SAVE THE FOLLOWING ITEMS FOR REUSE: TWO (2) SCREWS (HORN PAD) STEERING SHAFT NUT AND RETAINER INSTALLATION - FIGURE 1B. 1. PAINT SHROUD TO MATCH. 2. ASSEMBLE SHROUD TO ASSEMBLY WHEEL, USING SCREWS (11502816). 3. INSTALL SPRING AND STEERING WHEEL ON COLUMN. 4. TIGHTEN STEERING SHAFT NUT AND INSTALL RETAINER. 5. INSTALL LEVER AND ADJUSTER ASSEMBLY USING SCREWS (11502816). ADJUST FOR PROPER LOCK/RELEASE CONTROL OF TELESCOPE FEATURE. 6. INSTALL HORN CONTACT AND PAD ASSEMBLY. WARRANTY INFORMATION E7030 .4 HR. ADD .3 HR. TO PAINT SHROUD

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.