For 1990-2009 cars

#### Engine Component View -- Vin 1

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Idle Air Control (IAC) Valve
(3) | Mass Air Flow (MAF) Sensor
(4) | Throttle Position (TP) Sensor
(5) | Bypass Valve Actuator
(6) | Boost Control Solenoid
(7) | Ignition Control Module
(8) | Crankshaft Position (CKP) Sensor
(9) | Camshaft Position (CMP) Sensor
(10) | EVAP Canister Purge Valve
(11) | Heated Oxygen Sensor 1 (HO2S 1)
(12) | Manifold Absolute Pressure (MAP) Sensor
(13) | PCV Valve

#### Engine Component View Vin K

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Idle Air Control (IAC) Valve
(3) | Mass Air Flow (MAF) Sensor
(4) | Throttle Position (TP) Sensor
(5) | Engine Oil Level Switch
(6) | Ignition Control Module
(7) | Crankshaft Position (CKP) Sensor
(8) | Camshaft Position (CMP) Sensor
(9) | EVAP Canister Purge Valve
(10) | PCV Valve
(11) | Heated Oxygen Sensor 1 (HO2S 1)
(12) | Manifold Absolute Pressure (MAP) Sensor

Component Name | Location Refer to 8A-201 for Locator View
--- | ---
A/C Compressor Relay | Underhood Electrical Center
A/C Refrigerant Pressure Sensor | Right hand side of engine compartment, below A/C compressor
Bank 1 Knock Sensor (KS) | Front of engine, above starter
Bank 2 Knock Sensor (KS) | Lower RH rear of engine
Camshaft Position (CMP) Sensor | Right hand side of engine, below water pump
Crankshaft Position (CKP) Sensor | Lower right side of engine behind harmonic balancer
Data Link Connector (DLC) | On bottom of Instrument Panel, right of steering column
Engine Coolant Temperature (ECT) Sensor | Top left hand side of engine
Engine Oil Level Sensor | Front Center of engine oil pan near A/C compressor
EVAP Purge Valve | Top of engine
EVAP Vacuum Switch (All Except H Car with VIN K) | LH rear of engine
EVAP Canister Vent Valve (H Car with VIN K Only) | LH front of engine compartment, under PCM
Exhaust Gas Recirculation (EGR) Valve | Upper left hand side of engine
Fuel Injectors | Top of engine, mounted to fuel rail, at each cylinder intake port
Fuel Pressure Regulator | Mounted on the fuel rail, top LH side of engine
Fuel Pump/Fuel Level Sender | Mounted inside fuel tank
Fuel Pump Relay | I/P relay center
Fuel Pump Speed Control Module (VIN 1 Only) | LH Center of luggage compartment, behind rear seat
Fuel Tank Presure Sensor (H Car with VIN K Only) | Mounted in top of fuel tank
Fuse Block | LH side of instrument panel
Generator | Top RH side of engine
Heated Oxygen Sensor 1 (HO2S 1) | Rear of engine, in exhaust manifold
Heated Oxygen Sensor 2 (HO2S 2) | In exhaust system behind three way catalytic converter
High Speed Cooling Fan Relay | Rear center of engine compartment in underhood electrical center
Idle Air Control Valve (IAC) | Mounted to the throttle body assembly
Ignition Control Module (ICM) | RH side of engine
Ignition Control Module Ground | RH corner of engine, under ignition control module
Intake Air Temperature (IAT) Sensor | LH front of engine compartment, in air intake duct
LH Cooling Fan | LH side behind radiator
Low Engine Oil level Lamp | Instrument Panel Cluster
Low Speed Cooling Fan Relay | Rear center of engine compartment in underhood electrical center
Malfunction Indicator Lamp (MIL) | Instrument Panel Cluster
Manifold Absolute Pressure (MAP) Sensor (VIN 1) | Top rear of engine, on intake manifold
Manifold Absolute Pressure (MAP) Sensor (VIN K) | Top of engine, on crankcase ventilation valve cover
Mass Air Flow (MAF) Sensor | Mounted on throttle body
Powertrain Control Module (PCM) | Front LH corner of engine compartment.
Powertrain Control Module Ground | Bolt in engine block, rear of engine, left of oil filter adapter
Positive Crankcase Ventilation Valve (VIN 1) | Top RH side of engine, left of EGR valve
Positive Crankcase Ventilation Valve (VIN K) | Rear RH corner of engine, below Manifold Absolute Pressure (MAP) Sensor
RH Cooling Fan | RH side behind radiator
SMCC II Cruise Control Module | Mounted to bulkhead, rear LH side of engine compartment
TCC Brake Switch | Below LH side of I/P on brake pedal bracket
Theft Deterrent Module | Behind RH side of instrument panel, above glove compartment
Throttle Body | Mounted to the upper intake manifold, LH side of engine
Throttle Position (TP) Sensor | Mounted to throttle body assembly
Transaxle Range Switch / Park Neutral Position (PNP) Switch | Rear LH side of engine compartment, mounted to top of transaxle
Underhood Electrical Center | Rear center of engine compartment
Vehicle Speed Sensor (VSS) / Transaxle Output Speed Sensor (TOSS) | Mounted to transaxle below RH side of engine