For 1990-2009 cars

# CAMPAIGN: SHIFT INDICATOR ACTUATOR/TOURING SEDAN MODELS

CERTAIN 1988 OLDSMOBILE TOURING SEDAN MODELS

#### CONDITION

General Motors has determined that a defect which relates to motor vehicle safety may exist in some 1988 Oldsmobile Touring Sedan models. A clip on the shifter mechanism inside the console may become dislodged preventing indication of the correct gear under conditions of darkness. Also, there is a possibility this clip could bind part of the shifter mechanism in a way which would prevent the gear detents from operating; hence an inadvertent bump of the shifter could place the shifter in an undesired gear position. Either of these conditions could cause a vehicle crash without prior warning.

#### VEHICLES INVOLVED

Certain 1988 Oldsmobile Touring Sedan models within the following vehicle breakpoints:

Beginning Through and Including --------- -------------------- J4302017 J4311586

Approximately 1300 Touring Sedans were built between the above VIN breakpoints for sale in the United States. Of these, only 430 Touring Sedans will be affected by this product campaign.

Ninety-Eight Regencys and Ninety-Eight Regency Broughams between the above VIN breakpoints are NOT affected.

All vehicles listed on the dealer's campaign printout will require correction as outlined in the Service Procedure section of this bulletin.

Should a question exist concerning the campaign involvement of a specific vehicle(s) within the breakpoints listed above, dealers should call the Computerized Recall Information System (C.R.I.S.) for verification.

#### DEALER ACTION

Dealers are to replace the Clip, Transmission Shift Indicator Slot.

Dealers are to perform this campaign on all involved vehicles at no charge to owners, regardless of mileage, age of vehicle, or ownership from this time forward.

Whenever a vehicle subject to this campaign is taken into your new or used car inventory, or it is in your dealership for service, you are to ensure the campaign correction has been made before selling or releasing the vehicle.

Dealers are to contact owners of vehicles recently sold from your new vehicle inventory and arrange for the campaign correction to be performed.

#### SERVICE PROCEDURE

Instructions and illustration are based on a technician sitting in the driver's seat.

1. Place shift indicator in Park and set parking brake.

2. By hand, pull Transmission Control Dial, (1) in illustration, up out of console about 12 mm (1/2 inch). It "snaps" out. Then rotate the left edge of the dial plate upwards so the pin on the Transmission Control Indicator (2) comes out of the slot in the Clip, Transmission Shift Indicator Slot (3). Tilt Transmission Control Dial away from opening in console (it is not necessary to disconnect wires).

3. Using a small flat blade screwdriver if necessary, remove Clip, Transmission Shift indicator Slot (3).

Replace with new Clip (part number 25533234) and position it as shown in the illustration with the right hand tab against the right shaft of the shift lever. Be sure both locking tabs are fully seated.

4. Reverse Step 2., reinstalling Transmission Control Dial (1), taking care that the pin on the Transmission Control Indicator (2) engages the slot in the Clip (3).

5. Turn on ignition and headlights. Shield the shift indicator with a hand so the gear indicator light may be seen. Move the shift lever between gear positions and confirm that Transmission Control Indicator pin is engaged in the slot of the Clip (3).

Return the shift lever to Park position; turn off ignition and headlights.

6. Install a Campaign Identification Label.

#### CAMPAIGN IDENTIFICATION LABEL

Each label provides space to print the campaign number. and the five (5) digit dealer code of the dealer performing the campaign. Insert this information with a typewriter or ballpoint pen. When installing label, the campaign label where it is readily visible.

#### PARTS INFORMATION

Parts will be preshipped to those dealers having affected vehicles. Do not order parts from General Motors Service Parts Operations (GMSPO) unless the actual demand exceeds the stock sent; if necessary to order parts, place a C.I.O. order, with NO special instruction code, but order on an Advise Code (2). Use the following part number:

Description Part Number Quantity Per Vehicle ----------- ----------- --------------------

Clip, Transmission Shift 25533234 1 Indicator Slot

#### WARRANTY CLAIM INFORMATION

Pc PART-NO. TOT-PTS TC LAB-OP LHRS ST SUBLET -- ------- ------- -- ------ ----- -- ------ Replace Clip, Transmission Shift Indicator Slot

96 V4560 0.2* -- ---

*.1 hour for clerical administration may be added to the above operation.

Parts Allowance: A parts handling allowance of $.40 (30% of the dealer price of the preshipped "furnished" parts) may be applied for in the dealer material allowance column (Sublet Column) of the claim submission.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.