For 1990-2009 cars

# REMOTE KEYLESS ENTRY INOP (INSTALL NEW TRANSMITTER)

#### SUBJECT: REMOTE KEYLESS ENTRY (AUO) FOB PERFORMANCE (INSTALL NEW TRANSMITTER)

#### VEHICLES AFFECTED: 1991 "C" BUICK AND OLDSMOBILE MODELS

#### CONDITION:

---------- Owners of Buick and Oldsmobile "C" vehicles (built prior to 9/17/90) may comment about three possible conditions relating to the performance of the Key FOB (transmitter) for the Remote Keyless Entry System.

1. The case prematurely breaks at the attachment ring. 2. The transmitter may operate intermittently. 3. The useful range of operation is too short.

#### CORRECTION:

----------- A new transmitter has been released for service. Order part number #25602668.

If vehicle is being repaired under warranty use:

Labour Operation Time: .2 hr. (one or both)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.