For 1990-2009 cars

# WINDNOISE AT SUNROOF WEATHERSTRIP SEAL

#### SUBJECT: WINDNOISE AT SUNROOF WEATHERSTRIP SEAL - INSTALL NEW WEATHERSTRIP SEAL

#### MODELS/YEARS: 1991-93 NINETY EIGHT

CONDITION: Windnoise around sunroof weatherstrip seal.

CORRECTION: Install new slip coat weatherstrip seal, P/N 12536412, with Krytox coating.

o Follow service manual procedure in Section 10-9.

Parts are currently available from GMSPO.

Labor Operation Number: C1440

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.