For 1990-2009 cars

# SUPPLEMENTAL INFLATABLE RESTRAINT PARTS RETURN

#### MODELS/YEARS 1988-89 EIGHTY-EIGHT AND NINETY-EIGHT MODELS

Effective immediately, it is requested that SIR (supplemental inflatible restraint) parts listed in this bulletin, replaced for any reason other than deployment, be returned to the listed source. This request is being made so that General Motors and its suppliers can best satisfy our customers' expectations concerning quality.

This request includes 1988-1989 Eighty-Eight and 1989 Ninety-Eight cars equipped with the SIR option.

This request for the return of pans in no way implies that repairs or replacements will be covered under warranty beyond the original General Motors New Car Limited Warranty Coverage. Parts replaced beyond the warranty period should be returned only if the customer has no desire to retain the parts.

#### DELCO ELECTRONICS PARTS TO BE RETURNED

- IR Control Module (Passenger Compartment Sensor) 6072324; 16129674; 16130094

- Power Supply (Voltage Converter) 16072334; 18129684; 16130104

- Energy Reserve Module 16072344

- Forward Sensor 16072352; 16135684

- Arming Sensor 18077734

Address: Delco Electronics Division Truck Gate #4, Goyer Road Deliver to Reliability Engineering - Department 636 Mail Stop 6050 - Warranty Returns Kokomo, Indiana 46902

#### INLAND DIVISION PARTS TO BE RETURNED

- Inflator Module 17987134; 17987135; 17987136; 17987137; 17987138; 17988809; 17990899; 17990700

Address: Inflator Division-General Motors Division Main Receiving; Building 20 2525 Home Avenue Daylon, Ohio 45417 Attn: Bob Dunkle Building 13

#### SAGINAW DIVISION PARTS TO BE RETURNED:

- Steering Column Coil 26008744

Address: Saginaw Division- Plant #6 3900 Holland Avenue Saginaw, Michigan 48605 Attn: Carol Cook

These parts are to be returned to the designated source until further notice. The parts are to be repackaged in the service parts package and returned to the appropriate address. This is especially important when returning the Inflator Module to utilize the approved shipping carton the replacement part was received in. Deployed inflator Modules should be scrapped using normal scrapping procedures.

The following procedures should be followed when handling and shipping undeployed inflator modules:

#### INFLATOR MODULE

Live (Undeployed) Inflator Modules

Special care is necessary when handling and storing a live (undeployed) Inflator Module. The rapid gas generation produced during deployment of the air bag could cause the Inflator Module, or object in front of the inflator Module, to be thrown through the air in the unlikely event of an accidental deployment.

#### CAUTION:

When carrying a live inflator Module, make sure the bag and trim cover are pointed away from you. in case of an accidental deployment, the bag will then deploy with minimal chance of injury. When placing a live Inflator Module on a bench or other surface, always face the bag and trim cover up, away from the surface. This is necessary so that a free space is provided to allow the air bag to expand in the unlikely event of accidental deployment, otherwise personal injury may result. Also, never carry the Inflator Module by the wires or connector on the underside of the module.

Shipping Procedures for Live (Undeployed) Inflator Modules

The transportation of uninstalled Inflator Modules is regulated by the Hazardous Materials Regulations of the U.S. Department of Transportation (DOT) and most state governments. Special procedures are required for transportation. GENERAL MOTORS RECOMMENDS THAT THE DEALERS AND REPAIR SHOPS CHECK WITH THE HAZARDOUS MATERIAL SECTION OF THEIR RESPECTIVE STATE POLICE AUTHORITY FOR APPLICABLE SHIPPING REQUIREMENTS.

For all shipments on public roads, the DOT has classified the uninstalled Inflator Module as a flammable solid under a special exemption process. It should always be shipped and stored in the approved cardboard container in which it is purchased. The container should be marked with 'Flammable Solid, n.o.s., UN 1325, DOT-E8236" and labeled with the specffied red and white flammable solid label. Each shipping location must have a copy of the exemption on file. A shipping paper (e.g., a customer receipt) must accompany each shipment and identify the module as "Flammable Solid, n.o.s., UN1325, DOT- E8236". Transportation storage, and handling of the module should be in accordance with the exemption and the requiremnts for a DOT flammable solid. Do not expose the module to heat, open flame, impact, friction, or electrical charge.

Inflator Module Scrapping Procedures

#### CAUTION:

Failure to follow proper SIR Inflator Module disposal procedures can result in air bag deployment which may cause personal injury. Undeployed Inflator Modules must not be disposed of through normal refuse channels. The undeployed Inflator Module contains substances that can cause severe illness or personal injury of the sealed container is damaged during disposal. Disposal in any manner inconsistent with proper procedures may be a violation of federal, state, and/or local laws. It is the responsibility of those handling and disposing of the modules to ensure they comply with all applicable laws, rules, and regulations.

Claims are to be submitted using Labor Operation T4627 with Trouble Code 92. Freight expense must be listed in the sublet column. The dealer is responsible to retain and make available upon request the original paid receipts for freight costs.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.