For 1990-2009 cars

# TRAILER HITCH INST. DIFFICULTY (INSTALL ABSORBER & SPACER)

#### SUBJECT: TRAILER HITCH INSTALLATION DIFFICULTY (INSTALL SHORTER ENERGY ABSORBER AND SPACER)

#### MODELS: 1993 BUICK PARK AVENUE/PARK AVENUE ULTRA 1993 OLDSMOBILE NINETY EIGHT

#### CONDITION:

SOME VEHICLES MAY NOT ALLOW INSTALLATION OF A TRAILER HITCH.

#### CAUSE:

THE ENERGY ABSORBER WAS LENGTHENED AND A SPACER ELIMINATED. THE TRAILER HITCH MOUNTS IN PLACE OF THE SPACER. THE SHORTER ENERGY ABSORBER WITH A SPACER WAS RETURNED TO PRODUCTION AND HAS BEEN USED SINCE DECEMBER, 1992, CORRECTING THIS CONDITION.

#### CORRECTION:

REPLACE THE EXISTING PARTS WITH THE FOLLOWING PARTS TO ALLOW TRAILER HITCH INSTALLATION.

DESCRIPTION PART NUMBER =========== ===========

ENERGY ABSORBER - RIGHT SIDE 22136754 - LEFT SIDE 22136755

ATTACHING BOLTS (6 REQUIRED) 25609726

ATTACHING NUTS (6 REQUIRED) 11507036

EXHAUST HANGER 25559603

SPACER 25535925

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: B0967 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.