For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 6E3 REVISED DTC 61 AND 62 CHARTS

#### SUBJECT REVISED DTC 61 AND DTC 62 CHARTS

#### MODELS/YEARS 1993 EIGHTY EIGHT AND NINETY EIGHT WITH 3800 (VIN L) ENGINE

This bulletin updates the Diagnostic Trouble Code (DTC) 61 and DTC 62 Charts for 1993 Eighty Eight and Ninety Eight cars equipped with 3800 (VIN L) engine.

The following page numbers are affected:

DTC 61 Chart .......... 6E3 A-101 DTC 62 Chart .......... 6E3 A-1 03

On pages 6E3-A-l01 and 6E3-A-l03, the last two 'yes' and 'no' choice boxes should be interchanged, 'yes' becomes 'no' and 'no' becomes 'yes'.

On page 6E3-A-l03 in the last left side box, the abbreviation CKE should be CKT (circuit).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.