Fastener Tightening Specifications. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Filter Assembly Nut | 10 N·m | 89 Lb In
Camshaft Position Sensor | 10 N·m | 89 Lb In
Crankshaft Position (CKP) Sensors | 10 N·m | 89 Lb In
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 Lb Ft
EVAP Canister Purge Solenoid Bolt | 10 N·m | 88 Lb In
EVAP Canister Mounting Bracket Bolts | 9 N·m | 80 Lb In
Fuel Rail End-Point Bracket Bolt | 11 N·m | 97 Lb In
Fuel Rail Ground Wire Bolt | 6 N·m | 53 Lb In
Fuel Sender Mounting Nuts | 3 N·m | 27 Lb In
Heated Oxygen Sensor (HO2S) | 41 N·m | 30 Lb Ft
Idle Air Control Valve Attaching Bolts | 3 N·m | 27 Lb In
Ignition Coils | 3.5 N·m | 31 Lb In
Ignition Control Module Screws | 12 N·m | 106 Lb In
In-Line Fuel Filter Inlet and Outlet Nuts | 30 N·m | 22 Lb Ft
Intake Air Duct Clamp at MAF Filter | 3.5 N·m | 31 Lb In
Intake Air Duct Clamp at Air Cleaner | 1.8 N·m | 16 Lb In
Intake Manifold Bolts/Studs | 10 N·m | (89 Lb In)
Intake Manifold Top Cover Nuts | 3 N·m | 27 Lb In
Knock Sensor (KS) | 19 N·m | 14 Lb Ft
Relay Center Mounting Plate Bolts | 10 N·m | 89 Lb In
Rough Road Sensor | 19 N·m | 14 Lb Ft
Spark Plugs | 15 N·m | 11 Lb Ft
Throttle Body Attaching Bolts | 12 N·m | 106 Lb In
Throttle Body Spacer Attaching Bolts | 12 N·m | 106 Lb In
TP Sensor Attaching Screws | 2.3 N·m | 20 Lb In
Vehicle Speed Sensor (VSS) | 11 N·m | 97 Lb In