ROCKER PANEL REAR END CAPS LOOSE (NEW END CAP P/N). Oldsmobile Toronado 1990

For 1990-2009 cars

# ROCKER PANEL REAR END CAPS LOOSE (NEW END CAP P/N)

#### MODELS/YEARS 1990 TROFEO

Some 1990 Trofeos may experience a condition of loose rocker panel rear end caps. To repair this condition install an additional screw to the underside of the end cap as shown in the illustration on the back of this bulletin. If replacement is required, a modified end cap is available with the following part numbers:

Description Part Number

Cap-End Molding Outer Panel, Rocker RH 20750794 Cap-End Molding Outer Panel, Rocker LH 20750795

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.