FRONT DOOR WINDOW CLICKING OR CREAKING. Oldsmobile Toronado 1988

For 1990-2009 cars

# FRONT DOOR WINDOW CLICKING OR CREAKING

FRONT DOOR WINDOW CLICKING OR CREAKING

#### VEHICLES AFFECTED: 1988 E/K -----------------

Some 1988 E/K Cars may experience a clicking or creaking noise from the front door windows during either up or down travel. This condition may be caused by an incorrect surface finish of the counterbalance spring on the regulator assembly.

To repair this condition, replace the entire window regulator assembly with the part numbers listed below:

Right Side Left Side ---------- ---------

"E" Car: 20375834 20375835

Right Side Left Side

"K" Car: 20377438 20377439

Parts are currently available from CANSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.