CAMPAIGN: REAR SEAT EXTENDED RANGE SPEAKERS. Oldsmobile Toronado 1981

For 1990-2009 cars

# CAMPAIGN: REAR SEAT EXTENDED RANGE SPEAKERS

CONDITION GENERAL MOTORS HAS DETERMINED THAT SOME 1981 TORONADO MODELS ORDERED WITH ELECTRONICALLY TUNED RADIO'S (E.T.R.) OR OPTIONAL REAR DUAL EXTENDED RANGE SPEAKERS, (OPTION UQ1) MAY HAVE BEEN ASSEMBLED WITH THE INCORRECT SPEAKERS.

CARS AFFECTED

1981 TORONADO MODELS EQUIPPED WITH E.T.R. RADIO'S OR OPTION UQ1 BUILT AT THE LINDEN (E) ASSEMBLY PLANT FROM THE START OF PRODUCTION UP TO AND INCLUDING THE FOLLOWING VIN:

BE 306255

DEALER ACTION

DEALERS ARE TO REPLACE THE REAR SEAT SPEAKERS ON ALL VEHICLES LISTED ON THE PRINTOUT FURNISHED.

DEALERS ARE TO PERFORM THIS RECALL CAMPAIGN AT NO CHARGE TO THE OWNERS ON AFFECTED VEHICLES, REGARDLESS OF TIME, MILEAGE OR OWNERSHIP, AND ARE TO CORRECT ALL AFFECTED VEHICLES IN DEALER NEW AND USED CAR INVENTORY PRIOR TO THEIR SALE.

WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN IS TAKEN INTO YOUR NEW OR USED CAR INVENTORY IN THE FUTURE, YOU SHOULD TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE RESELLING THE VEHICLE.

DEALERS ARE TO PERFORM THE CAMPAIGN SERVICES ON ALL AFFECTED VEHICLES AS THEY ARE BROUGHT IN FOR ANY KIND OF SERVICE UNTIL ALL AFFECTED VEHICLES HAVE BEEN CORRECTED.

SERVICE PROCEDURE

THE EXTENDED RANGE SPEAKERS CAN BE IDENTIFIED BY THE MAGNET SIZE, THE STANDARD SPEAKER HAS A 2 1/4" MAGNET AND THE EXTENDED RANGE SPEAKER HAS A 3 1/4" MAGNET AS MEASURED ACROSS THE DIAMETER OF THE MAGNET.

1. OPEN DECK LID AND DISCONNECT ELECTRICAL ATTACHMENTS TO BOTH SPEAKERS AND REMOVE SPEAKERS.

2. INSTALL NEW SPEAKERS AND MAKE ELECRTRICAL CONNECTIONS.

3. INSTALL YELLOW CORRECTION LABEL 81-C-7 ON THE RADIATOR BAFFLE WHERE IT IS READILY VISIBLE.

PARTS INFORMATION

PARTS ARE TO BE OBTAINED AS REQUIRED FROM GENERAL MOTORS PARTS (GMWDD):

SPEAKER 22511166 (2 PER CAR)

TO INSURE THESE PARTS WILL BE OBTAINED AS SOON AS POSSIBLE, THEY SHOULD BE ORDERED FROM GMWDD ON A C.I.O. ORDER WITH NO SPECIAL INSTRUCTION CODE, BUT ORDER ON AN ADVISE CODE (2).

PARTS REMOVED FROM THE INVOLVED VEHICLES ARE TO BE HELD FOR DISPOSTION BY AN OLDSMOBILE REPRESENTATIVE.

WARRANTY CLAIM INFORMATION

DEALERS ARE TO SUBMIT CLAIMS ON THE CAMPAIGN CARD FURNISHED WITH THE PRINTOUT USING THE FOLLOWING INFORMATION. PARTS CREDIT WILL BE ISSUED AUTOMATICALLY. PARTS WILL BE CREDITED AT DEALER NET, PLUS 30% DEALER HANDLING ALLOWANCE.

OPERATION TIME

V0760 REPLACE TWO REAR SEAT SPEAKERS .3

.1 HOUR FOR CLERICAL ADMINISTRATION WILL BE ADDED TO THE ABOVE OPERATION. TO SUBMIT A CLAIM ON CARS CORRECTED BUT NOT ON YOUR PRINTOUT, USE A YELLOW STRIPE CARD.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.