CAMPAIGN: FRONT LEFT UPPER CONTROL ARM NUTS. Oldsmobile Toronado 1981

For 1990-2009 cars

# CAMPAIGN: FRONT LEFT UPPER CONTROL ARM NUTS

CONDITION

GENERAL MOTORS HAS DETERMINED THAT A DEFECT WHICH RELATES TO MOTOR VEHICLE SAFETY EXISTS IN SOME 1981 TORONADO MODELS. THE FRONT LEFT UPPER CONTROL ARM NUTS MAY NOT HAVE BEEN TIGHTENED TO THE SPECIFIED TORQUE. THERE IS A POSSIBILITY THAT THESE NUTS MAY LOOSEN AND COME OFF. WITH ADDITIONAL DRIVING, THE CONTROL ARM FRONT BOLT MAY EVENTUALLY WORK ITS WAY OUT OF POSITION. THIS WOULD CAUSE NOTICEABLE CHANGES IN STEERING CONTROL DURING ACCELERATION AND CORNERING. WHILE IT IS DOUBTFUL STEERING WOULD BE LOST, REDUCED CONTROLLABILITY COULD OCCUR. IF THIS WARNING OF THE NEED FOR REPAIRS IS NOT HEEDED, A VEHICLE CRASH CAN OCCUR.

CARS AFFECTED

CERTAIN 1981 OLDSMOBILE TORONADO MODELS BUILT AT LINDEN (E) ASSEMBLY PLANT BETWEEN THE FOLLOWING VIN NUMBERS.

BE314140-BE316302

DEALER ACTION

DEALERS ARE TO TORQUE BOTH FRONT LEFT SIDE UPPER CONTROL ARM NUTS AS DIRECTED IN THE SERVICE PROCEDURE OF THIS BULLETIN.

DEALERS ARE TO PERFORM THIS RECALL CAMPAIGN AT NO CHARGE TO THE OWNER ON AFFECTED VEHICLES, REGARDLESS OF TIME, MILEAGE OR OWNERSHIP, AND ARE TO CORRECT ALL AFFECTED VEHICLES IN DEALER NEW AND USED CAR INVENTORY PRIOR TO THEIR SALE.

WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN IS TAKEN INTO YOUR NEW OR USED CAR INVENTORY IN THE FUTURE, YOU SHOULD TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE RESELLING THE VEHICLE.

DEALERS ARE TO PERFORM THE CAMPAIGN SERVICES ON ALL AFFECTED VEHICLES AS THEY ARE BROUGHT IN FOR ANY KIND OF SERVICE UNTIL ALL AFFECTED VEHICLES HAVE BEEN CORRECTED.

SERVICE PROCEDURE

1. RAISE THE VEHICLE ALLOWING THE FRONT WHEELS TO DROP DOWN.

2. HOLD LEFT UPPER CONTROL ARM BOLT HEAD TO INSURE BOLT DOES NOT MOVE AND TORQUE BOTH LEFT UPPER CONTROL ARM NUTS TO 95 N.M (70 FT. LBS.). LOWER VEHICLE.

3. INSTALL YELLOW CORRECTION LABEL 81-C-10 ON THE RADIATOR BAFFLE WHERE IT IS READILY VISIBLE.

WARRANTY INFORMATION

DEALERS ARE TO SUBMIT CLAIMS ON THE CAMPAIGN CARD FURNISHED WITH THE PRINT- OUT USING THE FOLLOWING INFORMATION.

OPERATION V0880 TORQUE BOTH LEFT UPER CONTROL ARM NUTS .2 HR.

.1 HOUR FOR CLERICAL ADMINISTRATION WILL BE ADDED TO THE ABOVE OPERATION. TO SUBMIT A CLAIM ON CARS CORRECTED BUT NOT ON YOUR PRINTOUT, USE A YELLOW STRIPE CARD.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.