For 1990-2009 cars

The procedures below are designed to program the BCM correctly during BCM related service. Before you start, read these procedures carefully and completely.

Important: The vehicle will not start and many other functions may not operate properly if a replacement BCM is not properly set up. The following procedures must be followed:

1. Programming the BCM
2. Learning the restraints ID

#### Programming the BCM

From the Main Menu, select Service Programming System, then follow the instructions on the screen.

#### Learning the Restraints ID

Navigate on the scan tool to Body, Body Control Module, Programming, SDM ID, then follow the instructions on the screen.