For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint To Control Arm Nuts and Bolts | 68 N·m | 50 lb ft
Brake Hose Bracket To Strut Bolt | 15 N·m | 11 lb ft
Control Arm Ball Joint To Knuckle Nut | 10 N·m | 89 lb in
Control Arm To Cradle Front Nuts and Bolts | 120 N·m | 89 lb ft
Control Arm To Cradle Rear Nuts and Bolts | 70 N·m | 52 lb ft
Hub To Axle Shaft Nut | 205 N·m | 157 lb ft
Hub To Knuckle Bolts | 115 N·m | 85 lb ft
Outer Tie Rod To Knuckle Nut | 50 N·m | 37 lb ft
Stabilizer Link Nuts | 85 N·m | 63 lb ft
Stabilizer Shaft Insulator Bracket To Cradle Bolts | 50 N·m | 37 lb ft
Strut Shaft Nut | 75 N·m | 55 lb ft
Strut To Body Nuts | 30 N·m | 22 lb ft
Strut To Knuckle Nuts and Bolts | 180 N·m | 133 lb ft