For 1990-2009 cars

Connector 1: | Accelerator Pedal Position Sensor
Connector 2: | Camshaft Position (CMP) Sensor
Connector 3: | Crankshaft Position (CKP) Sensor
Connector 4: | Electronic Throttle Control
Connector 5: | Engine Coolant Temperature (ECT) Sensor
Connector 6: | EVAP Canister Purge Solenoid Valve
Connector 7: | Exhaust Gas Recirculation (EGR) Valve
Connector 8: | Fuel Injector 1
Connector 9: | Fuel Injector 2
Connector 10: | Fuel Injector 3
Connector 11: | Fuel Injector 4
Connector 12: | Fuel Pump Module
Connector 13: | Heated Oxygen Sensor (HO2S) 1
Connector 14: | Heated Oxygen Sensor (HO2S) 2
Connector 15: | Ignition Coil Module
Connector 16: | Intake Air Temperature (IAT) Sensor
Connector 17: | Knock Sensor
Connector 18: | Manifold Absolute Pressure (MAP) Sensor
Connector 19: | Oil Level Sensor
Connector 20: | Oil Pressure Switch

### Accelerator Pedal Position Sensor

#### Connector Part Information

- OEM: PED 15326830
- Service: N/A
- Description: 6-Way F GT 150 Unsealed

#### Accelerator Pedal Position Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BK | -- | Accelerator Pedal Position 5-Volt Reference 1
2 | D-BU | -- | Accelerator Pedal Position Signal 1
3 | BN | -- | Accelerator Pedal Position Low Reference 1
4 | PU | -- | Accelerator Pedal Position Low Reference 2
5 | L-GN | -- | Accelerator Pedal Position Signal 2
6 | BN | -- | Accelerator Pedal Position 5-Volt Reference 2

### Camshaft Position (CMP) Sensor

#### Connector Part Information

- OEM: KET MG640541-5
- Service: N/A
- Description: 3-Way F ITC Sealed

#### Camshaft Position (CMP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (3)
2 | BK/WH | -- | Camshaft Position Sensor Low Reference
3 | BN/WH | -- | Camshaft Position Sensor Signal

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Crankshaft POS Sensor Signal (3)
2 | YE/BK | -- | Crankshaft POS Sensor Low Reference (3)
3 | BK/WH | -- | Signal Ground

### Electronic Throttle Control

#### Connector Part Information

- OEM: FEP 42121700
- Service: N/A
- Description: 6-Way F Sealed

#### Electronic Throttle Control

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference
2 | GN | -- | TPS 1 Signal
3 | BK | -- | Low Reference
4 | BU | -- | TPS 2 Signal
5 | L-BU | -- | Idle Speed Motor Control Extend
6 | BU/BK | -- | Idle Speed Motor Control Retract

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: PKI 832238
- Service: N/A
- Description: 2-Way F 150.2 Sealed

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Engine Coolant Temperature Sensor Signal
2 | BN | -- | Sensor Low Reference

### EVAP Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: PKI 832229
- Service: N/A
- Description: 2-Way F Sealed

#### EVAP Canister Purge Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/WH | -- | Engine Main Relay Fused Control (3)
2 | D-GN/WH | -- | EVAP Canister Purge Solenoid Control

### Exhaust Gas Recirculation (EGR) Valve

#### Connector Part Information

- OEM: PKI 832503
- Service: N/A
- Description: 5-Way F 150 Sealed

#### Exhaust Gas Recirculation (EGR) Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | Exhaust Gas Recirculation Solenoid Control
2 | BN | -- | Sensor Low Reference
3 | GY | -- | Exhaust Recirculation Vacuum Regul Valve Signal
4 | GY | -- | 5-Volt Reference
5 | PK/BK | -- | Engine Main Relay Fused Controls (3)

### Fuel Injector 1

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (1)

### Fuel Injector 2

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | BN/WH | -- | Fuel Injector Control (3)

### Fuel Injector 3

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (4)

### Fuel Injector 4

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (2)

### Fuel Pump Module

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition Voltage
2 | BN/WH | -- | Fuel Level Sensor Low
3 | D-BU | -- | Primary Fuel Level Sensor
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: TYCO 174257-2
- Service: N/A
- Description: 4-Way F MARK-II Sealed

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated O2 Sensor High Signal Bank 1 Sensor 1
2 | PKBK | -- | Engine Main Relay Fused Control (2)
3 | BN/WH | -- | Heated O2 Sensor Low Signal Bank 1 Sensor 2
4 | D-GN | -- | Heated O2 Sensor Control Sensor 1

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP Sealed

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated O2 Sensor High Signal Bank 1 Sensor 2
2 | PK/BK | -- | Engine Main Relay Fused Control (2)
3 | BN/WH | -- | Heated O2 Sensor Low Signal Bank 1 Sensor 1
4 | L-BU | -- | Heated O2 Sensor Control Sensor 2

### Ignition Coil Module

#### Connector Part Information

- OEM: PKI 832311
- Service: N/A
- Description: 3-Way F 150 Sealed

#### Ignition Coil Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | -- | Ignition Coil 2 and 3 Control
2 | PK | -- | Run/Crank Ignition 1 Voltage
3 | L-BU | -- | Ignition Coil 1 and 4 Control

### Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: TYCO 85202-1
- Service: N/A
- Description: 2-Way F Sealed

#### Intake Air Temperature (IAT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | -- | Intake Air Temperature Sensor Low Reference
2 | BN | -- | Intake Air Temperature Sensor Signal

### Knock Sensor

#### Connector Part Information

- OEM: TYCO 368215-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Knock Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | -- | Knock Sensor Signal (1)
2 | BN | -- | Sensor Low Reference
3 | BK/WH | -- | Signal Ground

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: TYCO 174359-2
- Service: N/A
- Description: 3-Way F Mark II Sealed

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference
2 | L-GN | -- | Signal
3 | OG/BK | -- | Low Reference

### Oil Level Sensor

#### Connector Part Information

- OEM: PED 15326808
- Service: N/A
- Description: 3-Way F GT 150 Sealed

#### Oil Level Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Sensor Low Reference
2 | D-GN/WH | -- | Oil Temperature Sensor Signal
3 | BN | -- | Oil Level Switch Signal

### Oil Pressure Switch

#### Connector Part Information

- OEM: PKI 832104
- Service: N/A
- Description: 1-Way F 150 Sealed

#### Oil Pressure Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Oil Pressure Gage Signal