For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Jounce Bumper to Body Panel Hexagon Bolt | 15 N·m | 11 lb ft
Knuckle to Lower Control Arm Bolt | 160 N·m | 118 lb ft
Knuckle to Toe Link Bolt | 160 N·m | 118 lb ft
Knuckle to Trailing Arm Bolt | 110 N·m | 81 lb ft
Knuckle to Upper Control Arm Bolt | 160 N·m | 118 lb ft
Lower Control Arm to Support Assembly Bolt | 110 N·m | 81 lb ft
Lower Shock Bolt | 110 N·m | 81 lb ft
Park Brake Cable Clip | 25 N·m | 18 lb ft
Stabilizer Link to Lower Control Arm Nut | 15 N·m | 11 lb ft
Stabilizer Link to Stabilizer Shaft Nut | 57 N·m | 42 lb ft
Stabilizer Shaft Clamp Bolt | 70 N·m | 52 lb ft
Support to Body Bolts | 170 N·m | 125 lb ft
Toe Link to Support Bolts | 160 N·m | 118 lb ft
Trailing Arm Bracket to Body Bolts | 110 N·m | 81 lb ft
Trailing Arm Bushing to Bracket Bolt | 160 N·m | 118 lb ft
Upper Control Arm to Support Assembly Bolts | 160 N·m | 118 lb ft
Upper Shock Bolts | 110 N·m | 81 lb ft
Wheel Bearing/Hub Mounting Bolts - Rear | 84 N·m | 62 lb ft
Wheel Drive Shaft Spindle Nut | 205 N·m | 151 lb ft