For 1990-2009 cars

## Fluid and Lubricant Recommendations C100/Long Body Except Europe, Holden

Application | Fluid/Lubricant
--- | ---
Engine Oil

- Gasoline Engine

• | 0W-30

• | 0W-40

• | 5W-30

• | 5W-40

• | ACEA A3/B3

• | ACEA A3/B4

- Diesel Engine

• | 0W-40

• | 5W-40

• | ACEA C3

Engine Coolant | DEX-COOL® Coolant
Brake Fluid | DOT-4
Clutch Fluid | DOT-4
Power Steering System Fluid | DEXRON® II-D or DEXRON® III
Automatic Transaxle | JWS 3309 US ATF or JWS 3317
Manual Transaxle | SAE 75W-90
Transfer Case | Synthetic Hypoid 75W-90
Differential Carrier Assembly | Synthetic Hypoid 75W-90
Manual Transaxle Shift Linkage | Silicone Grease
Key Lock Cylinders | Silicone Grease
Automatic Transaxle Shift Linkage | Silicone Grease
Floor Shift Linkage Points | Engine Oil
Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

- Hood and Door Hinges
- Fuel Door Hinge
- Rear Compartment Lid Hinges

Engine Oil

Weatherstripping | Silicone Grease

## Fluid and Lubricant Recommendations C100/Long Body Europe

Application | Fluid/Lubricant
--- | ---
Engine Oil

- Gasoline Engine

• | 0W-30

• | 0W-40

• | 5W-30

• | 5W-40

• | ACEA A3/B3

• | ACEA A3/B4

- Diesel Engine

• | 0W-40

• | 5W-40

• | ACEA C3

Engine Coolant | DEX-COOL® Coolant
Brake Fluid | DOT-4
Clutch Fluid | DOT-4
Power Steering System Fluid | DEXRON® II-D or DEXRON® III
Automatic Transaxle | JWS 3309 US ATF
Manual Transaxle | SAE 75W-90
Transfer Case | Synthetic Hypoid 75W-90
Differential Carrier Assembly | Synthetic Hypoid 75W-90
Manual Transaxle Shift Linkage | Silicone Grease
Key Lock Cylinders | Silicone Grease
Automatic Transaxle Shift Linkage | Silicone Grease
Floor Shift Linkage Points | Engine Oil
Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

- Hood and Door Hinges
- Fuel Door Hinge
- Rear Compartment Lid Hinges

Engine Oil

Weatherstripping | Silicone Grease

## Fluid and Lubricant Recommendations C105/Short Body Except Holden

Application | Fluid/Lubricant
--- | ---
Engine Oil

- Gasoline Engine

• | 0W-30

• | 0W-40

• | 5W-30

• | 5W-40

• | ACEA A3/B3

• | ACEA A3/B4

- Diesel Engine

• | 0W-40

• | 5W-40

• | ACEA C3

Engine Coolant | DEX-COOL® Coolant
Brake Fluid | DOT-4
Clutch Fluid | DOT-4
Power Steering System Fluid | DEXRON® II-D
Automatic Transaxle | JWS 3309 US ATF
Manual Transaxle | SAE 75W-90
Transfer Case | Synthetic Hypoid 75W-90
Differential Carrier Assembly | Synthetic Hypoid 75W-90
Manual Transaxle Shift Linkage | Silicone Grease
Key Lock Cylinders | Silicone Grease
Automatic Transaxle Shift Linkage | Silicone Grease
Floor Shift Linkage Points | Engine Oil
Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

- Hood and Door Hinges
- Fuel Door Hinge
- Rear Compartment Lid Hinges

Engine Oil

Weatherstripping | Silicone Grease

## Fluid and Lubricant Recommendations C100/C105 Holden

Application | Fluid/Lubricant
--- | ---
Engine Oil

- Gasoline Engine

• | SAE 5W/30

• | SAE 10W/30

• | API SL

• | API SM

• | ILSAC GF3

- Diesel Engine

• | 0W/40

• | 5W/40

• | ACEA C3

Engine Coolant | DEX-COOL® Coolant
Brake Fluid | DOT-4
Clutch Fluid | DOT-4
Power Steering System Fluid | DEXRON® III
Automatic Transaxle | JWS 3309 or conforming to Holden spec HN2414
Manual Transaxle | SAE 75W/90 (GL5)
Transfer Case | Synthetic Hypoid 75W-90 (GL5)
Differential Carrier Assembly | Synthetic Hypoid 75W-90 (GL5)
Manual Transaxle Shift Linkage | Silicone Grease
Key Lock Cylinders | Silicone Grease
Automatic Transaxle Shift Linkage | Silicone Grease
Floor Shift Linkage Points | Engine Oil
Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose-type grease meeting requirements NLGI No. 1 or 2

- Hood and Door Hinges
- Fuel Door Hinge
- Rear Compartment Lid Hinges

Engine Oil

Weatherstripping | Silicone Grease