For 1990-2009 cars

## Scan Tool Output Controls Except Holden

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
LF Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
Pump Motor | -- | Commands the pump motor ON and OFF.
RF Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RF Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RR Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RR Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.

## Scan Tool Output Controls Holden

#### Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Return Pump Relay Test | Chassis / Actuator Test | Commands the pump motor ON and OFF.
Front Left Solenoid Valve Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Front Right Solenoid Valve Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Rear left Solenoid Valve Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Rear Right Solenoid Valve Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Front Left ESP Channel Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Front Right ESP Channel Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Rear Left ESP Channel Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.
Rear Right ESP Channel Test | Chassis / Actuator Test | Commands the solenoid ON and OFF.