For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the roof console assembly. Refer to Roof Console Replacement.

1 | Reading Lamp Lens

#### Procedure

Use a plastic flat-bladed tool to remove the lens.

2 | Mobile Communication Trim Cover

#### Procedure

Use a plastic flat-bladed tool to remove the cover.

3 | Reading Lamp Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
4 | Reading Lamp Housing
5 | Sun Roof Switch Screw (Qty: 3) Tighten 2 N·m (18 lb in)
6 | Sun Roof Switch Assembly