For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the sunroof window.

1 | Sunroof Air Deflector

#### Procedure

1. Push down on the right front side of the air deflector.
2. While pushing down on the right front side of air deflector. Lift up on the air deflector, releasing air deflector from the roof.
3. Remove the air deflector springs for the sunroof frame on both sides.

Tip:
Do not lift up on the spring of the air deflector with a strong force, the spring can be damaged.