For 1990-2009 cars

Table 1: | Turbine Shaft, Reluctor Wheel and Piston Removal
Table 2: | 4-5-6 Clutch Plate Removal
Table 3: | 4-5-6 Clutch Piston Removal
Table 4: | Reluctor Wheel and Piston Removal
Table 5: | 3-5 Reverse Clutch Plate Removal

### Turbine Shaft, Reluctor Wheel and Piston Removal

Callout | Component Name
--- | ---
1 | Turbine Shaft Retainer Ring Tip Discard the retainer ring. It is not re-usable.

#### Special Tools

J-5586-A Snap Ring Pliers or equivalent

2 | Turbine Shaft
3 | Reaction Carrier Hub Assembly
4 | Reaction Carrier Hub Thrust Bearing Assembly

### 4-5-6 Clutch Plate Removal

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Backing Plate Retaining Ring
2 | 4-5-6 Clutch Backing Plate
3 | 4-5-6 Clutch Plate Assembly (Qty: 4)
4 | 4-5-6 Clutch Plate (Qty: 3)
5 | 4-5-6 Clutch Apply Plate
6 | 4-5-6 Clutch Wave Plate

### 4-5-6 Clutch Piston Removal

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Dam Retaining Ring

#### Special Tools

• | DT-47951-2 Spring Compressor

• | J-5586-A Snap Ring Pliers or equivalent

2 | 4-5-6 Clutch Piston Fluid Dam Assembly Tip

1. Place the 3-5 reverse and 4-5-6 clutch housing onto the support hub in the case.
2. Apply shop air to the 4-5-6 clutch feed hole using a rubber tipped air gun to dislodge the dam piston and the 4-5-6 clutch piston from the clutch housing.

3 | 4-5-6 Clutch Piston Return Spring Assembly
4 | 4-5-6 Clutch Piston Tip Apply shop air to the 4-5-6 clutch feed hole using a rubber tipped air gun to dislodge the clutch piston.
5 | 4-5-6 Clutch Piston Inner Seal
6 | 4-5-6 Clutch Piston Outer Seal (DK Blue) (Stepped)
7 | 4-5-6 Clutch Piston Outer Seal (Large) (Rounded)

### Reluctor Wheel and Piston Removal

Callout | Component Name
--- | ---
1 | Input Shaft Speed Sensor Reluctor Ring Retainer Ring Caution: Compress the reluctor wheel just enough to clear the retainer. Over compressing the reluctor wheel will break the alignment tab and the clutch housing.

#### Special Tools

DT-47694 Piston Spring Compressor

2 | Input Shaft Speed Sensor Reluctor Wheel
3 | 3-5 Reverse Clutch Piston
4 | 3-5 Reverse Clutch Piston Return Spring Assembly
5 | 3-5 Reverse Clutch Piston Inner (Reluctor) Seal (Orange)
6 | 3-5 Reverse Clutch Piston Inner Seal
7 | 3-5 Reverse Clutch Piston Dam Seal (Black)

### 3-5 Reverse Clutch Plate Removal

Callout | Component Name
--- | ---
1 | 3-5 Reverse Clutch Backing Plate Ring Retainer Ring Tip Gently push down on the backing plate to get enough clearance between the backing plate and retainer.
2 | 3-5 Reverse Clutch Backing Plate
3 | 3-5 Reverse Clutch Plate Assembly (Qty: 3)
4 | 3-5 Reverse Clutch Plate (Qty: 3)
5 | 3-5 Reverse Clutch Apply Plate (Waved)