For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
2. Remove the driver information center bezel. Refer to Driver Information Display Bezel Replacement .
3. Remove the screws and the instrument panel lower compartment.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the instrument lower compartment with the screws.

Tighten
Tighten the instrument lower compartment with the screws to 2 N·m (18 lb in).

2. Install the instrument panel driver information center bezel. Refer to Driver Information Display Bezel Replacement .
3. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .