For 1990-2009 cars

Connector 1: | A/C Compressor
Connector 2: | A/C Refrigerant Pressure Sensor 2.0L
Connector 3: | Accelerator Pedal Position Sensor
Connector 4: | Alarm
Connector 5: | Ambient Light Sensor (w/C60)
Connector 6: | Ambient Light/Sunload Sensor (with C68)
Connector 7: | Audio Amplifier
Connector 8: | Backup Lamp Switch
Connector 9: | Body Control Module (BCM) X1
Connector 10: | Body Control Module (BCM) X2
Connector 11: | Body Control Module (BCM) X3
Connector 12: | Body Control Module (BCM) X4
Connector 13: | Body Control Module (BCM) X5
Connector 14: | Body Control Module (BCM) X6
Connector 15: | Body Control Module (BCM) X7
Connector 16: | Boost Pressure Sensor (2.0L Diesel)
Connector 17: | Brake Fluid Level Switch
Connector 18: | Camshaft Position (CMP) Sensor (2.0L Diesel)
Connector 19: | Camshaft Position (CMP) Sensor (2.4L)
Connector 20: | Camshaft Position (CMP) Sensor (2.4L)
Connector 21: | Center High Mounted Stop Lamp (CHMSL)
Connector 22: | Cigar Lighter
Connector 23: | Clock
Connector 24: | Clutch Start Switch
Connector 25: | Contact Coil
Connector 26: | Contact Coil
Connector 27: | Cooling Fan - Auxiliary
Connector 28: | Cooling Fan - Main
Connector 29: | Crankshaft Position (CKP) Sensor (2.0L Diesel)
Connector 30: | Crankshaft Position (CKP) Sensor (2.4L)
Connector 31: | Data Link Connector
Connector 32: | Diesel Particulate Filter Pressure Sensor (2.0L Diesel)
Connector 33: | Dome Lamp
Connector 34: | Door Latch - Driver
Connector 35: | Door Latch - Driver (w/Dead Locking)
Connector 36: | Door Latch - Left Rear
Connector 37: | Door Latch - Passenger
Connector 38: | Door Latch - Right Rear
Connector 39: | Door Lock Switch - Driver
Connector 40: | Driver Information Center (C100/Long Body)
Connector 41: | Driver Information Center (C105/Short Body)
Connector 42: | Electronic Brake Control Module (EBCM)
Connector 43: | Engine Control Module (ECM) X1 (LD9)
Connector 44: | Engine Control Module (ECM) X1 (LLW)
Connector 45: | Engine Control Module (ECM) X1 (LU1)
Connector 46: | Engine Control Module (ECM) X2 (LD9)
Connector 47: | Engine Control Module (ECM) X2 (LLW)
Connector 48: | Engine Control Module (ECM) X2 (LU1)
Connector 49: | Engine Coolant Temperature (ECT) Sensor (2.0L Diesel)
Connector 50: | Engine Coolant Temperature (ECT) Sensor (2.4L)
Connector 51: | Engine Oil Pressure Sensor (LU1)
Connector 52: | EVAP Canister Purge Solenoid Valve (2.4L)
Connector 53: | EVAP Canister Purge Solenoid Valve (3.2L)
Connector 54: | Exhaust Gas Recirculation (EGR) Valve (2.0L Diesel)
Connector 55: | Exhaust Gas Recirculation (EGR) Valve (2.4L)
Connector 56: | Exhaust Gas Temperature Sensor I (2.0 Diesel)
Connector 57: | Exhaust Gas Temperature Sensor 2 (2.0L Diesel)
Connector 58: | Fog Lamp
Connector 59: | Folding Mirror Unit
Connector 60: | Fuel Door Lock Actuator
Connector 61: | Fuel Filter Heater/Temperature Sensor (2.0L Diesel)
Connector 62: | Fuel Injector 1 (2.0L Diesel)
Connector 63: | Fuel Injector 1 (2.4L)
Connector 64: | Fuel Injector 2 (2.0L Diesel)
Connector 65: | Fuel Injector 2 (2.4L)
Connector 66: | Fuel Injector 3 (2.0L Diesel)
Connector 67: | Fuel Injector 3 (2.4L)
Connector 68: | Fuel Injector 4 (2.0L Diesel)
Connector 69: | Fuel Injector 4 (2.4L)
Connector 70: | Fuel Pump Module (2.4L)
Connector 71: | Fuel Pump Module (2.0L Diesel)
Connector 72: | Fuel Pump Module (3.2L)
Connector 73: | Fuel Rail Pressure Control Valve (2.0L Diesel)
Connector 74: | Fuel Rail Pressure Sensor (2.0L Diesel)
Connector 75: | Fuel Tank Pressure Sensor (3.2L)
Connector 76: | Generator
Connector 77: | Glow Plug Control Unit (2.0L Diesel)
Connector 78: | Hands Free Unit
Connector 79: | Hazard Switch
Connector 80: | Head Lamp Washer Pump
Connector 81: | Headlamp - Left
Connector 82: | Headlamp - Left (w/Leveling)
Connector 83: | Headlamp - Right
Connector 84: | Headlamp - Right (w/Leveling)
Connector 85: | Heated Oxygen Sensor HO2S 1 (2.4L)
Connector 86: | Heated Oxygen Sensor (HO2S) 2 (2.4L)
Connector 87: | Heated Oxygen Sensor Bank 2 (3.2L)
Connector 88: | Heated Seat - Left
Connector 89: | Heated Seat - Right
Connector 90: | Heated Seat Switch - Left
Connector 91: | Heated Seat Switch - Left
Connector 92: | Heated Seat Switch - Right
Connector 93: | Heated Seat Switch - Right
Connector 94: | High Pressure Pump (2.0L Diesel)
Connector 95: | Hill Descent Switch
Connector 96: | Hood Open Switch
Connector 97: | HVAC Control Module X1 (C68)
Connector 98: | I/P Compartment Lamp
Connector 99: | I/P Compartment Lamp Switch
Connector 100: | Ignition Coil Module (2.4L)
Connector 101: | Ignition Key Cylinder Lamp
Connector 102: | Ignition Switch
Connector 103: | Inclination Sensor
Connector 104: | Inflatable Restraint Retractor Pretensioner - Left Front (C105/Short Body)
Connector 105: | Inflatable Restraint Retractor Pretensioner - Right Front (C105/Short Body)
Connector 106: | Inflatable Restraint Roof Rail Module - Left
Connector 107: | Inflatable Restraint Roof Rail Module - Right
Connector 108: | Inflatable Restraint Side Impact Sensor - Left Front
Connector 109: | Inflatable Restraint Side Impact Sensor - Right Front
Connector 110: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 111: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 112: | Instrument Cluster
Connector 113: | Intake Air Temperature (IAT) Sensor (2.4L)
Connector 114: | Intrusion Sensor
Connector 115: | Knock Sensor (2.4L)
Connector 116: | License Lamp
Connector 117: | Liftgate Actuator
Connector 118: | Liftgate Ajar
Connector 119: | Liftgate Glass
Connector 120: | Liftgate Key Cylinder
Connector 121: | Manifold Absolute Pressure (MAP) Sensor (2.4L)
Connector 122: | Map Lamp
Connector 123: | Mass Air Flow (MAF) Sensor (2.0L Diesel)
Connector 124: | Mass Air Flow (MAF) Sensor (3.2L)
Connector 125: | Navigation Unit
Connector 126: | Object Detection Module
Connector 127: | Object Sensor - Left Rear Corner
Connector 128: | Object Sensor - Left Rear Middle
Connector 129: | Object Sensor - Right Rear Corner
Connector 130: | Object Sensor - Right Rear Middle
Connector 131: | Oil Level Sensor (2.4L)
Connector 132: | Oil Level Switch (2.0L Diesel)
Connector 133: | Oil Pressure Switch (2.0L Diesel)
Connector 134: | Oil Pressure Switch (2.4L)
Connector 135: | Outside Air Temperature/Air Quality Sensor
Connector 136: | Outside Air Temperature/Air Quality Sensor (C68)
Connector 137: | Outside Rearview Mirror (OSRVM) - Left (LHD)
Connector 138: | Outside Rearview Mirror (OSRVM) - Left (RHD)
Connector 139: | Outside Rearview Mirror (OSRVM) - Right (LHD)
Connector 140: | Outside Rearview Mirror (OSRVM) - Right (RHD)
Connector 141: | Outside Rearview Mirror (OSRVM) Switch
Connector 142: | Park Brake Switch
Connector 143: | Park/Turn Signal Lamp - Left
Connector 144: | Park/Turn Signal Lamp - Left (TR6)
Connector 145: | Park/Turn Signal Lamp - Right
Connector 146: | Park/Turn Signal Lamp - Right (TR6)
Connector 147: | Passenger Seatbelt Indicator
Connector 148: | Power Outlet - Cargo
Connector 149: | Power Outlet - Rear
Connector 150: | Power Seat Switch
Connector 151: | Power Seat Test Connector
Connector 152: | Power Sounder
Connector 153: | Power Steering Control Module
Connector 154: | Power Steering Magnetic Coil
Connector 155: | PRND Lamp
Connector 156: | PTC Heater (2.0L Diesel)
Connector 157: | Radio X1 (C100/Long Body)
Connector 158: | Radio X2 (C100/Long Body)
Connector 159: | Radio (C105/Short Body)
Connector 160: | Rain Sensor
Connector 161: | Rear Compartment Courtesy Lamp
Connector 162: | Rear Differential Clutch Control Module
Connector 163: | Rear Monitor
Connector 164: | Rear Window Wiper Module
Connector 165: | Rear Window Washer Fluid Pump
Connector 166: | Remote Control Door Lock Receiver
Connector 167: | Resistor
Connector 168: | Seatbelt Reminder Sensor
Connector 169: | Seatbelt Switch - Left
Connector 170: | Seatbelt Switch - Right
Connector 171: | Sensing and Diagnostic Module (SDM)
Connector 172: | Speaker - Left Front
Connector 173: | Speaker - Left Rear
Connector 174: | Speaker - Right Front
Connector 175: | Speaker - Right Front
Connector 176: | Speaker - Right Rear
Connector 177: | Steering Angle Sensor
Connector 178: | Stepwell Lamp - Left
Connector 179: | Stepwell Lamp - Right
Connector 180: | Stop Lamp Switch
Connector 181: | Subwoofer
Connector 182: | Sunroof Module
Connector 183: | Sunroof Switch
Connector 184: | Sunvisor Lamp - Left
Connector 185: | Sunvisor Lamp - Right
Connector 186: | Tail Lamp - Right
Connector 187: | Theft Deterrent Control Module
Connector 188: | Throttle Body (LD9)
Connector 189: | Throttle Body (LLW)
Connector 190: | Throttle Body (LU1)
Connector 191: | Traction Control Switch
Connector 192: | Trailer Relay Module (V92)
Connector 193: | Transmission Control Module (TCM) X1
Connector 194: | Transmission Control Module (TCM) X2
Connector 195: | Turn Signal/Multifunction Switch
Connector 196: | Turn Signal Repeater Lamp - Left
Connector 197: | Turn Signal Repeater Lamp - Right
Connector 198: | Tweeter - Left Front
Connector 199: | Tweeter - Left Rear
Connector 200: | Tweeter - Right Front
Connector 201: | Tweeter - Right Rear
Connector 202: | Water in Fuel Sensor (2.0L Diesel)
Connector 203: | Wheel Speed Sensor - Left Front
Connector 204: | Wheel Speed Sensor - Left Rear
Connector 205: | Wheel Speed Sensor - Right Front
Connector 206: | Wheel Speed Sensor - Right Rear
Connector 207: | Windshield Washer Fluid Level Switch
Connector 208: | Windshield Washer Fluid Pump
Connector 209: | Windshield Wiper Motor
Connector 210: | Windshield Wiper Switch
Connector 211: | XBCM X1
Connector 212: | XBCM X2
Connector 213: | Yaw Sensor

### A/C Compressor

#### Connector Part Information

- OEM: PED 12162017
- Service: N/A
- Description: 2-Way F 150 Sealed

#### A/C Compressor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 150 | Ground (LD9/LU1)
A | 0.35 BK | 250 | Ground (LLW)
B | 0.35 D-GN | 59 | A/C Compressor Clutch Supply Volt

### A/C Refrigerant Pressure Sensor 2.0L

#### Connector Part Information

- OEM: PKI 832316
- Service: N/A
- Description: 3-Way F 150.2 Sealed

#### A/C Refrigerant Pressure Sensor 2.0L

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 1274 | 5-Volt Reference (LD9)
1 | 0.35 GY | 2700 | 5-Volt Reference (LLW/LU1)
2 | 0.35 BK/WH | 2751 | Low Reference (LD9/LLW)
2 | 0.35 BN | 5514 | Low Reference (LU1)
3 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position Sensor

#### Connector Part Information

- OEM: PED 15326830
- Service: N/A
- Description: 6-Way F GT 150 Series Unsealed

#### Accelerator Pedal Position Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH/BK | 1164 | Accelerator Pedal Position Low Reference 1
B | 0.35 D-BU | 1161 | Accelerator Pedal Position Signal 1
C | 0.35 BN | 1271 | Accelerator Pedal Position Low Reference 1
D | 0.35 PU | 1272 | Accelerator Pedal Position 5-Volt Reference 2
E | 0.35 L-BU | 1162 | Accelerator Pedal Position Signal 2
F | 0.35 BN | 1274 | Accelerator Pedal Position Low Reference 2

### Alarm

#### Connector Part Information

- OEM: PED 15313469
- Service: N/A
- Description: 4-Way F Micro 064 Unsealed

#### Alarm

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | -- | Low Reference
2 | 0.35 YE | -- | Signal
3 | -- | -- | Not Used
4 | 0.35 D-BU | -- | 12-Volt Reference

### Ambient Light Sensor (w/C60)

#### Connector Part Information

- OEM: PED 12059249
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Unsealed (NA)

#### Ambient Light Sensor (w/C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 278 | Ambient Light Sensor Signal
B | 0.35 WH/BK | 351 | Signal Ground

### Ambient Light/Sunload Sensor (with C68)

#### Connector Part Information

- OEM: PED 12064760
- Service: N/A
- Description: 4-Way F Metri-Pack Unsealed

#### Ambient Light/Sunload Sensor (with C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU/BK | 590 | Solar Sensor Driver Signal
B | 0.35 WH | 278 | Ambient Light Sensor Signal
C | 0.35 L-BU | 590 | Solar Sensor Driver Signal
D | 0.35 BK/WH | 351 | Ground

### Audio Amplifier

#### Connector Part Information

- OEM: TYCO 368544-1
- Service: N/A
- Description: 18-Way F MS-AL Unsealed

#### Audio Amplifier

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 550 | Ground
2 | 0.35 RD/BK | 2540 | Battery Positive Voltage
3 | 0.35 YE | 116 | Left Rear Speaker Signal (-)
4 | 0.35 BN | 119 | Left Rear Speaker (+)
5 | 0.35 D-GN | 117 | Right Front Speaker Signal (-)
6 | 0.35 L-GN | 200 | Right Front Speaker (+)
7 | -- | -- | Not Used
8 | 0.35 YE | 1860 | Front Center Speaker (+)
9 | 0.35 BK | 550 | Ground
10 | 0.35 RD/WH | 2540 | Battery Positive Voltage
11 | -- | -- | Not Used
12 | 0.35 L-BU | 115 | Right Rear Speaker Signal (-)
13 | 0.35 D-BU | 46 | Right Rear Speaker (+)
14 | 0.35 GY | 118 | Left Front Speaker Signal (-) 1
15 | 0.35 BN | 24 | Left Front Speaker (+) 1
16-17 | -- | -- | Not Used
18 | 0.35 L-BU | 1960 | Front Center Speaker (-)

### Backup Lamp Switch

#### Connector Part Information

- OEM: PED 15419715
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Backup Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-BU | 38 | Backup Lamp Relay Control
A | 0.35 D-BU | 6316 | Reverse Gear SW Signal
B | 0.35 BK | 250 | Ground

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: JST HITPB-25-D-K
- Service: N/A
- Description: 25-Way F 064+280 (BK)

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1240 | Battery Positive Voltage
2 | 0.35 RD/WH | 1440 | Battery Positive Voltage
3 | 0.35 RD/WH | 1540 | Battery Positive Voltage
4 | 0.35 RD/WH | 1340 | Battery Positive Voltage
5 | 0.35 D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Volt
6 | -- | -- | Not Used
7 | 0.35 YE | 196 | Wiper Motor Park Switch Signal
8-10 | -- | -- | Not Used
11 | 0.35 D-GN/WH | 1317 | Fog Lamp Relay Control
12 | 0.35 OG | 5186 | Left Trailer Turn Signal Lamp
13 | 0.35 YE | 5187 | Right Trailer Turn Signal Lamp
14 | 0.35 L-GN | 482 | Rain Sensor Signal
15 | 0.35 OG | 2268 | Windshield Washer Relay Control
16 | 0.35 BN/WH | 1969 | HDLP High Beam Relay Control
17 | -- | -- | Not Used
18 | 0.35 BN | 481 | Rain Sensor Signal
19 | 0.35 D-BU | 5985 | Accessory Wakeup Serial Data
20 | 0.35 YE | 1977 | Rear Fog Lamp Relay Control
21 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
22 | 0.35 L-BU | 1344 | Liftgate Release Relay Control
23 | -- | -- | Not Used
24 | 0.35 WH | 2282 | Headlamp Washer Relay Control
25 | 0.35 WH | 1080 | Park Brake Relay Supply Voltage

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: JST HITPB-25-E-N
- Service: N/A
- Description: 25-Way F 064+280 (BN)

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
2 | 0.35 D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
3 | -- | -- | Not Used
4 | 0.35 L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
5 | -- | -- | Not Used
6 | 0.35 BN | 683 | Rear Defog Indicator Supply Voltage
7-10 | -- | -- | Not Used
11 | 0.35 BN | 755 | RAP Relay Coil Control
12 | -- | -- | Not Used
13 | 0.35 L-GN | 5486 | Run Relay Coil Control
14 | 0.35 BN | 4 | Accessory Voltage
15 | 0.35 PU | 5531 | Hood Closed Switch Signal
16 | 0.35 L-BU | 1134 | Park Brake Switch Signal
17 | -- | -- | Not Used
18 | 0.35 BN | 288 | Horn Relay Control
19 | 0.35 WH | 193 | Rear Defog Relay Control
20 | 0.35 GY | 91 | Wiper Motor Relay Coil Supply Voltage
21 | 0.35 BN | 860 | F/Windshield Wiper Switch High Signal
22 | -- | -- | Not Used
23 | 0.35 PK/WH | 1970 | HDLP Low Beam Relay Control
24 | 0.35 D-BU | 45 | Park Lamp Relay Control
25 | -- | -- | Not Used

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: JST HITPB-25-F-PK
- Service: N/A
- Description: 25-Way F 064+280 (PK)

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY/BK | 690 | Courtesy Lamp Relay Control
2 | 0.35 L-GN | 24 | Backup Lamp Supply Voltage
3-7 | -- | -- | Not Used
8 | 0.35 BN/WH | 746 | Right Front Door Ajar Switch Signal
9 | -- | -- | Not Used
10 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
11 | 0.35 GY | 6137 | EVAP Core Temp Sensor Signal
12 | 0.35 PK/BK | 1303 | Lift Gate Ajar Switch Signal 1
13-14 | -- | -- | Not Used
15 | 0.35 GY | 6127 | Liftgate Unlatch Switch Signal
16 | 0.35 PU | 5059 | Intrusion Arm On Signal
17-19 | -- | -- | Not Used
20 | 0.35 PU | 1124 | Door Lock Key Switch Unlock Signal
21 | 0.35 YE | 1491 | Backuplight Lamp Control
22 | 0.35 L-GN | 1123 | Door Lock Key Switch Lock Signal
23 | 0.35 BN | 305 | Trunk Key Switch Signal
24-25 | -- | -- | Not Used

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: JST HITPB-28-G-H
- Service: N/A
- Description: 28-Way F 064+280 (GY)

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 PK | 6190 | Liftgate Glass/Trunk Exterior Release Control
3-5 | -- | -- | Not Used
6 | 0.35 L-BU | 5921 | Fuel Door Lock Relay Control
7 | 0.35 L-GN | 1391 | Left Front Door Lock Relay Control
8 | 0.35 OG | 9000 | Rear Wiper Auto On Signal
9 | 0.35 PK/BK | 5291 | Driver Door Unlock Relay
10 | 0.35 BN/WH | 6724 | Head Lamp Washer Pump Switch Signal
11 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal
12 | 0.35 OG/BK | 782 | Driver Door Lock Switch Lock Signal
13-14 | -- | -- | Not Used
15 | 0.35 D-GN | 1376 | Alarm Armed Signal
16 | 0.35 L-BU | 187 | Rear Fog Lamp Switch Signal
17-21 | -- | -- | Not Used
22 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
23 | 0.35 BN | 126 | Left Front Door Open Switch Signal
24 | 0.35 D-GN/WH | 762 | A/C Request Signal
25 | 0.35 PU/WH | 1382 | LED Dimming Signal
26-28 | -- | -- | Not Used

### Body Control Module (BCM) X5

#### Connector Part Information

- OEM: HITPB-27-A-LM
- Service: N/A
- Description: 27-Way F HIT Series (L-GN)

#### Body Control Module (BCM) X5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 WH/BK | 1073 | Ignition Key Resister Signal
3 | 0.35 GY | 1884 | Cruise Control Switch Signal
4 | 0.35 WH | 530 | Off/Run/Crank Voltage
5 | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
6-7 | -- | -- | Not Used
8 | 0.35 BN/BK | 6009 | Windshield Wiper Switch Low Reference
9 | 0.35 L-BU | 1714 | Windshield Wiper Switch Low Signal
10-13 | -- | -- | Not Used
14 | 0.35 PK | 39 | Run/Crank Ignition 1 Voltage
15 | 0.35 L-BU/WH | 1414 | Left Front Turn Switch Signal
16 | 0.35 D-BU/WH | 1415 | Right Front Turn Switch Signal
17 | 0.35 PK | 1444 | 12-Volt Reference
18 | 0.35 PU | 524 | HDLP Dimmer Switch High Beam
19 | 0.35 BN | 2144 | Hazard Switch Signal
20 | 0.35 D-GN | 5525 | Tap Up/Down Enable Signal
21 | 0.35 YE | 43 | Accessory Voltage
22 | -- | -- | Not Used
23 | 0.35 L-BU | 553 | Shift Select Switch Perform Signal
24 | 0.35 PK | 94 | Windshield Washer Switch Signal
25 | 0.35 YE | 307 | HDLP Switch Flash To Pass Signal
26 | 0.35 BN/WH | 816 | BTSI Solenoid Control (M98)
27 | -- | -- | Not Used

### Body Control Module (BCM) X6

#### Connector Part Information

- OEM: JST HITPB-25-B-5
- Service: N/A
- Description: 25-Way F (WH)

#### Body Control Module (BCM) X6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 1732 | Electronic Control Unit 12-Volt Reference 3
2 | 0.35 RD/WH | 1640 | Battery Positive Voltage
3 | 0.35 BN/WH | 230 | I/P Lamp Dimming Control
4-7 | -- | -- | Not Used
8 | 0.35 L-BU | 13 | HDLP Switch Park Lamp Signal
9 | -- | -- | Not Used
10 | 0.35 D-BU | 6189 | Lift Glass/Trunk Release Signal
11 | 0.35 WH | 278 | Ambient Light Sensor Signal
12 | 0.35 WH | 103 | Headlamp Switch On Signal
13-16 | -- | -- | Not Used
17 | 0.35 D-GN | 306 | HDLP Switch Off Signal Control
18 | 0.35 PK | 5068 | Intrusion Sensor Switch Disable
19 | -- | -- | Not Used
20 | 0.35 L-BU | 292 | Rear Defog Switch Signal
21 | 0.35 L-BU | 1788 | Traction Control Switch Signal (1)
22-24 | -- | -- | Not Used
25 | 0.35 PU | 328 | Interior Lamp Defeat Switch Signal

### Body Control Module (BCM) X7

#### Connector Part Information

- OEM: JST HITPB-25-C-LE
- Service: N/A
- Description: 25-Way F 064+280 (L-BU)

#### Body Control Module (BCM) X7

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 350 | Ground
2 | 0.35 RD/WH | 1140 | Battery Positive Voltage
3 | 0.35 RD/WH | 1040 | Battery Positive Voltage
4 | -- | -- | Not Used
5 | 0.35 BK | 350 | Ground
6 | -- | -- | Not Used
7 | 0.35 YE | 749 | Security Indicator Control
8 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
9 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-)
10 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
11 | 0.35 D-GN | 44 | I/P Lamp Dimmer Switch Signal
12 | 0.35 OG/WH | 812 | 12-Volt Reference
13 | 0.35 PU | 7062 | Brake Pedal Switch Normally Closed Contact Signal
14 | 0.35 BN | 6138 | EVAP Core Temp Sensor Low Reference
15 | -- | -- | Not Used
16 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
17 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-)
18 | 0.35 YE | 1491 | Backlight Lamp Control
19 | 0.35 L-BU | 5986 | Serial Data Communication Enable
20 | -- | -- | Not Used
21 | 0.35 OG | 192 | Front Fog Lamp Switch Signal
22-24 | -- | -- | Not Used
25 | 0.35 PU/WH | 1382 | LED Dimming Signal

### Boost Pressure Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: TYCO 368162-1
- Service: N/A
- Description: 4-Way F JPT Sealed

#### Boost Pressure Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN/WH | 3123 | Boost Pressure Sensor Low Reference
2 | 0.35 YE | 3135 | Boost Pressure Temperature Signal
3 | 0.35 GN/WH | 3113 | 5 Volt Reference
4 | 0.35 WH | 3140 | Boost Pressure Sensor Signal

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: PED 12162193
- Service: N/A
- Description: 2-Way F 150.2 Sealed

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BN | 333 | Brake Fluid Sensor Signal
B | 0.35 BK | 650 | Ground

### Camshaft Position (CMP) Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Camshaft Position (CMP) Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BN | -- | Signal
2 | RD | -- | Heated O2 Sensor High Signal
3 | PK/BK | -- | Engine Main Relay Fused Control (3)

### Camshaft Position (CMP) Sensor (2.4L)

#### Connector Part Information

- OEM: KET MG640541-5
- Service: N/A
- Description: 3-Way F ITC Sealed

#### Camshaft Position (CMP) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (3)
2 | BK/WH | -- | Camshaft Position Sensor Low Reference
3 | BN/WH | -- | Camshaft Position Sensor Signal

### Camshaft Position (CMP) Sensor (2.4L)

#### Connector Part Information

- OEM: KET MG640541-5
- Service: N/A
- Description: 3-Way F ITC Sealed

#### Camshaft Position (CMP) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (3)
2 | BK/WH | -- | Camshaft Position Sensor Low Reference
3 | BN/WH | -- | Camshaft Position Sensor Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: MG 630679
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Stop Lamp Supply Voltage
2 | BK | -- | Ground

### Cigar Lighter

#### Connector Part Information

- OEM: MG 630685-5
- Service: N/A
- Description: 2-Way F 205+250 Type Unsealed

#### Cigar Lighter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Ignition Voltage
2 | BK | -- | Ground

### Clock

#### Connector Part Information

- OEM: PED 15499930
- Service: N/A
- Description: 6-Way F Mirco 064 Unsealed

#### Clock

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RD/WH | -- | Battery Positive Voltage
3 | YE | -- | Accessory Voltage
4 | YE | -- | Backlight Lamp Control
5 | BN/WH | -- | Signal Ground
6 | -- | -- | Not Used

### Clutch Start Switch

#### Connector Part Information

- OEM: PED 15313469
- Service: N/A
- Description: 4-Way F 064 Micro Unsealed

#### Clutch Start Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Ignition 1 Voltage
2 | GY | -- | Clutch Pedal Position Signal
3-4 | -- | -- | Not Used

### Contact Coil

#### Connector Part Information

- OEM: PED 15393433
- Service: N/A
- Description: 10-Way F 064 Unsealed

#### Contact Coil

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN | -- | Remote Compact Disc/Cassette Player Supply Voltage
3 | GY | -- | Cruise Control Set/Coast/Resume/Accelerate Switch Signal
4 | L-GN | -- | Handset Volume Control Ground
5 | L-GN | -- | Remote Radio Control Signal
6 | PK | -- | 12-Volt Reference
7 | D-BU/WH | -- | Handset Volume Control Supply
8 | -- | -- | Not Used
9 | BK | -- | Ground
10 | BN | -- | Horn Relay Control

### Contact Coil

#### Connector Part Information

- OEM: PED 15393433
- Service: N/A
- Description: 10-Way F 064 Unsealed

#### Contact Coil

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN | -- | Remote Compact Disc/Cassette Player Supply Voltage
3 | GY | -- | Cruise Control Set/Coast/Resume/Accelerate Switch Signal
4 | L-GN | -- | Handset Volume Control Ground
5 | L-GN | -- | Remote Radio Control Signal
6 | PK | -- | 12-Volt Reference
7 | D-BU/WH | -- | Handset Volume Control Supply
8 | -- | -- | Not Used
9 | BK | -- | Ground
10 | BN | -- | Horn Relay Control

### Cooling Fan - Auxiliary

#### Connector Part Information

- OEM: TYCO 6-176146-6
- Service: N/A
- Description: 2-Way F Sealed (GY)

#### Cooling Fan - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Cooling Fan Motor Low
2 | GY | -- | Cooling Fan Motor Supply Voltage

### Cooling Fan - Main

#### Connector Part Information

- OEM: TYCO 176146-2
- Service: N/A
- Description: 2-Way F Sealed (BK)

#### Cooling Fan - Main

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU | -- | Cooling Fan Motor Supply Voltage

### Crankshaft Position (CKP) Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Crankshaft Position (CKP) Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Input
2 | GY | -- | Heated O2 Sensor Heater Low Control Bank 1 Sensor 1
3 | BK/WH | -- | Input

### Crankshaft Position (CKP) Sensor (2.4L)

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Crankshaft Position (CKP) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Crankshaft POS Sensor Signal (3)
2 | YE/BK | -- | Crankshaft POS Sensor Low Reference (3)
3 | BK/WH | -- | Signal Ground

### Data Link Connector

#### Connector Part Information

- OEM: MOLEX 51115-1611
- Service: N/A
- Description: 16-Way F OBD II Unsealed

#### Data Link Connector

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | BK | -- | Ground
5 | BK/WH | -- | Signal Ground
6 | BN/BK | -- | High Speed GMLAN Serial Data (+)
7 | PU | -- | Engine/Radio Serial Data K Line
8 | WH | -- | Central Control Module Diagnosis Enable
9-13 | -- | -- | Not Used
14 | BN | -- | High Speed GMLAN Serial Data (-)
15 | -- | -- | Not Used
16 | RD/WH | -- | Battery Positive Voltage

### Diesel Particulate Filter Pressure Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: FEP 1J0973703
- Service: N/A
- Description: 3-Way F Sealed

#### Diesel Particulate Filter Pressure Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | 5-Volt Reference (LHD)
D-GN | -- | 5-Volt Reference (RHD)
2 | BN/WH | -- | Low Reference
3 | D-GN | -- | Signal

### Dome Lamp

#### Connector Part Information

- OEM: TYCO 936227-1
- Service: N/A
- Description: 4-Way F Unsealed

#### Dome Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | OG | -- | BCM 12-Volt Reference
3 | BK | -- | Ground
4 | -- | -- | Not Used

### Door Latch - Driver

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Driver Door Ajar Switch Signal
2 | BN | -- | Driver Door Open Switch Signal
3 | BK | -- | Ground
4 | PU | -- | Door Lock Key Switch Unlock Signal
5 | -- | -- | Not Used
6 | BN | -- | Driver Door Double Lock Actuator Lock Control
7 | BN | -- | Door Lock Actuator Unlock Control
8 | GY | -- | Door Lock Actuator Lock Control
9 | L-GN | -- | Door Lock Key Switch Lock Signal
10 | -- | -- | Not Used

### Door Latch - Driver (w/Dead Locking)

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Driver (w/Dead Locking)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Driver Door Double Lock Actuator Lock Signal
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | L-GN | -- | Door Lock Key Switch Signal
5 | -- | -- | Not Used
6 | BN/WH | -- | Driver Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | BK | -- | Ground
9 | PU | -- | Door Lock Key Switch Unlock Signal
10 | -- | -- | Not Used

### Door Latch - Left Rear

#### Connector Part Information

- OEM: TYCO 6-1355683-1
- Service: N/A
- Description: 6-Way F M/T Sealed

#### Door Latch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Door Double Lock Actuator Lock
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | BN/WH | -- | Left Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | BK | -- | Ground

### Door Latch - Passenger

#### Connector Part Information

- OEM: TYCO 6-1355688-1
- Service: N/A
- Description: 10-Way F M/T Sealed

#### Door Latch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Passenger Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | BK | -- | Ground
4 | PU | -- | Door Lock Key Switch Unlock Signal
5 | -- | -- | Not Used
6 | BN | -- | Passenger Door Double Lock Actuator Lock Control
7 | BN | -- | Door Lock Actuator Unlock Control
8 | GY | -- | Door Lock Actuator Lock Control
9 | L-GN | -- | Door Lock Key Switch Lock Signal
10 | -- | -- | Not Used

### Door Latch - Right Rear

#### Connector Part Information

- OEM: TYCO 6-1355683-1
- Service: N/A
- Description: 6-Way F M/T Sealed

#### Door Latch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Door Double Lock Actuator Lock
2 | BN | -- | Door Lock Actuator Unlock Control
3 | GY | -- | Door Lock Actuator Lock Control
4 | BN/WH | -- | Right Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | BK | -- | Ground

### Door Lock Switch - Driver

#### Connector Part Information

- OEM: PED 13513469
- Service: N/A
- Description: 4-Way F 064 Unsealed

#### Door Lock Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Lock Signal
2 | BK | -- | Ground
3 | OG/BK | -- | Unlock Signal
4 | -- | -- | Not Used

### Driver Information Center (C100/Long Body)

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F Mirco 064 Unsealed

#### Driver Information Center (C100/Long Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | YE | -- | Backlight Lamp Control
5 | BN/WH | -- | Signal Ground
6 | PK | -- | Run/Crank Ignition 1 Voltage
7 | D-GN | -- | Low Speed GMLAN Serial Data
8-14 | -- | -- | Not Used
15 | BN/WH | -- | CAN Bus High Serial Data
16 | -- | -- | Not Used

### Driver Information Center (C105/Short Body)

#### Connector Part Information

- OEM: TYCO 968265-1
- Service: N/A
- Description: 32-Way F 064 Quadlock (BK)

#### Driver Information Center (C105/Short Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BK/WH | -- | Ground
3 | RD/WH | -- | Battery Positive Voltage
4 | -- | -- | Not Used
5 | RD/WH | -- | Battery Positive Voltage
6-16 | -- | -- | Not Used
17 | BN/WH | -- | MID Speed CAN High
18 | BN | -- | MID Speed CAN Low
19 | BN | -- | MID Speed CAN Low
20 | BN/WH | -- | MID Speed CAN High
21 | -- | -- | Not Used
22 | BN/WH | -- | MID Speed CAN High
23 | BN | -- | MID Speed CAN Low
24 | -- | -- | Not Used
25 | GN | -- | Low Speed GMLAN Serial Data
26-32 | -- | -- | Not Used

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: TYCO 1355628-2
- Service: N/A
- Description: 47-Way F

#### Electronic Brake Control Module (EBCM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | -- | -- | Not Used
3 | D-GN/WH | -- | Vehicle Speed Signal
4-7 | -- | -- | Not Used
8 | L-BU | -- | Serial Data
9-10 | -- | -- | Not Used
11 | BN/BK | -- | High Speed GMLAN (+)
12 | BN/BK | -- | High Speed GMLAN (+)
13 | BN | -- | High Speed GMLAN (-)
14 | BN | -- | High Speed GMLAN (-)
15 | -- | -- | Not Used
16 | BK/WH | -- | Ground
17 | -- | -- | Not Used
18 | BN/WH | -- | CAN (+)
19 | OG/BK | -- | CAN (-)
20-21 | -- | -- | Not Used
22 | D-GN | -- | 12-Volt Reference
23-28 | -- | -- | Not Used
29 | L-BU | -- | Low Reference
30-31 | -- | -- | Not Used
32 | RD/WH | -- | Battery Positive Voltage
33 | BN | -- | Right Front Wheel Speed Sensor Low Reference
34 | D-GN | -- | Right Front Wheel Speed Sensor Signal
35 | -- | -- | Not Used
36 | BN | -- | Left Rear Wheel Speed Sensor Signal
37 | OG | -- | Left Rear Wheel Speed Sensor Low Reference
38 | L-BU | -- | Hill Descent Switch Signal
39-41 | -- | -- | Not Used
42 | WH | -- | Right Rear Wheel Speed Sensor Low Reference
43 | BN | -- | Right Rear Wheel Speed Sensor Signal
44 | -- | -- | Not Used
45 | L-BU | -- | Left Front Wheel Speed Sensor Signal
46 | YE | -- | Left Front Wheel Speed Sensor Low Reference
47 | -- | -- | Not Used

### Engine Control Module (ECM) X1 (LD9)

#### Connector Part Information

- OEM: BOSCH 1928403454
- Service: N/A
- Description: 81-Way F ECU 81P Assembly Seal

#### Engine Control Module (ECM) X1 (LD9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | PK/BK | -- | Engine Main Relay Fused Control (1)
5-12 | -- | -- | Not Used
13 | OG/BK | -- | Trans Park/Neutral Signal (1)
14-15 | -- | -- | Not Used
16 | D-BL | -- | APM Signal (1)
17 | -- | -- | Stop Lamp Supply Voltage
18 | RD/WH | -- | Battery Positive Voltage
19 | BN | -- | APM 5-Volt Reference (2)
20 | GY | -- | F/Pump Pressure Sensor 5-Volt Reference
21 | WH/BK | -- | APM 5-Volt Reference (1)
22 | -- | -- | Not Used
23 | D-GN/WH | -- | A/C Comp Clutch Supply Voltage
24 | D-BU | -- | High Speed Cooling Fan Relay Control
25-29 | -- | -- | Not Used
30 | BN/BK | -- | High Speed GMLAN Serial Data (+) 1
31 | -- | -- | Not Used
32 | BN | -- | Charge Indicator Control
33 | D-BU | -- | Backup Lamp Relay Control
34 | -- | -- | Not Used
35 | L-BU | -- | Secondary Fuel Level Sensor Signal
36 | D-BU | -- | Primary Fuel Level Sensor Signal
37 | -- | -- | Not Used
38 | PU | -- | Engine/Radio Serial Data K-Line
39 | PK | -- | Run/Crank Ignition 1 Voltage
40 | BN | -- | Engine Main Relay Coil Control
41-42 | -- | -- | Not Used
43 | D-GN | -- | Low Speed Cooling Fan Relay Control
44-48 | -- | -- | Not Used
49 | BN | -- | High Speed GMLAN Serial Data (1) 1
50 | -- | -- | Not Used
51 | D-GN/WH | -- | Fuel Pump Primary Relay Control
52-53 | -- | -- | Not Used
54 | L-BU | -- | APM Signal (2)
55 | OG/BK | -- | A/C Refrigerant Press Sensor Signal
56-62 | -- | -- | Not Used
63 | WH | -- | EVAP Canister Vent Solenoid Control
64-66 | -- | -- | Not Used
67 | BK | -- | Ground
68 | BK | -- | Ground
69 | -- | -- | Not Used
70 | GY | -- | Generator Field Duty Cylinder Signal
71 | -- | -- | Not Used
72 | BN/WH | -- | Cruise Control Clutch Pedal Pstn S/W Signal
73 | D-BU | -- | Accessory Wakeup Serial Data
74 | D-GN | -- | F/Pump Pressure Sensor Signal
75 | -- | -- | Not Used
76 | BN/WH | -- | Fuel Level Sensor Low Reference
77 | BK/WH | -- | Signal Ground
78 | PU | -- | APM Low Reference (2)
79 | BN | -- | APM Low Reference (1)
80 | -- | -- | Not Used
81 | YE | -- | Starter Relay Coil Control

### Engine Control Module (ECM) X1 (LLW)

#### Connector Part Information

- OEM: TYCO 284743-1
- Service: N/A
- Description: 94-Way F FIAT Housing Assembly Sealed

#### Engine Control Module (ECM) X1 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PK/BK | 5291 | Main Relay Fused Coil Control (2)
2 | 0.35 BK | 250 | Ground
3 | 0.35 PK/BK | 5290 | Main Relay Fused Coil Control (1)
4 | 0.35 BK | 250 | Ground
5 | 0.35 PK/BK | 5290 | Main Relay Fused Coil Control (1)
6 | 0.35 BK | 250 | Ground
7 | -- | -- | Not Used
8 | 0.35 PU | 1272 | APM Low Reference (2)
9 | 0.35 D-BU | 1161 | APM Signal (1)
10 | 0.35 BK/WH | 3210 | Heated O2 Sensor High Signal Bank 1 Sensor (2)
11 | 0.35 D-GN | 3211 | Heated O2 Sensor Low Signal Bank 1 Sensor (2)
12 | 0.35 BK/WH | 275 | Signal Ground
13 | 0.35 OG/BK | 380 | TCC On/Off Solenoid A Contact
14 | 0.35 BN/WH | 6281 | Fuel Level Sensor Low Reference
15 | 0.35 D-BU | 1936 | Primary Fuel Level Sensor
16 | -- | -- | Not Used
17 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
18 | 0.35 GY | 3141 | CTS Ground
19 | 0.35 BN | 25 | Change Indicator Control
20 | 0.35 D-GN/WH | 465 | Fuel Pump Primary Relay Control
21 | -- | -- | Not Used
22 | 0.35 GY | 2700 | ACP 5-Volt Reference
23-24 | -- | -- | Not Used
25 | 0.35 PU | 1319 | Engine/Radio Serial Data K-Line
26-27 | -- | -- | Not Used
28 | 0.35 PK | 539 | Run/Crank Ignition 1 Voltage
29 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control
30 | 0.35 BN | 1271 | APM Low Reference (1)
31 | 0.35 L-BU | 1162 | APM Signal (2)
32 | 0.35 D-GN/BK | 3032 | Temperature Sensor 2
33 | 0.35 BK | 3033 | Temperature Sensor 2
34 | 0.35 D-GN | 3034 | Temperature Sensor 1
35 | 0.35 BK/WH | 3035 | Temperature Sensor 1
36 | -- | -- | Not Used
37 | 0.35 BK/WH | 3037 | CTS Signal
38-39 | -- | -- | Not Used
40 | 0.35 D-BU | 38 | Backup Lamp Relay Control
41-42 | -- | -- | Not Used
43 | 0.35 D-BU | 5985 | ACC Wakeup Serial Data
44 | 0.35 PU | 3044 | CTS Signal
45 | 0.35 WH/BK | 1164 | APM 5-Volt Reference (1)
46 | 0.35 BN | 1274 | APN 5-Volt Reference (2)
47-51 | -- | -- | Not Used
52 | 0.35 WH | 3052 | GPCU 01
53-54 | -- | -- | Not Used
55 | 0.35 YE | 447 | Starter Relay Coil Control
56 | -- | -- | Not Used
57 | 0.35 WH/BK | 910 | PTC Request Signal
58 | 0.35 WH | 3058 | WIT Sensor
59-63 | -- | -- | Not Used
64 | 0.35 D-GN | 3064 | CTS Signal
65 | -- | -- | Not Used
66 | 0.35 YE | 3158 | CTS Signal
67 | -- | -- | Not Used
68 | 0.35 D-GN | 1488 | Noise Reduction Microphone (+)
69 | 0.345 D-GN | 335 | Low Speed Cool Fan Relay Control
70-71 | -- | -- | Not Used
72 | 0.35 BN | 5069 | Engine Main Relay Coil Control
73-74 | -- | -- | Not Used
75 | 0.35 GY | 23 | Generator Field Duty Cycle Signal
76-79 | -- | -- | Not Used
80 | 0.35 BN/WH | 379 | Cruise Control Clutch Switch Signal
81 | 0.35 OG/BK | 1786 | Trans P/N Signal (1)
82 | -- | -- | Not Used
83 | 0.35 TN | 2501 | Low Speed GMLAN Serial Data (-)
84 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
85-89 | -- | -- | Not Used
90 | 0.35 D-BU | 473 | High Speed Cool Fan Relay Control
91 | 0.35 L-GN/WH | 6549 | Auxiliary GAS/PTC Relay Coil Control
92 | -- | -- | Not Used
93 | 0.35 WH/RD | 3093 | GPCU ST
94 | 0.35 YE | 2197 | PTC Heater Relay Coil Supply Volt

### Engine Control Module (ECM) X1 (LU1)

#### Connector Part Information

- OEM: 1928404927
- Service: See Catalog
- Description: 96-Way F 120 Series, Sealed (BK)

#### Terminal Part Information

- Pins: 7, 9, 12-13, 18-20, 26, 31-37, 40, 44, 46-49, 53-96
- Terminal/Tray: 33467-0003/23
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X1 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid (1)
2 | 0.8 PU | 5284 | Camshaft Phaser Intake Solenoid (1)
3 | -- | -- | Not Used
4 | 0.5 YE/BK | 846 | Fuel Injector 6 Control
5 | 0.5 GN/WH | 428 | EVAP Canister Purge Solenoid Control
6 | -- | -- | Not Used
7 | 0.5 OG | 5275 | Camshaft Position Intake Sensor (1)
8 | -- | -- | Not Used
9 | 0.5 PU | 5274 | Camshaft Position Exhaust Sensor (2)
10 | 0.5 OG | 225 | Generator Turn On Signal
11 | 0.35 BN | 1174 | Oil Level Switch Signal
12 | 0.35 BN/GN | 6392 | IMT Valve Control
13 | 0.35 PK | 6414 | Ignition Coil 2, 4, 6 Low Reference
14 | -- | -- | Not Used
15 | 0.5 GY | 705 | 5-Volt Reference
16-23 | -- | -- | Not Used
24 | 0.5 YE | 582 | TAC Motor Control - 2
25 | 0.8 WH | 5283 | Camshaft Phaser Exhaust Solenoid (2)
26 | 0.35 D-GN | 1746 | Fuel Injector 3 Control
27 | -- | -- | Not Used
28 | 1 BN/WH | 845 | Fuel Injector 5 Control
29 | -- | -- | Not Used
30 | 0.5 GY | 23 | Generator Field Duty Cycle Signal
31-32 | -- | -- | Not Used
33 | 0.5 YE | 5276 | Camshaft Position (CMP) Sensor Signal - Bank 2 Intake
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor (1)
35 | 0.5 WH | 5039 | CKP Sensor High
36-38 | -- | -- | Not Used
39 | 0.5 GY | 2701 | 5 Volt Reference
40 | 0.5 GY | 605 | 5 Volt Reference
41 | 0.5 BN/RD | 470 | Low Reference
42 | -- | -- | Not Used
43 | 0.5 BN/RD | 470 | Low Reference
44 | 0.5 BN/RD | 470 | Low Reference
45 | 0.5 BN | 5024 | CKP Sensor Low
46 | 0.5 GY/BK | 798 | Crank Shaft Position Sensor
47 | -- | -- | Not Used
48 | 0.5 BN | 581 | TAC Motor Control - 1
49 | 0.8 OG | 5272 | Camshaft Position (CMP) Actuator Solenoid Control - Bank 2 Intake
50 | 1 L-BU | 844 | Fuel Injector 4 Control
51 | 1 BN/D-BU | 1744 | Fuel Injector 1 Control
52 | 1 L-GN/BU | 1745 | Fuel Injector 2 Control
53-54 | -- | -- | Not Used
55 | 0.5PU | 2121 | Ignition Control (1)
56 | 0.5 L-BU | 2123 | Ignition Control (3)
57 | 0.5 D-GN | 2125 | Ignition Control (5)
58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | Knock Sensor Signal (1)
60 | 0.5 BN | 407 | Low Reference
61 | 0.5 BN/BK | 231 | Oil Pressure Switch Signal
62-64 | -- | -- | Not Used
65 | 0.5 D-BU/WH | 5041 | Intake Manifold - Signal - 1
66 | -- | -- | Not Used
67 | 0.5 BU/WH | 1667 | Heated Oxygen Sensor Low Reference - Bank 1 Sensor (1)
68 | 0.5 OG | 5280 | Heated Oxygen Sensor Pump Current Bank 2 Sensor (2)
69 | 0.5 WH | 5279 | Heated Oxygen Sensor Input Pump Current Bank 1 Sensor (1)
70 | 0.5 PU/WH | 1665 | Heated Oxygen Sensor High Signal - Bank 2 Sensor (1)
71 | -- | -- | Not Used
72 | 0.8 D-BU | 5038 | Heated Oxygen Sensor Heater Low Control Bank 2 Sensor (1)
73-77 | -- | -- | Not Used
78 | 0.5 PU | 6413 | Ignition Coil 1, 3, 5 Low Reference
79 | 0.5 OG/WH | 2122 | Ignition Coil 2 Control
80 | 0.5 D-GN/WH | 2124 | Ignition Coil 4 Control
81 | 0.5 L-BU/WH | 2126 | Ignition Coil 6 Control
82 | 0.5 YE | 410 | Engine Coolant Temperature Sensor Signal
83 | 0.5 GY | 1716 | Knock Sensor Low Reference (1)
84 | 0.5 L-BU | 1876 | Knock Sensor Signal (2)
85 | 0.5 Gn/WH | 357 | Oil Temperature Sensor Signal
86-87 | -- | -- | Not Used
88 | 0.5 BN/YE | 2752 | Low Reference
89 | 0.5 PU | 486 | Throttle Position Sensor Signal (2)
90 | 0.5 D-GN | 485 | Throttle Position Sensor Signal (1)
91 | 0.5PU/WH | 5281 | Heated Oxygen Sensor Pump Current Bank 2 Sensor (1)
92 | 0.5 PU | 1666 | Heated Oxygen Sensor High Signal Bank 1 Sensor (1)
93 | 0.5 BN/WH | 1653 | Heated Oxygen Sensor Low Signal Bank 2 Sensor (1)
94 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Bank 1 Sensor (1)
95 | -- | -- | Not Used
96 | 0.8 PU/WH | 5037 | Heated Oxygen Sensor Heater Low Control Bank 1 Sensor (1)

### Engine Control Module (ECM) X2 (LD9)

#### Connector Part Information

- OEM: BOSCH 1928403462
- Service: N/A
- Description: 40-Way F ECU 40P Assembly Seal

#### Engine Control Module (ECM) X2 (LD9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
82 | -- | -- | Not Used
83 | L-GN/BK | -- | Fuel Injector Control (2)
84 | BN/WH | -- | Heated O2 Sensor Low Signal Bank 1 Sensor (1)
85 | BK | -- | Ground
86 | OG/BK | -- | Intake Air Temperature Sensor Low Reference
87 | BN | -- | Sensor Low Reference
88 | BK/WH | -- | Camshaft Position Sensor Low Reference
89 | BN | -- | Sensor Low Reference
90 | -- | -- | Not Used
91 | L-BU | -- | Fuel Injector Control (4)
92 | L-BU | -- | Heated O2 Sensor Control Sensor 2
93 | GY | -- | 5-Volt Reference
94 | GY | -- | 5-Volt Reference
95 | D-BU/WH | -- | Crankshaft POS Sensor Signal (3)
96 | YE/BK | -- | Crankshaft POS Sensor Low Reference (3)
97 | D-BU | -- | Knock Sensor Signal (1)
98 | -- | -- | Not Used
99 | BN/WH | -- | Fuel Injector Control (3)
100 | L-GN | -- | Manifold Absolute Pressure Sensor Signal
101 | D-GN/WH | -- | Oil Temperature Sensor Signal
102 | PU/WH | -- | Heated O2 Sensor High Signal Bank 1 Sensor (2)
103 | PU/WH | -- | Heated O2 Sensor high Signal Bank 1 Sensor (1)
104 | D-GN | -- | High Idle Switch Control
105 | BN | -- | Oil Pressure Gage Signal
106 | D-GN/WH | -- | EVAP Canister Purge Solenoid Control
107 | BN | -- | Fuel Injector Control (1)
108 | BN | -- | Intake Air Temperature Sensor Signal
109 | YE | -- | Engine Coolant Temperature Sensor Signal
110 | GY | -- | Exhaust Gas Recirculation Vacuum Regulator Valve Signal
111 | BN | -- | Oil Level Switch Signal
112 | D-BU | -- | Throttle POS Sensor Signal (5)
113 | BN/WH | -- | Camshaft Position Sensor Signal
114 | D-BU | -- | Idle Speed Control Motor Control Retract
115 | -- | -- | Not Used
116 | L-BU | -- | Ignition Coil 1 and 4 Control
117 | D-GN | -- | Heated O2 Sensor Control Sensor 1
118 | GY | -- | Exhaust Gas Recirculation Solenoid Control
119 | L-BU | -- | Idle Speed Control Motor Control Extend
120 | -- | -- | Not Used
121 | D-GN/WH | -- | Ignition Coil 2 and 3 Control

### Engine Control Module (ECM) X2 (LLW)

#### Connector Part Information

- OEM: TYCO 284742-1
- Service: N/A
- Description: 60-Way F MQS+1 MM Unsealed

#### Engine Control Module (ECM) X2 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE/BK | 3101 | High
2 | 0.35 YE/D-BU | 3102 | High
3 | -- | -- | Not Used
4 | 0.35 D-BU/WH | 3104 | Ground
5-6 | -- | -- | Not Used
7 | 0.35 BK/WH | 3107 | Input
8 | 0.35 WH | 3108 | Ground
9-11 | -- | -- | Not Used
12 | 0.35 GY | 3112 | Heated O2 Sensor Heated High Contact Bank 1 Sensor (1)
13 | 0.35 GY/WH | 3113 | Heated O2 Sensor Heated Low Contact Bank 1 Sensor (1)
14 | -- | -- | Not Used
15 | 0.35 YE | 3115 | Signal
16 | 0.35 D-GN | 3116 | High
17 | 0.35 YE | 3117 | High
18 | -- | -- | Not Used
19 | 0.35 RD/BK | 3119 | Low
20 | 0.35 RD | 3120 | Heated O2 Sensor High Signal Bank 1 Sensor (2)
21 | 0.35 L-GN | 1174 | Oil Level Switch Signal
22 | -- | -- | Not Used
23 | 0.35 BN/WH | 3123 | Heated O2 Sensor Heater High Control Bank 1 Sensor (2)
24-26 | -- | -- | Not Used
27 | 0.35 D-GN | 3127 | Input
28 | 0.35 YE | 3128 | Supply
29-30 | -- | -- | Not Used
31 | 0.35 D-BU | 3131 | Low
32 | -- | -- | Not Used
33 | 0.35 GY | 3133 | Heated O2 Sensor Heater High Control Bank 1 Sensor (3)
34 | 0.35 BN | 3134 | Supply
35 | 0.35 BN | 445 | Oil Pressure Gage Signal
36 | -- | -- | Not Used
37 | 0.35 D-GN | 3137 | Signal
38-39 | -- | -- | Not Used
40 | 0.35 WH | 3140 | Battery Positive Voltage
41 | 0.35 D-BU/WH | 6282 | Fuel Level Sensor #2 Low Reference
42 | 0.35 YE | 3142 | Signal
43 | 0.35 D-BU | 3143 | Signal
44 | 0.35 D-GN | 3144 | Ground
45 | -- | -- | Not Used
46 | 0.35 D-GN/BK | 3146 | Low
47 | 0.35 WH | 3147 | Low
48 | -- | -- | Not Used
49 | 0.35 BK | 3149 | Ground
50 | 0.35 WH/BK | 3150 | Signal
51 | -- | -- | Not Used
52 | 0.35 WH | 3152 | TPA
53 | 0.35 YE | 3153 | Signal
54-57 | -- | -- | Not Used
58 | 0.35 L-BU | 1937 | Secondary Fuel Level Sensor Signal
59 | 0.35 D-GN | 3159 | TPA
60 | 0.35 PK | 3160 | EGR

### Engine Control Module (ECM) X2 (LU1)

#### Connector Part Information

- OEM: BOSCH 1928404780 (W/Cover)
- Service: N/A
- Description: 58-Way F ECU Sealed

#### Engine Control Module (ECM) X2 (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 250 | Ground
2 | 0.35 BK | 250 | Ground
3 | 0.35 PK/BK | 5290 | Engine Main Relay Fused Control (1)
4 | 0.35 BK | 250 | Ground
5 | 0.35 PK/BK | 5290 | Engine Main Relay Fused Control (1)
6 | 0.35 PK/BK | 5290 | Engine Main Relay Fused Control (1)
7 | 0.35 GY/WH | 3122 | Heated O2 Sensor Low Bank 1 (2)
8 | -- | -- | Not Used
9 | 0.35 BN | 452 | Sensor Low Reference
10 | 0.35 D-GN/WH | 465 | Fuel Pump Primary Relay
11 | 0.35 BN | 5514 | Sensor low Reference
12 | -- | -- | Not Used
13 | 0.35 YE | 492 | Mass Air Flow Sensor Signal
14 | -- | -- | Not Used
15 | 0.35 D-BU | 1161 | APM Signal (1)
16 | 0.35 BN/WH | 379 | Cruise Control Clutch S/W Signal
17 | 0.35 OG/BN | 1785 | Tans Park/Neutral Signal (1)
18 | 0.35 PK/BK | 6316 | Engine Reverse Gear SW Signal
19 | -- | -- | Not Used
20 | 0.35 OG/WH | 3225 | Heat O2 Sensor Low Bank 2 (2)
21 | -- | -- | Not Used
22 | 0.35 BN | 2760 | Intake Air Temperature Sensor Low Reference
23 | 0.35 BN/WH | 1669 | Heat O2 Low Signal Bank 1 (2)
24 | 0.35 BN | 1671 | Heated O2 Low Signal Bank 1 Sensor (2)
25 | 0.35 L-BU | 1162 | APM Signal (1)
26 | 0.35 L-BU | 1937 | Secondary Fuel Level Sensor Signal
27-33 | -- | -- | Not Used
34 | 0.35 BN | 1271 | APM Low Reference (1)
35 | 0.35 D-GN | 2700 | 5-Volt Reference
36 | 0.35 D-BU | 1936 | Primary Fuel Level Sensor
37 | -- | -- | Not Used
38 | 0.35 PU/WH | 1668 | Heated O2 Sensor High Signal Bank 1 (2)
39 | 0.35 OG/BK | 380 | ACP Sensor Signal
40 | -- | -- | Not Used
41 | 0.35 D-BU | 5985 | Accessory Wakeup Serial Data
42 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1
43 | -- | -- | Not Used
44 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control
45 | 0.35 D-BU | 473 | High Speed Cooling Fan Relay Control
46 | 0.35 D-GN | 335 | Low Speed Cooling Fan Relay Control
47 | 0.35 PU | 1272 | APM Low References (2)
48 | 0.35 BN | 1274 | APM 5-Volt Reference (2)
49 | 0.35 WH/BK | 1164 | APM 5-Volt Reference (1)
50 | 0.35 BN | 472 | Intake Air Temperature Sensor Signal
51 | 0.35 PU | 1670 | Heated O2 High Signal Bank 2 (2)
52 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
53 | -- | -- | Not Used
54 | 0.35 PK | 539 | Run/Crank Ignition 1 Voltage
55 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) 1
56 | 0.35 RD/WH | 40 | Battery Positive Voltage
57 | 0.35 PU/WH | 1035 | Starter Relay Coil Control
58 | 0.35 BN | 5069 | Engine Main Relay Coil Control

### Engine Coolant Temperature (ECT) Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: PED 12040753
- Service: N/A
- Description: 2-Way F 150 Series Sealed

#### Engine Coolant Temperature (ECT) Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | CTS Ground
2 | YE | -- | CTS Signal

### Engine Coolant Temperature (ECT) Sensor (2.4L)

#### Connector Part Information

- OEM: PKI 832238
- Service: N/A
- Description: 2-Way F 150.2 Sealed

#### Engine Coolant Temperature (ECT) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Engine Coolant Temperature Sensor Signal
2 | BN | -- | Sensor Low Reference

### Engine Oil Pressure Sensor (LU1)

#### Connector Part Information

- OEM: 7283-2429
- Service: N/A
- Description: 3-Way F 150.2 Sealed (GY)

#### Engine Oil Pressure Sensor (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN/RD | 470 | Low Reference
2 | 0.35 GY | 605 | 5 Volt Reference
3 | 0.35 BN/BK | 231 | Engine Oil Pressure Sensor Signal

### EVAP Canister Purge Solenoid Valve (2.4L)

#### Connector Part Information

- OEM: PKI 832229
- Service: N/A
- Description: 2-Way F Sealed

#### EVAP Canister Purge Solenoid Valve (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/WH | -- | Engine Main Relay Fused Control (3)
2 | D-GN/WH | -- | EVAP Canister Purge Solenoid Control

### EVAP Canister Purge Solenoid Valve (3.2L)

#### Connector Part Information

- OEM: PKI 832229
- Service: N/A
- Description: 2-Way F Sealed

#### EVAP Canister Purge Solenoid Valve (3.2L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | EVAP Canister Vent Solenoid Control
2 | PK | -- | Run/Crank Ignition 1 Voltage

### Exhaust Gas Recirculation (EGR) Valve (2.0L Diesel)

#### Connector Part Information

- OEM: TYCO 827551-3
- Service: N/A
- Description: 2-Way F Timmer Sealed

#### Exhaust Gas Recirculation (EGR) Valve (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | EGR
2 | PK/BK | -- | Engine Main Relay Coil Control (3)

### Exhaust Gas Recirculation (EGR) Valve (2.4L)

#### Connector Part Information

- OEM: PKI 832503
- Service: N/A
- Description: 5-Way F 150 Sealed

#### Exhaust Gas Recirculation (EGR) Valve (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Exhaust Gas Recirculation Solenoid Control
2 | BN | -- | Sensor Low Reference
3 | GY | -- | Exhaust Recirculation Vacuum Valve Signal
4 | GY | -- | 5-Volt Reference
5 | PK/BK | -- | Engine Main Relay Fused Controls (3)

### Exhaust Gas Temperature Sensor I (2.0 Diesel)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Exhaust Gas Temperature Sensor I (2.0 Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN | -- | Signal 1
2 | BK/WH | -- | Low Reference

### Exhaust Gas Temperature Sensor 2 (2.0L Diesel)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Exhaust Gas Temperature Sensor 2 (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN/BK | -- | Signal 2
2 | BK | -- | Low Reference

### Fog Lamp

#### Connector Part Information

- OEM: PED 12124819
- Service: N/A
- Description: 2-Way Sealed

#### Fog Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Front Fog Lamp Supply Voltage
2 | BK | -- | Ground

### Folding Mirror Unit

#### Connector Part Information

- OEM: KUM PH 845-05010
- Service: N/A
- Description: 5-Way F CDR Unsealed

#### Folding Mirror Unit

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Fold Signal
2 | YE | -- | Extend Signal
3 | BK | -- | Ground
4 | PK | -- | Relay Control
5 | YE | -- | Accessory Voltage

### Fuel Door Lock Actuator

#### Connector Part Information

- OEM: PED 15332130
- Service: N/A
- Description: 2-Way M GT 150 Unsealed

#### Fuel Door Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Door Lock Actuator Lock Control
2 | BN | -- | Door Lock Actuator Unlock Control

### Fuel Filter Heater/Temperature Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: FCI 17260406A
- Service: N/A
- Description: 6-Way F 150/280 Series Sealed

#### Fuel Filter Heater/Temperature Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | -- | Ground (LHD)
Ignition Voltage (RHD)
4 | BU | -- | Power Take Off Enable Switch (LHD)
Fuel Filter Heater (RHD)
5 | GN | -- | Heated Oxygen Sensor Low Signal Bank 2 Sensor 1 (LHD)
Fuel Temperature Signal (RHD)
6 | BK/WH | -- | Heated Oxygen Sensor High Signal Bank 2 Sensor 1 (LHD)
Fuel Temperature Ground (RHD)

### Fuel Injector 1 (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 1 (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | High
2 | WH | -- | Low

### Fuel Injector 1 (2.4L)

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 1 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (1)

### Fuel Injector 2 (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 2 (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/D-BU | -- | High
2 | D-BU | -- | Low

### Fuel Injector 2 (2.4L)

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 2 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | BN/WH | -- | Fuel Injector Control (3)

### Fuel Injector 3 (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 3 (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | High
2 | D-GN/BK | -- | Low

### Fuel Injector 3 (2.4L)

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 3 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (4)

### Fuel Injector 4 (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Injector 4 (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | High
2 | GY | -- | Low

### Fuel Injector 4 (2.4L)

#### Connector Part Information

- OEM: PED 12131678
- Service: N/A
- Description: 2-Way F Minifuse Sealed

#### Fuel Injector 4 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | L-BU | -- | Fuel Injector Control (2)

### Fuel Pump Module (2.4L)

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition Voltage
2 | BN/WH | -- | Fuel Level Sensor Low
3 | D-BU | -- | Primary Fuel Level Sensor
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Fuel Pump Module (2.0L Diesel)

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition Voltage
2 | BN/WH | -- | Fuel Level Sensor Low
3 | D-BU | -- | Primary Fuel Level Sensor
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Fuel Pump Module (3.2L)

#### Connector Part Information

- OEM: KET MG641521
- Service: N/A
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module (3.2L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition Voltage
2 | BN/WH | -- | Fuel Level Sensor Low
3 | D-BU | -- | Primary Fuel Level Sensor
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Fuel Rail Pressure Control Valve (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Control Valve (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Low
2 | D-BU/WH | -- | Ground

### Fuel Rail Pressure Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403968
- Service: N/A
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Ground
2 | D-BU | -- | Signal
3 | YE | -- | Supply

### Fuel Tank Pressure Sensor (3.2L)

#### Connector Part Information

- OEM: PKI 832311
- Service: N/A
- Description: 3-Way F 150 Sealed

#### Fuel Tank Pressure Sensor (3.2L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Fuel Level Sensor Low
2 | D-GN | -- | Fuel Tank Pressure Sensor Signal
3 | GY | -- | Fuel Tank Pressure Sensor 5-Volt Reference

### Generator

#### Connector Part Information

- OEM: PED 12186568
- Service: N/A
- Description: 4-Way F 150 Unsealed

#### Generator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN | -- | Charge Indicator Control
3 | GY | -- | Generator Field Duty Cycle Signal
4 | -- | -- | Not Used

### Glow Plug Control Unit (2.0L Diesel)

#### Connector Part Information

- OEM: FCI 60432001
- Service: N/A
- Description: 11-Way F Sealed

#### Glow Plug Control Unit (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Shunt High Signal
2 | GY | -- | Shunt High Signal
3 | GY | -- | Shunt High Signal
4 | GY | -- | Shunt High Signal
5 | -- | -- | Not Used
6 | PK/BK | -- | Ignition Voltage
7 | BK/WH | -- | Signal Ground
8 | -- | -- | Not Used
9 | WH | -- | GPCU 01
10 | RD/WH | -- | Battery Positive Voltage
11 | WH/RD | -- | GPCU ST

### Hands Free Unit

#### Connector Part Information

- OEM: KET MG 651563
- Service: N/A
- Description: 23-Way F MS-AL Unsealed

#### Hands Free Unit

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Audio Earpiece Signal
2 | -- | -- | Not Used
3 | PK | -- | Audio Handset Low Ref
4 | GY | -- | Cell RF Boost Control Signal
5 | YE/BK | -- | Cell Mute Signal
6 | L-BU/BK | -- | Cell Voice Low Ref
7 | -- | -- | Not Used
8 | D-BU | -- | Cell Voice Signal
9 | -- | -- | Not Used
10 | PK | -- | Ext Speaker (+)
11 | GY/BK | -- | Transceiver Low Ref
12 | L-GN | -- | Handset Volume Control Ground
13 | -- | -- | Not Used
14 | D-BU/WH | -- | Handset Volume Control Supply
15-16 | -- | -- | Not Used
17 | GY/BK | -- | Mic (+)
18 | GY/BK | -- | Mic Signal
19 | BK | -- | Ground
20 | D-GN | -- | Cell Mic Low Ref
21 | YE | -- | Ignition Voltage
22 | GY | -- | Cell Mic Signal
23 | GY | -- | Ext Speaker (-)

### Hazard Switch

#### Connector Part Information

- OEM: PED 15499928
- Service: N/A
- Description: 6-Way F HVT Unsealed

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Traction Control Signal
2 | BK | -- | Ground
3-5 | -- | -- | Not Used
6 | YE | -- | IP Dimming

### Head Lamp Washer Pump

#### Connector Part Information

- OEM: GHW 18255050000
- Service: N/A
- Description: 2-Way F Sealed

#### Head Lamp Washer Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Headlamp Washer Pump Control
2 | BK | -- | Ground

### Headlamp - Left

#### Connector Part Information

- OEM: KUM PB625-04027
- Service: N/A
- Description: 4-Way F NMWP Sealed

#### Headlamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Headlamp Low Beam Supply Voltage
2 | D-GN/WH | -- | Left Headlamp High Beam Supply Voltage
3 | BK | -- | Ground
4 | -- | -- | Not Used

### Headlamp - Left (w/Leveling)

#### Connector Part Information

- OEM: KUM PB625-06027
- Service: N/A
- Description: 6-Way F GT 150 Series Sealed

#### Headlamp - Left (w/Leveling)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PU | -- | Left Park Lamp Supply Voltage
3 | D-GN | -- | Headlamp Leveling Motor Supply Voltage
4 | D-GN/WH | -- | Left Headlamp High Beam Supply Voltage
5 | YE | -- | Left Headlamp Low Beam Supply Voltage
6 | BK | -- | Ground

### Headlamp - Right

#### Connector Part Information

- OEM: KUM PB625-04027
- Service: N/A
- Description: 4-Way F NMWP Sealed

#### Headlamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Right Headlamp Low Beam Supply Voltage
2 | L-GN/BN | -- | Right Headlamp High Beam Supply Voltage
3 | BN | -- | Ground
4 | -- | -- | Not Used

### Headlamp - Right (w/Leveling)

#### Connector Part Information

- OEM: KUM PB625-06027
- Service: N/A
- Description: 6-Way F NWMP Sealed

#### Headlamp - Right (w/Leveling)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BN/WH | -- | Right Park Lamp Supply Voltage
3 | D-GN | -- | Hold Leveling Motor Supply Voltage
4 | L-GN/BK | -- | Right Headlamp High Beam Supply Voltage
5 | BN/WH | -- | Right Headlamp Low Beam Supply Voltage
6 | BK | -- | Ground

### Heated Oxygen Sensor HO2S 1 (2.4L)

#### Connector Part Information

- OEM: TYCO 174257-2
- Service: N/A
- Description: 4-Way F MARK-II Sealed

#### Heated Oxygen Sensor (HO2S) 1 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated O2 Sensor High Signal Bank 1 Sensor 1
2 | PK/BK | -- | Engine Main Relay Fused Control (2)
3 | BN/WH | -- | Heated O2 Sensor Low Signal Bank 1 Sensor 2
4 | D-GN | -- | Heated O2 Sensor Control Sensor 1

### Heated Oxygen Sensor (HO2S) 2 (2.4L)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP Sealed

#### Heated Oxygen Sensor (HO2S) 2 (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated O2 Sensor High Signal Bank 1 Sensor 2
2 | PK/BK | -- | Engine Main Relay Fused Control (2)
3 | BN/WH | -- | Heated O2 Sensor Low Signal Bank 1 Sensor 1
4 | L-BU | -- | Heated O2 Sensor Control Sensor 2

### Heated Oxygen Sensor Bank 2 (3.2L)

#### Connector Part Information

- OEM: BOSCH 1928403453
- Service: N/A
- Description: 4-Way F Sealed

#### Heated Oxygen Sensor Bank 2 (3.2L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Engine Main Relay Fused Control (4)
2 | OG/WH | -- | Heated O2 Sensor Bank 2 (2)
3 | BN | -- | Heated O2 Low Signal Bank 2 (2)
4 | PU | -- | Heated O2 High Signal Bank 2 (2)

### Heated Seat - Left

#### Connector Part Information

- OEM: MG 610207
- Service: N/A
- Description: 2-Way F Unsealed

#### Heated Seat - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Heated Seat Switch Signal
2 | BK | -- | Ground

### Heated Seat - Right

#### Connector Part Information

- OEM: MG 610207
- Service: N/A
- Description: 2-Way F Unsealed

#### Heated Seat - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Heated Seat Switch Signal
2 | BK | -- | Ground

### Heated Seat Switch - Left

#### Connector Part Information

- OEM: PED 15499928
- Service: N/A
- Description: 6-Way F 064 Unsealed

#### Heated Seat Switch - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | L-BU | -- | Signal
5 | BN | -- | Ignition 3 Voltage
6 | BK | -- | Ground

### Heated Seat Switch - Left

#### Connector Part Information

- OEM: PED 15406141
- Service: N/A
- Description: 8-Way F 064 Unsealed

#### Heated Seat Switch - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | BN | -- | Ignition 3 Voltage
4 | BU | -- | Left Heated Seat Back Switch Signal
5 | PU/WH | -- | LED Dimming Signal
6 | L-BU | -- | Left Heated Seat Low Indicator
7 | WH/BK | -- | Left Heated Seat Medium Indicator
8 | GN | -- | Left Heated Seat High Indicator

### Heated Seat Switch - Right

#### Connector Part Information

- OEM: PED 15406141
- Service: N/A
- Description: 8-Way F 064 Unsealed

#### Heated Seat Switch - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | BN | -- | Ignition 3 Voltage
4 | PU | -- | Right Heated Seat Back Switch Signal
5 | PU/WH | -- | LED Dimming Signal
6 | YE | -- | Right Heated Seat Low Indicator
7 | WH/BK | -- | Right Heated Seat Medium Indicator
8 | BN | -- | Right Heated Seat High Indicator

### Heated Seat Switch - Right

#### Connector Part Information

- OEM: PED 15499928
- Service: N/A
- Description: 6-Way F 064 Unsealed

#### Heated Seat Switch - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | L-BU | -- | Signal
5 | BN | -- | Ignition 3 Voltage
6 | BK | -- | Ground

### High Pressure Pump (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Service: N/A
- Description: 2-Way F Sealed

#### High Pressure Pump (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | -- | Low
2 | BK | -- | Ground

### Hill Descent Switch

#### Connector Part Information

- OEM: PED 15499927
- Service: N/A
- Description: 6-Way F Micro 064 Unsealed

#### Hill Descent Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Hill Descent Switch Signal
2 | BK | -- | Ground
3-5 | -- | -- | Not Used
6 | YE | -- | Illumination Signal

### Hood Open Switch

#### Connector Part Information

- OEM: PED 15326808
- Service: N/A
- Description: 3-Way F Sealed

#### Hood Open Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Hood Closed S/W Signal
2 | -- | -- | Not Used
3 | BK | -- | Ground

### HVAC Control Module X1 (C68)

#### Connector Part Information

- OEM: PED 15326953
- Service: N/A
- Description: 16-Way F GT 280 Unsealed

#### HVAC Control Module X1 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | EVAP Core Temperature Sensor Signal
2 | D-GN/WH | -- | Steering Wheel Module Low Signal
3 | L-BU | -- | Rear Defog Switch Signal
4 | D-GN | -- | Low Speed GMLAN Serial Data
5 | BN/WH | -- | I/P Lamp Dimming Control
6 | BN | -- | Run Ignition 3 Voltage
7 | BN | -- | Run Ignition 3 Voltage
8 | RDWH | -- | Battery Positive Voltage
9 | BN | -- | EVAP Core Temperature Sensor Low Reference
10 | BN | -- | Rear Defog Indicator Supply Voltage
11 | WH/BK | -- | PTC Heater Request Signal
12 | WH | -- | RR Defog Relay Control
13 | BN/WH | -- | I/P Lamp Dimming Control
14 | L-BU | -- | Solar Sensor Driver Signal
15 | PU/WH | -- | Air Quality Sensor Signal
16 | BK | -- | Ground

### I/P Compartment Lamp

#### Connector Part Information

- OEM: PKI 836277
- Service: N/A
- Description: 2-Way F G/Lam Unsealed

#### I/P Compartment Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | Body Control Module 12-Volt Reference
2 | PU | -- | I/P Compartment Lamp Control

### I/P Compartment Lamp Switch

#### Connector Part Information

- OEM: PKI 836277
- Service: N/A
- Description: 2-Way F G/Lam Unsealed

#### I/P Compartment Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | PU | -- | I/P Compartment Lamp Control

### Ignition Coil Module (2.4L)

#### Connector Part Information

- OEM: PKI 832311
- Service: N/A
- Description: 3-Way F 150 Sealed

#### Ignition Coil Module (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | -- | Ignition Coil 2 and 3 Control
2 | PK | -- | Run/Crank Ignition 1 Voltage
3 | L-BU | -- | Ignition Coil 1 and 4 Control

### Ignition Key Cylinder Lamp

#### Connector Part Information

- OEM: AMP 368502-1
- Service: N/A
- Description: 6-Way F Unsealed

#### Ignition Key Cylinder Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground
3 | D-GN | -- | Serial Data
4 | BK | -- | Ground
5 | D-BU | -- | Serial Data
6 | RD/WH | -- | Battery Positive Voltage

### Ignition Switch

#### Connector Part Information

- OEM: JAE IL-AG5-6S-S3C1
- Service: N/A
- Description: 6-Way F IL5 Unsealed

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Accessory Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | PK | -- | Ignition 1 Voltage
4 | WH/BK | -- | Ignition Key Resistor Signal
5 | WH | -- | Off/Run/Crank Voltage
6 | -- | -- | Not Used

### Inclination Sensor

#### Connector Part Information

- OEM: PED 15324229
- Service: N/A
- Description: 4-Way F Timer Micro I Unsealed (BK)

#### Inclination Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | -- | -- | Not Used
3 | L-BU | -- | Incline Sensor Alarm On Signal
4 | D-GN | -- | Alarm Armed Signal

### Inflatable Restraint Retractor Pretensioner - Left Front (C105/Short Body)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Inflatable Restraint Retractor Pretensioner - Left Front (C105/Short Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | LF Retractor Pretensioner High Control
2 | PU | -- | LF Retractor Pretensioner Low Control

### Inflatable Restraint Retractor Pretensioner - Right Front (C105/Short Body)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way F

#### Inflatable Restraint Retractor Pretensioner - Right Front (C105/Short Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | RF Retractor Pretensioner High Control
2 | GN | -- | RF Retractor Pretensioner Low Control

### Inflatable Restraint Roof Rail Module - Left

#### Connector Part Information

- OEM: FCI 4100-1101
- Service: N/A
- Description: 2-Way F Unsealed

#### Inflatable Restraint Roof Rail Module - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | LF Roof Rail Module Low
2 | PU/WH | -- | LF Roof Rail Module High

### Inflatable Restraint Roof Rail Module - Right

#### Connector Part Information

- OEM: FCI 4100-1101
- Service: N/A
- Description: 2-Way F Unsealed

#### Inflatable Restraint Roof Rail Module - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | -- | RF Roof Rail Module Low
2 | YE/BK | -- | RF Roof Rail Module High

### Inflatable Restraint Side Impact Sensor - Left Front

#### Connector Part Information

- OEM: PED 15356723
- Service: N/A
- Description: 2-Way F 150 GT Sealed

#### Inflatable Restraint Side Impact Sensor - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BN | -- | LT MID SISM Low Reference
2 | D-GN/WH | -- | LT MID SISM Signal

### Inflatable Restraint Side Impact Sensor - Right Front

#### Connector Part Information

- OEM: PED 15356723
- Service: N/A
- Description: 2-Way F 150 GT Sealed

#### Inflatable Restraint Side Impact Sensor - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | -- | RT MID SISM Low Reference
2 | L-BU/BK | -- | RT MID SISM Signal

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BN | 180 | Remote CD/Cassette Player Supply Voltage (C100)
B | 0.35 L-GN | 1011 | Remote Radio Control Signal (C105)
C | 0.35 GY | 1884 | Cruise Controls Switch Signal (C100)
C | 0.35 BK | 351 | Ground (C105)
D | 0.35 L-GY | 902 | Handset Volume Control Ground (C100/LHD)
E | 0.35 L-GN | 1011 | Remote Radio Control Signal (C100)
E | 0.35 PK | 1444 | 12-Volt Reference (C105)
F | 0.35 PK | 1444 | 12-Volt Reference (C100)
F | 0.35 YE/BK | 9088 | I/P Lamp Supply Voltage (C105)
G | 0.35 BU/WH | 901 | Handset Volume Control Supply (C100/LHD)
H | -- | -- | Not Used
J | 0.35 BK | 350 | Ground
K | 0.35 TN | 28 | Horn Relay Control

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BN | 180 | Remote CD/Cassette Player Supply Voltage (C100)
B | 0.35 L-GN | 1011 | Remote Radio Control Signal (C105)
C | 0.35 GY | 1884 | Cruise Controls Switch Signal (C100)
C | 0.35 BK | 351 | Ground (C105)
D | 0.35 L-GY | 902 | Handset Volume Control Ground (C100/LHD)
E | 0.35 L-GN | 1011 | Remote Radio Control Signal (C100)
E | 0.35 PK | 1444 | 12-Volt Reference (C105)
F | 0.35 PK | 1444 | 12-Volt Reference (C100)
F | 0.35 YE/BK | 9088 | I/P Lamp Supply Voltage (C105)
G | 0.35 BU/WH | 901 | Handset Volume Control Supply (C100/LHD)
H | -- | -- | Not Used
J | 0.35 BK | 350 | Ground
K | 0.35 TN | 28 | Horn Relay Control

### Instrument Cluster

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F Mirco 064 Unsealed

#### Instrument Cluster

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Run/Crank Ignition 1 Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | -- | -- | Not Used
4 | PU | -- | Passenger Seat Belt Indicator
5 | BN/WH | -- | Transfer Case Positive Switch Ch 4 Encoder Signal
6 | OG/BK | -- | Sensor Low Reference
7 | D-GN/WH | -- | Outside Ambient Air Temperature Sensor S
8 | BN/WH | -- | Windshield Washer Fluid Level Sensor Signal
9 | YE | -- | Backlight Lamp Control
10 | BK | -- | Ground
11 | -- | -- | Not Used
12 | GY | -- | Rear Parking Assist Red Indicator Control
13 | BK | -- | Ground
14 | D-GN | -- | Low Speed GMLAN Serial Data
15 | -- | -- | Not Used
16 | PU | -- | Brake Fluid Level Sensor Signal

### Intake Air Temperature (IAT) Sensor (2.4L)

#### Connector Part Information

- OEM: TYCO 85202-1
- Service: N/A
- Description: 2-Way F Sealed

#### Intake Air Temperature (IAT) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Intake Air Temperature Sensor Low Reference
2 | BN | -- | Intake Air Temperature Sensor Signal

### Intrusion Sensor

#### Connector Part Information

- OEM: TYCO 368500-1
- Service: N/A
- Description: 3-Way F 070 Unsealed

#### Intrusion Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN | -- | Alarm Armed Signal
2 | PU | -- | Intrusion Sensor Alarm ON Signal
3 | RD/WH | -- | Battery Positive Voltage

### Knock Sensor (2.4L)

#### Connector Part Information

- OEM: TYCO 368215-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Knock Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Knock Sensor Signal (1)
2 | BN | -- | Sensor Low Reference
3 | BK/WH | -- | Signal Ground

### License Lamp

#### Connector Part Information

- OEM: MG 630679
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### License Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Left Park Lamp Supply Voltage
2 | BK | -- | Ground

### Liftgate Actuator

#### Connector Part Information

- OEM: MG 620490
- Service: N/A
- Description: 2-Way M MN-AL Unsealed

#### Liftgate Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Door Lock Actuator Unlock Control
2 | GY | -- | Door Lock Actuator Lock Control

### Liftgate Ajar

#### Connector Part Information

- OEM: MG 651201-4
- Service: N/A
- Description: 2-Way F 090III Unsealed (GY)

#### Liftgate Ajar

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Liftgate Ajar Switch Signal (1)
2 | BK | -- | Ground

### Liftgate Glass

#### Connector Part Information

- OEM: TYCO 936227-1
- Service: N/A
- Description: 4-Way F 090III Unsealed

#### Liftgate Glass

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Ground
2 | PK/BK | -- | Liftgate Ajar SW Signal 1
3 | BN | -- | Lift Glass/Trunk MTR Release Control
4 | BK | -- | Ground

### Liftgate Key Cylinder

#### Connector Part Information

- OEM: TYCO 368538-1
- Service: N/A
- Description: 2-Way F 070 Unsealed

#### Liftgate Key Cylinder

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Trunk Key Switch Signal
2 | BK | -- | Ground

### Manifold Absolute Pressure (MAP) Sensor (2.4L)

#### Connector Part Information

- OEM: TYCO 174359-2
- Service: N/A
- Description: 3-Way F Mark II Sealed

#### Manifold Absolute Pressure (MAP) Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference
2 | L-GN | -- | Signal
3 | OG/BK | -- | Low Reference

### Map Lamp

#### Connector Part Information

- OEM: PED 13513470
- Service: N/A
- Description: 8-Way F Unsealed

#### Map Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PU | -- | Dome Lamp Defeat
3 | -- | -- | Not Used
4 | BK | -- | Ground
5 | PU | -- | Intrusion Disable Signal
6 | OG | -- | BCM 12-Volt Supply
7 | BK | -- | Ground
8 | -- | -- | Not Used

### Mass Air Flow (MAF) Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: BOSCH 1928403736
- Service: N/A
- Description: 4-Way F Sealed

#### Mass Air Flow (MAF) Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition 1 Voltage
2 | D-GN | -- | Ground
3 | D-GN | -- | Signal
4 | YE | -- | STC

### Mass Air Flow (MAF) Sensor (3.2L)

#### Connector Part Information

- OEM: PED 15355207
- Service: N/A
- Description: 5-Way F GT 150 Sealed

#### Mass Air Flow (MAF) Sensor (3.2L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 492 | MAF Sensor Signal
B | 0.35 PK | 539 | Ignition 1 Voltage
C | 0.35 BK/WH | 251 | Ground
D | 0.35 BN | 2760 | IAT Sensor Low Reference
E | 0.35 L-BU | 492 | IAT Sensor Signal

### Navigation Unit

#### Connector Part Information

- OEM: TYCO 368542-1
- Service: N/A
- Description: 12-Way F 064 Unsealed

#### Navigation Unit

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | YE | -- | Ignition Voltage
4 | D-GN/WH | -- | VSS Signal
5-8 | -- | -- | Not Used
9 | GY/BK | -- | Mic (+)
10 | GY/BK | -- | Mic Signal
11 | BN/WH | -- | Serial Data (High)
12 | GY/WH | -- | Serial Data (High)

### Object Detection Module

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F 064 Unsealed

#### Object Detection Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Run Ignition 3 Voltage
2 | GY | -- | Park Assist Alarm Low Reference
3 | D-BU | -- | Park Assist Alarm Volt Reference
4 | L-GN | -- | Backup Lamp Supply Voltage
5 | YE | -- | Left Rear Corner Object Sensor Signal
6 | OG | -- | Left Rear Middle Object Sensor Signal
7 | D-GN | -- | Right Rear Middle Object Sensor Signal
8 | PU | -- | Right Rear Corner Object Sensor Signal
9 | BK | -- | Ground
10 | -- | -- | Not Used
11 | YE | -- | Park Assist Alarm Signal
12 | L-BU | -- | Park Brake Switch Signal
13 | GY | -- | Object Sensor Low Reference
14 | -- | -- | Not Used
15 | GY | -- | RR Parking Assist RED Indicator Control
16 | GY/BK | -- | Object Sensor Low Reference

### Object Sensor - Left Rear Corner

#### Connector Part Information

- OEM: PED 15419715
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Object Sensor - Left Rear Corner

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Object Sensor Low Reference
2 | YE | -- | Left Rear Corner Object Sensor Signal

### Object Sensor - Left Rear Middle

#### Connector Part Information

- OEM: PED 15419715
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Object Sensor - Left Rear Middle

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Object Sensor Low Reference
2 | OG | -- | Left Rear Middle Object Sensor Signal

### Object Sensor - Right Rear Corner

#### Connector Part Information

- OEM: PED 15419715
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Object Sensor - Right Rear Corner

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Object Sensor Low Reference
2 | PU | -- | Right Rear Corner Object Sensor Signal

### Object Sensor - Right Rear Middle

#### Connector Part Information

- OEM: PED 15419715
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Object Sensor - Right Rear Middle

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Object Sensor Low Reference
2 | D-GN | -- | Right Rear Middle Object Sensor Signal

### Oil Level Sensor (2.4L)

#### Connector Part Information

- OEM: PED 15326808
- Service: N/A
- Description: 3-Way F GT 150 Sealed

#### Oil Level Sensor (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Sensor Low Reference
2 | D-GN/WH | -- | Oil Temperature Sensor Signal
3 | BN | -- | Oil Level Switch Signal

### Oil Level Switch (2.0L Diesel)

#### Connector Part Information

- OEM: PED 12052641
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series Sealed

#### Oil Level Switch (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Oil Level SW Signal
2 | BN | -- | Ground

### Oil Pressure Switch (2.0L Diesel)

#### Connector Part Information

- OEM: PKI 832104
- Service: N/A
- Description: 1-Way F 150 Series Sealed

#### Oil Pressure Switch (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Oil Pressure Gage Signal

### Oil Pressure Switch (2.4L)

#### Connector Part Information

- OEM: PKI 832104
- Service: N/A
- Description: 1-Way F 150 Sealed

#### Oil Pressure Switch (2.4L)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Oil Pressure Gage Signal

### Outside Air Temperature/Air Quality Sensor

#### Connector Part Information

- OEM: KET MG 610331
- Service: N/A
- Description: 4-Way F SWP Sealed

#### Outside Air Temperature/Air Quality Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Low Reference
2 | BN | -- | Ignition 3 Voltage
3 | GN/WH | -- | Outside Air Temperature Signal
4 | PU/WH | -- | Air Quality Sensor Signal

### Outside Air Temperature/Air Quality Sensor (C68)

#### Connector Part Information

- OEM: KET MG 610331
- Service: N/A
- Description: 4-Way F SWP Sealed

#### Outside Air Temperature/Air Quality Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Low Reference
2 | BN | -- | 12-Volt Reference
3 | D-GN/WH | -- | Outside Air Temperature Sensor Signal
4 | PU/WH | -- | Air Quality Sensor Signal

### Outside Rearview Mirror (OSRVM) - Left (LHD)

#### Connector Part Information

- OEM: TYCO 174045-2
- Service: N/A
- Description: 12-Way F 040 Unsealed

#### Outside Rearview Mirror (OSRVM) - Left (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | L-BU/WH | -- | Left Front T/Signal Lamp Supply Voltage
4 | WH | -- | Left Mirror Right Control
5 | YE | -- | Mirror Motor Right/Up Control
6 | L-GN | -- | Left Mirror Motor Down Control
7 | -- | -- | Not Used
8 | YE | -- | Left Folding Mirror Motor Extend Control
9 | L-BU | -- | Left Folding Mirror Motor Retract Control
10 | OG | -- | Mirror Heater Element Voltage
11 | BK | -- | Ground
12 | -- | -- | Not Used

### Outside Rearview Mirror (OSRVM) - Left (RHD)

#### Connector Part Information

- OEM: TYCO 174045-2
- Service: N/A
- Description: 12-Way F 040 Unsealed

#### Outside Rearview Mirror (OSRVM) - Left (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU/WH | -- | Right Front T/Signal Lamp Supply Voltage
4 | OG/WH | -- | Right Mirror Motor Right Control
5 | YE | -- | Mirror Motor Right Up Control
6 | PU/WH | -- | Right Mirror Motor Down Control
7 | -- | -- | Not Used
8 | YE | -- | Left Folding Mirror Motor Extend Control
9 | L-BU | -- | Left Folding Mirror Motor Retract Control
10 | OG | -- | Mirror Heater Element Volume
11 | BK | -- | Ground
12 | -- | -- | Not Used

### Outside Rearview Mirror (OSRVM) - Right (LHD)

#### Connector Part Information

- OEM: TYCO 174045-2
- Service: N/A
- Description: 12-Way F 040 Unsealed

#### Outside Rearview Mirror (OSRVM) - Right (LHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Right Mirror Motor Down Control
2 | YE | -- | Mirror Motor Right/Up Control
3 | OG/WH | -- | Right Mirror Motor Right Control
4 | D-BU | -- | Right GRT T/Signal Lamp Supply Voltage
5-7 | -- | -- | Not Used
8 | BK | -- | Ground
9 | OG | -- | Mirror Heater Element Voltage
10 | L-BU | -- | Left Folding Mirror Motor Retract Control
11 | YE | -- | Left Folding Mirror Motor Extend Control
12 | -- | -- | Not Used

### Outside Rearview Mirror (OSRVM) - Right (RHD)

#### Connector Part Information

- OEM: TYCO 174045-2
- Service: N/A
- Description: 12-Way F 040 Unsealed

#### Outside Rearview Mirror (OSRVM) - Right (RHD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Left Mirror Motor Down Control
2 | YE | -- | Mirror Motor Right/Up Control
3 | WH | -- | Left Mirror Motor Right Control
4 | L-BU/WH | -- | Left Front T/Signal Lamp Supply Voltage
5-7 | -- | -- | Not Used
8 | BK | -- | Ground
9 | OG | -- | Mirror Heater Element Voltage
10 | L-BU | -- | Left Folding Mirror Motor Retract Control
11 | YE | -- | Left Folding Mirror Motor Extend Control
12 | -- | -- | Not Used

### Outside Rearview Mirror (OSRVM) Switch

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F 064 Unsealed

#### Outside Rearview Mirror (OSRVM) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | -- | Ground
4 | WH | -- | Left Mirror Motor Right Control
5 | YE | -- | Mirror Motor Right/Up Control
6 | PU/WH | -- | Right Mirror Motor Down Control
7 | PK | -- | Folding Mirror Extend Motor Relay Control
8 | L-GN | -- | Left Mirror Motor Down Control
9 | BN/WH | -- | Headlamp Washer Pump Switch Signal
10 | BN/WH | -- | Right Headlamp Low Beam Supply Voltage
11 | D-GN | -- | Headlamp Leveling Motor Supply Voltage
12 | OG/WH | -- | 12-Volt Reference
13 | D-GN | -- | Instrument Panel Lamp dimmer Switch Signal
14 | YE | -- | Backlight Lamp Control
15 | YE | -- | Accessory Voltage
16 | OG/WH | -- | Right Mirror Motor Right Control

### Park Brake Switch

#### Connector Part Information

- OEM: PED 15326871
- Service: N/A
- Description: 2-Way F GT280 Sealed

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Park Brake Switch Signal
B | BK | -- | Ground

### Park/Turn Signal Lamp - Left

#### Connector Part Information

- OEM: TYCO 936187-1
- Service: N/A
- Description: 3-Way F 090 Sealed

#### Park/Turn Signal Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PU | -- | Left Park Lamp Supply Voltage
3 | L-BU/WH | -- | Left Front Turn Signal Lamp Supply Voltage

### Park/Turn Signal Lamp - Left (TR6)

#### Connector Part Information

- OEM: TYCO 936184-1
- Service: N/A
- Description: 2-Way F 090 Sealed

#### Park/Turn Signal Lamp - Left (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU/WH | -- | Left Front Turn Signal Lamp Supply Voltage

### Park/Turn Signal Lamp - Right

#### Connector Part Information

- OEM: TYCO 936187-1
- Service: N/A
- Description: 3-Way F 090 Sealed

#### Park/Turn Signal Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BN/WH | -- | Right Park Lamp Supply Voltage
3 | D-BU/WH | -- | Right Front Turn Signal Lamp Supply Voltage

### Park/Turn Signal Lamp - Right (TR6)

#### Connector Part Information

- OEM: TYCO 936184-1
- Service: N/A
- Description: 2-Way F 090 Sealed

#### Park/Turn Signal Lamp - Right (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU/WH | -- | Right Front Turn Signal Lamp Supply Voltage

### Passenger Seatbelt Indicator

#### Connector Part Information

- OEM: PED 15499929
- Service: N/A
- Description: 6-Way F Micro 064 HVT Unsealed

#### Passenger Seatbelt Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2-4 | PK | -- | Not Used
5 | PU | -- | Passenger Seatbelt Indicator
6 | -- | -- | Not Used

### Power Outlet - Cargo

#### Connector Part Information

- OEM: MG 630685-5
- Service: N/A
- Description: 2-Way F 205+250 Type Unsealed

#### Power Outlet - Cargo

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground

### Power Outlet - Rear

#### Connector Part Information

- OEM: MG 630685-3
- Service: N/A
- Description: 2-Way F 205+250 Type Unsealed

#### Power Outlet - Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground

### Power Seat Switch

#### Connector Part Information

- OEM: MG 610267
- Service: N/A
- Description: 4-Way F 250 Unsealed

#### Power Seat Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Heated Seat Switch Signal
2 | RD/WH | -- | Battery Positive Voltage
3 | BK | -- | Ground
4 | BK | -- | Ground

### Power Seat Test Connector

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Unsealed

#### Power Seat Test Connector

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground

### Power Sounder

#### Connector Part Information

- OEM: TYCO 1-967640-1
- Service: N/A
- Description: 4-Way F MQs Sealed

#### Power Sounder

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Run/Crank Ignition 1 Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | PK | -- | Power Sounder Enable Signal
4 | BK | -- | Ground

### Power Steering Control Module

#### Connector Part Information

- OEM: TYCO 368543-1
- Service: N/A
- Description: 14-Way F 070-Sealed

#### Power Steering Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Variable Effort Steering Solenoid Control
2 | L-BU | -- | Variable Effort Steering Solenoid Supply Voltage
3-5 | -- | -- | Not Used
6 | D-GN/WH | -- | Vehicle Speed Signal (VSS)
7 | -- | -- | Not Used
8 | BN | -- | Ignition 3-Voltage
9 | BN/WH | -- | Indicator Control
10 | BN/WH | -- | Ground
11-12 | -- | -- | Not Used
13 | D-BU/WH | -- | Serial Data
14 | -- | -- | Not Used

### Power Steering Magnetic Coil

#### Connector Part Information

- OEM: PED 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack Sealed

#### Power Steering Magnetic Coil

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Variable Effort Steering Solenoid Supply Voltage
2 | PU | -- | Variable Effort Steering Solenoid Control

### PRND Lamp

#### Connector Part Information

- OEM: MG611857
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### PRND Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | BN/WH | -- | I/P Lamp Dimming Control

### PTC Heater (2.0L Diesel)

#### Connector Part Information

- OEM: PED15326878
- Service: N/A
- Description: 3-Way F GT 280 Series Unsealed

#### PTC Heater (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU/WH | -- | PTC Heater Supply Voltage
GY | -- | Fuel Tank Pressure Sensor 5-Volt Reference
2 | YE/BK | -- | PTC Heater Supply Voltage
GY | -- | Fuel Tank Pressure Sensor Signal
3 | BN | -- | PTC Heater Supply Voltage

### Radio X1 (C100/Long Body)

#### Connector Part Information

- OEM: PED 1590072
- Service: N/A
- Description: 14-Way F 064+150 Unsealed

#### Radio X1 (C100/Long Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BN | -- | Left Front Speaker (+) 1
3 | L-GN | -- | Right Front Speaker (+) 1
4 | PK | -- | External Speaker Signal (+)
5 | GY | -- | External Speaker Signal
6 | GY | -- | Antenna Motor Up Control
7 | YE | -- | Backlight Lamp Control
8 | BK/WH | -- | Signal Ground
9 | GY | -- | Right Front Speaker Signal (-) 1
10 | D-GN | -- | Right Front Speaker Signal (-) 1
11 | -- | -- | Not Used
12 | BN | -- | Remote CD/Cassette Player Supply Voltage
13-14 | -- | -- | Not Used

### Radio X2 (C100/Long Body)

#### Connector Part Information

- OEM: PED 15394150
- Service: N/A
- Description: 16-Way F 064 Unsealed

#### Radio X2 (C100 Long Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Cellular Telephone RF Boost Control Signal
2 | PK/BK | -- | Amplifier powered Woofer Control (2)
3 | D-GN | -- | Right Subwoofer Speaker (+)
4 | YE/BK | -- | Cellular Telephone Mute Signal
5 | BN | -- | Left Rear Speaker (+)
6 | D-BU | -- | Right Rear Speaker (+)
7-8 | -- | -- | Not Used
9 | PU/WH | -- | Amplifier Powered Woofer Control (1)
10 | -- | -- | Not Used
11 | L-BU/BK | -- | Right Subwoofer Speaker (-)
12 | L-GN | -- | Remote Radio Control Signal
13 | YE | -- | Left Rear Speaker Signal (-)
14 | L-BU | -- | Right Rear Speaker Signal (-)
15 | -- | -- | Not Used
16 | YE | -- | Accessory Voltage

### Radio (C105/Short Body)

#### Connector Part Information

- OEM: FCI 30235101
- Service: N/A
- Description: 40-Way F Unsealed

#### Radio (C105/Short Body)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Right Rear Speaker (+)
2 | L-GN | -- | Right Front Speaker (+)
3 | BN | -- | Left Front Speaker (+)
4 | BN | -- | Left Rear Speaker (+)
5 | L-BU | -- | Right Rear Speaker Signal (-)
6 | GN | -- | Right Front Speaker Signal (-)
7 | GY | -- | Left Front Speaker Signal (-)
8 | YE | -- | Left Rear Speaker Signal
9 | BN/WH | -- | MID Speed CAN High
10 | BN | -- | MID Speed CAN Low
11 | YE/BK | -- | Cell Phone Mute Signal
12 | BK | -- | Ground
13 | -- | -- | Not Used
14 | L-BU | -- | Center Speaker
15 | RD/WH | -- | Battery Positive Voltage
16 | YE | -- | Center Speaker
17-33 | -- | -- | Not Used
34 | BU | -- | Cell Phone Voice Signal
35-36 | -- | -- | Not Used
37 | GN/WH | -- | EHU
38-39 | -- | -- | Not Used
40 | L-BU/BK | -- | Cell Phone Voice Signal

### Rain Sensor

#### Connector Part Information

- OEM: MOLEX 43645-0400
- Service: N/A
- Description: 4-Way F Micro Fit Unsealed

#### Rain Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Rain Sense Signal 2
2 | BN | -- | Rain Sense Signal 1
3 | BK | -- | Ground
4 | BN | -- | Accessory Voltage

### Rear Compartment Courtesy Lamp

#### Connector Part Information

- OEM: TYCO 936227-1
- Service: N/A
- Description: 4-Way F Unsealed

#### Rear Compartment Courtesy Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | OG | -- | BCM 12-Volt Reference
3 | BK | -- | Ground
4 | -- | -- | Not Used

### Rear Differential Clutch Control Module

#### Connector Part Information

- OEM: PED PE134674
- Service: N/A
- Description: 10-Way F 0.64 Sealed

#### Rear Differential Clutch Control Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | -- | Serial Data Communication Enable
2 | -- | -- | Not Used
3 | BK | -- | Ground
4-6 | -- | -- | Not Used
7 | BN/BK | -- | High Speed GMLAN Serial Data (+) 1
8 | BN | -- | High Speed GMLAN Serial Data (-) 1
9 | -- | -- | Not Used
10 | RD/WH | -- | Battery Positive Voltage

### Rear Monitor

#### Connector Part Information

- OEM: TYCO 368542-1
- Service: N/A
- Description: 12-Way F 064 Unsealed

#### Rear Monitor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | 12V Reference
2 | GY/BK | -- | Courtesy Lamp Relay Control
3 | -- | -- | Not Used
4 | -- | -- | Not Used
5 | YE | -- | Ignition Voltage
6 | BK | -- | Ground
7-10 | -- | -- | Not Used
11 | BK | -- | Ground
12 | RD/WH | -- | Battery Positive Voltage

### Rear Window Wiper Module

#### Connector Part Information

- OEM: TYCO 936230-1
- Service: N/A
- Description: 6-Way F 090III Unsealed

#### Rear Window Wiper Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Rear Window Wiper Switch Signal
2 | OG | -- | Rear Wiper Auto On Signal
3 | PK/BK | -- | Lift Gate Ajar Switch Signal
4 | BK | -- | Ground
5 | RD/WH | -- | Battery Positive Voltage
6 | D-GN | -- | Rear Window Washer Pump Control

### Rear Window Washer Fluid Pump

#### Connector Part Information

- OEM: KET MG 640605-5
- Service: N/A
- Description: 2-Way F 090 Sealed

#### Rear Window Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | D-GN | -- | Rear Window Washer Pump

### Remote Control Door Lock Receiver

#### Connector Part Information

- OEM: JAEIL AG5-4S-S3C1
- Service: N/A
- Description: 4-Way F AG5 Unsealed

#### Remote Control Door Lock Receiver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | GN | -- | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | BK | -- | Ground

### Resistor

#### Connector Part Information

- OEM: PED 15326801
- Service: N/A
- Description: 2-Way F GT 150 Sealed

#### Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/BK | -- | High Speed GMLAN Serial Data (+) 1
2 | BN | -- | High Speed GMLAN Serial Data (-) 1

### Seatbelt Reminder Sensor

#### Connector Part Information

- OEM: TYCO 368538-1
- Service: N/A
- Description: 2-Way F 070 Unsealed

#### Seatbelt Reminder Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Seatbelt Indicator Control
2 | PK | -- | Seat Position Switch Low Reference

### Seatbelt Switch - Left

#### Connector Part Information

- OEM: PED 15304649
- Service: N/A
- Description: 6-Way Unsealed

#### Seatbelt Switch - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Driver Seat Belt Pretensioner High
2 | PK | -- | Seat Position Switch Low Reference
3 | YE/BK | -- | LFR SIS Module Low Control
4 | OG/BK | -- | Driver Seat Belt Pretensioner Low
5 | BN/WH | -- | Driver Seat Belt Switch Signal
6 | BN | -- | LFR SIS Module High Control

### Seatbelt Switch - Right

#### Connector Part Information

- OEM: PED 15304649
- Service: N/A
- Description: 6-Way Unsealed

#### Seatbelt Switch - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Passenger Seat Belt Pretensioner High
2 | PK | -- | Seat Position Switch Low Reference
3 | L-GN | -- | RFR SIS Module Low Control
4 | OG | -- | Passenger Seat Belt Pretensioner Low
5 | OG | -- | Passenger Seat Belt Switch Signal
6 | BN/WH | -- | RFR SIS Module High Control

### Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: TYCO 5-638595-7
- Service: N/A
- Description: 60-Way F GET Unsealed

#### Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | D-GN | -- | Serial Data
3 | -- | -- | Not Used
4 | OG/BK | -- | Driver Seat Belt Pretensioner Low Control
5 | BN/WH | -- | Driver Seat Belt Pretensioner High Control
6 | L-GN | -- | Passenger Seat Belt Pretensioner High Control
7 | OG | -- | Passenger Seat Belt Pretensioner Low Control
8 | D-GN | -- | Steering Wheel Module Low Control
9 | WH | -- | Steering Wheel Module High Control
10 | WH/BK | -- | Passenger I/P Module High Control
11 | D-GN/WH | -- | Passenger I/P Module Low Control
12 | YE/BK | -- | LFR SIS Module Low Control
13 | BN | -- | LFT SIS Module High Control
14 | BN/WH | -- | RFR SIS Module High Control
15 | L-GN | -- | RFR SIS Module Low Control
16 | PK | -- | LF Roof Rail Module Low
17 | PU/WH | -- | LF Roof Rail Module High
18 | YE/BK | -- | RF Roof Rail Module High
19 | WH/BK | -- | RF Roof Rail Module Low
20-23 | -- | -- | Not Used
24 | -- | -- | Not Used (Long Body)
PU | -- | LF Retractor pretensioner Low Control (Short Body)
25 | -- | -- | Not Used (Long Body)
OG | -- | LF Retractor Pretensioner High Control (Short Body)
26 | -- | -- | Not Used (Long Body)
GY | -- | RF Retractor Pretensioner High Control (Short Body)
27 | -- | -- | Not Used (Long Body)
GN | -- | RF Retractor Pretensioner Low Control (Short Body)
28 | PK | -- | Seat Position SW Low Reference
29 | YE | -- | Seat Belt Reminder Signal
30 | -- | -- | Not Used
31 | RD/WH | -- | Battery Positive Voltage
32 | PK | -- | Ignition Voltage
33-35 | -- | -- | Not Used
36 | -- | -- | Not Used (Long Body)
L-BU/BK | -- | RT MID SISM Signal (Short Body)
37 | -- | -- | Not Used
38 | -- | -- | Not Used (Long Body)
L-GN/WH | -- | RT MID SISM Low Reference (Short Body)
39 | -- | -- | Not Used
40 | GY/BK | -- | LT MID SISM Low Reference
41 | -- | -- | Not Used (Short Body)
L-GN/WH | -- | RT MID SISM Low Reference (Long Body)
42 | D-GN/WH | -- | LT MID SISM Signal
43 | -- | -- | Not Used (Short Body)
L-BU | -- | RT MID SISM Signal (Long Body)
44-58 | -- | -- | Not Used
59 | BN/BK | -- | Driver Seat Belt SW Signal
60 | OG | -- | Passenger Seat Belt SW Signal

### Speaker - Left Front

#### Connector Part Information

- OEM: KET MG651026
- Service: N/A
- Description: 2-Way F 090II Unsealed

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Left Front Speaker (+)
2 | GY | -- | Left Front Speaker Signal (-) (1)

### Speaker - Left Rear

#### Connector Part Information

- OEM: KET MG651026
- Service: N/A
- Description: 2-Way F 090II Unsealed

#### Speaker - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Left Rear Speaker (+)
2 | YE | -- | Left Rear Speaker Signal (-)

### Speaker - Right Front

#### Connector Part Information

- OEM: KET MG651026
- Service: N/A
- Description: 2-Way F 090II Unsealed

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Speaker Feed - Right Front
2 | D-GN | -- | Speaker Return - Right Front Signal

### Speaker - Right Front

#### Connector Part Information

- OEM: KET MG651026
- Service: N/A
- Description: 2-Way F 090II Unsealed

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Speaker Feed - Right Front
2 | D-GN | -- | Speaker Return - Right Front Signal

### Speaker - Right Rear

#### Connector Part Information

- OEM: KET MG651026
- Service: N/A
- Description: 2-Way F 090II Unsealed

#### Speaker - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Right Rear Speaker (+)
2 | L-BU | -- | Right Rear Speaker Signal (-)

### Steering Angle Sensor

#### Connector Part Information

- OEM: TYCO 1488752-1
- Service: N/A
- Description: 6-Way F Micro 064 Unsealed

#### Steering Angle Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | 12-Volt Reference
2 | WH | -- | CAN (-)
3 | BN/WH | -- | CAN (+)
4 | OG/BK | -- | CAN (-)
5 | PK | -- | CAN (+)
6 | L-GN | -- | Low Reference

### Stepwell Lamp - Left

#### Connector Part Information

- OEM: MOLEX 49228-0210
- Service: N/A
- Description: 2-Way F Unsealed

#### Stepwell Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground

### Stepwell Lamp - Right

#### Connector Part Information

- OEM: MOLEX 49228-0210
- Service: N/A
- Description: 2-Way F Unsealed

#### Stepwell Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground

### Stop Lamp Switch

#### Connector Part Information

- OEM: YZK 7123-6043-30
- Service: N/A
- Description: 4-Way F M Type Unsealed

#### Stop Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/WH | -- | 12-Volt Reference
2 | PU | -- | Brake Pedal Switch Closed Signal
3 | RD/WH | -- | Battery Positive Voltage
4 | L-BU | -- | Stop Lamp Supply Voltage

### Subwoofer

#### Connector Part Information

- OEM: TYCO 368540-1
- Service: N/A
- Description: 8-Way F MS-AL Unsealed

#### Subwoofer

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RW | -- | Battery Positive Voltage
2 | RW | -- | Battery Positive Voltage
3 | D-GN | -- | Right Subwoofer Speaker (+)
4 | BK | -- | Ground
5 | BK | -- | Ground
6 | PK/BK | -- | Amplifier Powered Woofer Control (2)
7 | PU/WH | -- | Amplifier Powered Woofer Control (1)
8 | L-BU/BK | -- | Right Subwoofer Speaker (-)

### Sunroof Module

#### Connector Part Information

- OEM: PED 12047886
- Service: N/A
- Description: 8-Way F Metri-Pack 150 Unsealed

#### Sunroof Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Sunroof Switch Open Signal
B | D-GN | -- | Sunroof Switch Express Signal
C | OG/BN | -- | Sunroof Switch Open Vent Signal
D | D-BU | -- | Sunroof Switch Low Reference
E | YE | -- | Accessory Voltage
F | BK | -- | Ground
G | RD/WH | -- | Battery Positive Voltage
H | -- | -- | Not Used

### Sunroof Switch

#### Connector Part Information

- OEM: PED 13513469
- Service: N/A
- Description: 4-Way F 064 Unsealed

#### Sunroof Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Sunroof Switch Open Signal
2 | OG/BK | -- | Sunroof Switch Open Vent Signal
3 | D-BU | -- | Sunroof Switch Low Reference
4 | D-GN | -- | Sunroof Switch Express Signal

### Sunvisor Lamp - Left

#### Connector Part Information

- OEM: TYCO 936224-1
- Service: N/A
- Description: 2-Way F 090III Unsealed

#### Sunvisor Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | BCM 12-Volt Reference
2 | BK | -- | Ground

### Sunvisor Lamp - Right

#### Connector Part Information

- OEM: TYCO 936224-1
- Service: N/A
- Description: 2-Way F 090III Unsealed

#### Sunvisor Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | BCM 12-Volt Reference
2 | BK | -- | Ground

### Tail Lamp - Right

#### Connector Part Information

- OEM: Ket MG 641053
- Service: N/A
- Description: 8-Way F Unsealed

#### Tail Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BK | -- | Ground
3 | BK | -- | Ground
4 | BN/WH | -- | Park Lamp Supply
5 | L-BU | -- | Stop Lamp Switch Output
6 | L-GN | -- | Backup Lamp Switch Output
7 | D-GN | -- | Right Turn Signal
8 | OG | -- | Rear Fog Lamp Supply

### Theft Deterrent Control Module

#### Connector Part Information

- OEM: TYCO 368502-1
- Service: N/A
- Description: 6-Way F 070 Unsealed

#### Theft Deterrent Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Courtesy Lamp Relay Control
2 | BK | -- | Ground
3 | D-GN | -- | Low Speed GMLAN Serial Data
4 | BK | -- | Ground
5 | D-BU | -- | Accessory Wakeup Serial Data
6 | RD/WH | -- | Battery Positive Voltage

### Throttle Body (LD9)

#### Connector Part Information

- OEM: FEP 42121700
- Service: N/A
- Description: 6-Way F Sealed

#### Throttle Body (LD9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference
2 | GN | -- | TPS 1 Signal
3 | BK | -- | Low Reference
4 | BU | -- | TPS 2 Signal
5 | L-BU | -- | Idle Speed Motor Control Extend
6 | BU/BK | -- | Idle Speed Motor Control Retract

### Throttle Body (LLW)

#### Connector Part Information

- OEM: FEP 42121400
- Service: N/A
- Description: 4-Way F Sealed

#### Throttle Body (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | PK/BK | -- | Ignition Voltage
3 | GN | -- | Feedback
4 | WH | -- | Control

### Throttle Body (LU1)

#### Connector Part Information

- OEM: FEP 7158-6642-20
- Service: N/A
- Description: 6-Way F GT150, Sealed (PU)

#### Throttle Body (LU1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 581 | TAC Motor Control - 1
2 | 0.35 BN | 582 | TAC Motor Control - 2
3 | 0.35 BN/YE | 2752 | Low Reference
4 | 0.35 D-GN | 485 | TP Sensor 1 Signal
5 | 0.35 GY | 2701 | 5-Volt Reference
6 | 0.35 PU | 486 | TP Sensor 2 Signal

### Traction Control Switch

#### Connector Part Information

- OEM: PED 15499931
- Service: N/A
- Description: 6-Way F Micro 064 Unsealed

#### Traction Control Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Traction Control Switch Signal
2 | BK | -- | Ground
3-5 | -- | -- | Not Used
6 | YE | -- | Illumination Signal

### Trailer Relay Module (V92)

#### Connector Part Information

- OEM: Molex 35284-1610
- Service: N/A
- Description: 16-Way F Unsealed

#### Trailer Relay Module (V92)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Trailer Backup Lamp Supply Voltage
2 | BK | -- | Ground
3 | RD/WH | -- | Battery Positive Voltage
4 | L-GN | -- | Back Up Lamp Supply Voltage
5 | RD/WH | -- | Battery Positive Voltage
6 | BK | -- | Ground
7 | PU/WH | -- | Trailer Brake Lamp
8 | RD/WH | -- | Battery Positive Voltage
9 | RD/WH | -- | Battery Positive Voltage
10 | YE | -- | Right Trailer Turn Signal Lamp
11 | GN | -- | Right Rear Stop/Turn Lamp Supply Voltage
12 | RD/WH | -- | Battery Positive Voltage
13 | OG | -- | Left Trailer Turn Signal Lamp
14 | YE | -- | Left Rear Stop/Turn Lamp Supply Voltage
15 | RD/WH | -- | Battery Positive Voltage
16 | RD/WH | -- | Battery Positive Voltage

### Transmission Control Module (TCM) X1

#### Connector Part Information

- OEM: Molex 1318756-2
- Service: N/A
- Description: 24-Way M 90 Series (BK)

#### Transmission Control Module (TCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 351 | Ground (RHD)
1 | 0.35 BK | 650 | Ground (LHD)
2 | 0.35 WH | 5503 | Transmission Mainline Pressure Solenoid Low Reference
3 | 0.35 BUWH | 5502 | TCC/Clutch Select Solenoid Low Reference
4 | 0.35 D-BU | 1530 | Transmission Mainline Pressure Solenoid Control
5 | 0.35 PK/BK | 5501 | TCC/Clutch Select Solenoid Control
6 | 0.35 RD/WH | 2440 | Battery Positive Voltage
7 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1)
8 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1)
9-10 | -- | -- | Not Used
11 | 0.35 BN/WH | 585 | Transmission Oil Temperature Sensor Signal
12 | 0.35 GN/BK | 586 | Transmission Oil Temperature Sensor Low Reference
13 | 0.35 BU | 1528 | Shift Solenoid Supply Voltage (4)
14 | 0.35 L-GN | 1527 | Shift Solenoid Supply Voltage (3)
15 | 0.35 WH | 1526 | Shift Solenoid Supply Voltage (2)
16 | 0.35 OG | 1525 | Shift Solenoid Supply Voltage (1)
17 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
18 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
19 | 0.35 GY | 324 | Shift Relay Coil Control
20 | -- | -- | Not Used
21 | 0.35 BN | 323 | Shift Solenoid Supply Voltage
22 | 0.35 PU | 1529 | Shift Solenoid Supply Voltage (5)
23 | 0.35 BK | 351 | Ground (RHD)
23 | 0.35 BK | 650 | Ground (LHD)
24 | 0.35 BU | 5985 | Accessory Wakeup Serial Data

### Transmission Control Module (TCM) X2

#### Connector Part Information

- OEM: Molex 1318757-1
- Service: N/A
- Description: 26-Way M 025/90 Series (WH)

#### Transmission Control Module (TCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.35 BN/BK | 6357 | Output Speed Shielded Signal
6 | 0.35 BU | 6253 | Transmission Input Speed Sensor Ground
7 | 0.35 YE | 772 | Transmission Position Switch Bit 2 Signal
8 | 0.35 BN/WH | 771 | Transmission Position Switch Bit 1 Signal
9-13 | -- | -- | Not Used
14 | 0.35 PK | 6358 | Output Speed Signal
15 | -- | -- | Not Used
16 | 0.35 BN/WH | 6254 | Transmission Input Speed Sensor Signal
17-18 | -- | -- | Not Used
19 | 0.35 WH | 776 | Transmission Position Switch Parity Bit Signal
20 | 0.35 GY | 773 | Transmission Position Switch Bit 3 Signal
21 | 0.35 PK | 639 | Run/Crank Ignition 1 Voltage
22 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
23-26 | -- | -- | Not Used

### Turn Signal/Multifunction Switch

#### Connector Part Information

- OEM: PED 15332161
- Service: N/A
- Description: 12-Way F GT 150 Unsealed

#### Turn Signal/Multifunction Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Headlamp Switch On Signal
2 | L-BU | -- | Headlamp Switch Park Lamp Signal
3 | D-GN | -- | Headlamp Switch Headlamps Off Signal Control
4 | BK | -- | Ground
5 | OG | -- | Front Fog Lamp Switch Signal
6 | L-BU | -- | Rear Fog lamp Switch Signal
7 | BK | -- | Ground
8 | PU | -- | Headlamp Dimmer Switch High Beam Signal
9 | YE | -- | Headlamp Switch Flash to Pass Signal
10 | L-BU/WH | -- | Left Front Turn Signal Switch Signal
11 | D-BU/WH | -- | Right Front Turn Signal Switch Signal
12 | BK | -- | Ground

### Turn Signal Repeater Lamp - Left

#### Connector Part Information

- OEM: MG 610320
- Service: N/A
- Description: 2-Way F SWP Sealed

#### Turn Signal Repeater Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/WH | -- | Left Front T/Signal Lamp Supply Voltage
2 | BK | -- | Ground

### Turn Signal Repeater Lamp - Right

#### Connector Part Information

- OEM: MG 610320
- Service: N/A
- Description: 2-Way F SWP Sealed

#### Turn Signal Repeater Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Right Front T/Signal Lamp Supply Voltage
2 | BN | -- | Ground

### Tweeter - Left Front

#### Connector Part Information

- OEM: KET MG610070
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### Tweeter - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Front Tweeter Speaker (-)
2 | BN | -- | Left Front Tweeter Speaker (+)

### Tweeter - Left Rear

#### Connector Part Information

- OEM: KET MG610070
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### Tweeter - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Left Rear Tweeter Speaker (-)
2 | OG | -- | Left Rear Tweeter Speaker (+)

### Tweeter - Right Front

#### Connector Part Information

- OEM: KET MG610070
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### Tweeter - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Right Front Tweeter Speaker (-)
2 | L-GN | -- | Right Front Tweeter Speaker (+)

### Tweeter - Right Rear

#### Connector Part Information

- OEM: KET MG610070
- Service: N/A
- Description: 2-Way F 090 Unsealed

#### Tweeter - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Right Rear Tweeter Speaker (-)
2 | WH | -- | Right Rear Tweeter Speaker (+)

### Water in Fuel Sensor (2.0L Diesel)

#### Connector Part Information

- OEM: TYCO 85205-1
- Service: N/A
- Description: 3-Way F JPT Sealed

#### Water in Fuel Sensor (2.0L Diesel)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | WIF Sensor
2 | BK | -- | Ground
3 | PK | -- | Run/Crank Ignition 1 Voltage

### Wheel Speed Sensor - Left Front

#### Connector Part Information

- OEM: PED 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack Sealed

#### Wheel Speed Sensor - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Front Wheel Speed Sensor Low Reference
2 | L-BU | -- | Left Front Wheel Speed Sensor Signal

### Wheel Speed Sensor - Left Rear

#### Connector Part Information

- OEM: PED 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack Sealed

#### Wheel Speed Sensor - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | Left Rear Wheel Speed Sensor Low Reference
2 | BN | -- | Left Rear Wheel Speed Sensor Signal

### Wheel Speed Sensor - Right Front

#### Connector Part Information

- OEM: PED 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack Sealed

#### Wheel Speed Sensor - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Right Front Wheel Speed Sensor Low Reference
2 | D-GN | -- | Right Front Wheel Speed Sensor Signal

### Wheel Speed Sensor - Right Rear

#### Connector Part Information

- OEM: PED 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack Sealed

#### Wheel Speed Sensor - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Right Rear Wheel Speed Sensor Low Reference
2 | BN | -- | Right Rear Wheel Speed Sensor Signal

### Windshield Washer Fluid Level Switch

#### Connector Part Information

- OEM: TYCO 174352-2
- Service: N/A
- Description: 2-Way F Mark-II Sealed

#### Windshield Washer Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BN/WH | -- | Windshield Washer Fluid Level Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: PED 12052641
- Service: N/A
- Description: 2-Way F 090 Sealed

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | OG | -- | Windshield Washer Pump Control

### Windshield Wiper Motor

#### Connector Part Information

- OEM: TYCO 936254-1
- Service: N/A
- Description: 4-Way F MCP-E(280) Sealed

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Park Signal
2 | BK | -- | Ground
3 | PU | -- | High Speed Control
4 | GN | -- | Low Speed Control

### Windshield Wiper Switch

#### Connector Part Information

- OEM: PED 15332145
- Service: N/A
- Description: 8-Way F 150 GT Unsealed

#### Windshield Wiper Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Windshield Washer Switch Signal
2 | BN/BK | -- | Windshield Wiper Switch Low Reference
3 | L-GN | -- | Windshield Wiper Switch High Signal
4 | L-BU | -- | Windshield Wiper Switch Low Signal
5 | GY | -- | Rear Window Wiper Switch Signal
6 | BN | -- | Accessory Voltage
7-8 | -- | -- | Not Used

### XBCM X1

#### Connector Part Information

- OEM: PED 12110088
- Service: N/A
- Description: 24-Way F Metri-Pack Unsealed

#### XBCM X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | RD/WH | -- | Battery Positive Voltage
A3 | D-GN | -- | Low Speed GMLAN Serial Data
A4-A6 | -- | -- | Not Used
A7 | BK | -- | Ground
A8-A12 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | PK | -- | Run/Crank Ignition Voltage
B3 | -- | -- | Not Used
B4 | BN/BK | -- | Power Sounder Enable Signal
B5-B6 | -- | -- | Not Used
B7 | BK | -- | Ground
B8 | -- | -- | Not Used
B9 | YE | -- | Security Indicator Control
B10 | L-BU | -- | Inclination Sensor Alarm On Signal
B11 | -- | -- | Not Used
B12 | WH | -- | Power Sounder Enable Signal

### XBCM X2

#### Connector Part Information

- OEM: PED 15357040
- Service: N/A
- Description: 8-Way F Metri-Pack 280 Unsealed (GN)

#### XBCM X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RD/WH | -- | Battery Positive Voltage
C | RD/WH | -- | Battery Positive Voltage
D | BN | -- | Door Double Actuator Lock Control
E | -- | -- | Not Used
F | BN | -- | Ground
G-H | -- | -- | Not Used

### Yaw Sensor

#### Connector Part Information

- OEM: TYCO 1-967616-1
- Service: N/A
- Description: 6-Way F Unsealed

#### Yaw Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | CAN (+)
2 | WH | -- | CAN (-)
3 | GY | -- | 12-Volt Reference
4 | -- | -- | Not Used
5 | L-BU | -- | Low Reference
6 | -- | -- | Not Used