For 1990-2009 cars

### Removal Procedure

1. Remove the rear transmission mount bracket. Refer to Transmission Mount Bracket Replacement - Rear .
2. Remove the rear transmission mount to frame bolts (1).
3. Remove the rear transmission mount (2).

### Installation Procedure

1. Install the rear transmission mount (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear transmission mount to frame bolts (1) and tighten to 90 N·m (66 lb ft) .
3. Install the rear transmission mount bracket. Refer to Transmission Mount Bracket Replacement - Rear .